(kicad_pcb (version 20160815) (host pcbnew "(2016-12-15 revision b13c7e4)-master")
  (general
    (links 60)
    (no_connects 0)
    (area 111.079999 73.5 174.955001 110.500001)
    (thickness 1.6)
    (drawings 11)
    (tracks 222)
    (zones 0)
    (modules 25)
    (nets 27)
  )
  (page A4)
  (title_block
    (title "Tool Head PCB")
    (date 2017-03-17)
    (rev 0.7)
    (company "Aleph Objects Inc.")
    (comment 1 "GNU GPLv3, Copyright 2016-2017")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 0.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /T-)
  (net 3 /T+)
  (net 4 "Net-(D1-Pad1)")
  (net 5 /ENC_A)
  (net 6 /ENC_B)
  (net 7 "Net-(D2-Pad1)")
  (net 8 /HEAT)
  (net 9 /E-FAN)
  (net 10 /OB2)
  (net 11 /OB1)
  (net 12 /OA2)
  (net 13 /OA1)
  (net 14 /SCLK)
  (net 15 /~SS1)
  (net 16 /~SS0)
  (net 17 /MOSI)
  (net 18 /MISO)
  (net 19 +3V3)
  (net 20 +5V)
  (net 21 "Net-(P2-Pad2)")
  (net 22 "Net-(P1-Pad9)")
  (net 23 "Net-(P1-Pad12)")
  (net 24 "Net-(P1-Pad14)")
  (net 25 "Net-(P1-Pad16)")
  (net 26 /SCLK_P1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net +3V3)
    (add_net +5V)
    (add_net /E-FAN)
    (add_net /ENC_A)
    (add_net /ENC_B)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCLK)
    (add_net /SCLK_P1)
    (add_net /T+)
    (add_net /T-)
    (add_net /~SS0)
    (add_net /~SS1)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad2)")
  )
  (net_class Heat ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /HEAT)
  )
  (net_class Motors ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /OA1)
    (add_net /OA2)
    (add_net /OB1)
    (add_net /OB2)
  )
  (module Pin_Headers:Pin_Header_Angled_1x10 (layer F.Cu) (tedit 5845BBB2)
    (at 164.08 83.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value DOCK (at 0 24.5) (layer F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +3V3))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /~SS1))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /MOSI))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /SCLK_P1))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /~SS0))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /MISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /HEAT))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58CC1733)
    (at 129.005 85 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value HEAT (at -2.1 1.2 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /HEAT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (thermal_width 0.5))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ToolHead_PCB:MountingHole_3mm_Pad (layer F.Cu) (tedit 5845BBB2)
    (at 144.5 91)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module Pin_Headers:Pin_Header_Angled_2x10 (layer F.Cu) (tedit 5845BBB2)
    (at 124.505 100.2 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2 25.5 180) (layer F.SilkS) hide)
    (fp_text value CARRIAGE (at 1.305 24.5 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +3V3) (thermal_width 0.5))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /MOSI))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /~SS1))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /SCLK_P1))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /~SS0))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /MISO))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /ENC_B))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /ENC_A))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /OB2))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /OB1))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /OA2))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /OA1))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /E-FAN))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /HEAT))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x10.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ToolHead_PCB:MountingHole_3mm_Pad (layer F.Cu) (tedit 5845BBB2)
    (at 121.465 105.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module ToolHead_PCB:MountingHole_3mm_Pad (layer F.Cu) (tedit 5845BBB2)
    (at 164.58 78.85)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 58CC1750)
    (at 150.405 85 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value ENCODER (at -1.7 3.8025 180) (layer F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ToolHead_PCB:THERMOCOUPLE (layer F.Cu) (tedit 58CC1761)
    (at 132 103.55)
    (fp_text reference P8 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value THERMO (at 0 -5.25) (layer F.SilkS))
    (fp_text user + (at 4.9 -3.45) (layer F.SilkS))
    (pad 1 smd rect (at 3 0) (size 3 6) (layers F.Cu F.Mask)
      (net 3 /T+))
    (pad 2 smd rect (at -3 0) (size 3 6) (layers F.Cu F.Mask)
      (net 2 /T-))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5845BBB2)
    (at 127.5 90.35 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.6 0 -180) (layer F.SilkS))
    (fp_text value 15μF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 58CC173C)
    (at 137.165 85 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value E-MOTOR (at -1.9 3.985) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /OA1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /OA2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /OB1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /OB2))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58CC1779)
    (at 158.025 99.1 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value HS-FAN (at -2.2 1.2 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58CC176E)
    (at 144.785 99.1 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value E-FAN (at -2.2 1.2 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /E-FAN) (zone_connect 1))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:SO-8 (layer F.Cu) (tedit 58CC1815)
    (at 132 91.5)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U2 (at 1.95 -4.2) (layer F.SilkS))
    (fp_text value MAX31855KASA (at 0 0) (layer F.Fab) hide)
    (pad 8 smd oval (at -1.905 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd oval (at -0.635 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 18 /MISO))
    (pad 6 smd oval (at 0.635 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 16 /~SS0))
    (pad 5 smd oval (at 1.905 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCLK))
    (pad 4 smd oval (at 1.905 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 3 smd oval (at 0.635 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 /T+))
    (pad 2 smd oval (at -0.635 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 /T-))
    (pad 1 smd oval (at -1.905 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 1) (thermal_gap 0.152))
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CC181F)
    (at 137.5 91.5)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value EEPROM (at 0 2.9) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 /~SS1))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /MISO))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 /MOSI))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCLK))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5894CFAF)
    (at 127.6 98.1 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.4 0 180) (layer F.SilkS))
    (fp_text value 15μF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (thermal_gap 0.184))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58CC1798)
    (at 136.2 96.9)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.1 -1.1) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58CC1793)
    (at 132 96.9 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.1 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /T-))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /T+))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ToolHead_PCB:SOD-523F (layer F.Cu) (tedit 5845BBB2)
    (at 151.835 89.77)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at -3.25 0) (layer F.SilkS))
    (fp_text value RB751S40 (at 0 1.7) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /ENC_A))
  )
  (module ToolHead_PCB:SOD-523F (layer F.Cu) (tedit 5845BBB2)
    (at 156.635 89.77 180)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D2 (at -3.25 0 180) (layer F.SilkS))
    (fp_text value RB751S40 (at 0 1.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1 0) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /ENC_B))
    (pad 1 smd rect (at -1 0) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58CC17F3)
    (at 156.635 91.77 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3.25 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /ENC_B))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58CC17E7)
    (at 151.835 91.77)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -3.25 0) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /ENC_A))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58CC17D9)
    (at 151.835 87.77)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.25 0) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58CC17ED)
    (at 156.635 87.77 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -3.25 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5898B8E2)
    (at 127.2 94)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB1 (at 0 -1.25) (layer F.SilkS))
    (fp_text value "2.5 kΩ@100MHz" (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 /SCLK_P1))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCLK))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58CC1882)
    (at 152 100.05 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.45 0) (layer F.SilkS))
    (fp_text value 15μF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 121.465 109.25) (end 168.58 109.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.58 78.85) (end 168.58 109.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.465 105.25) (end 117.465 74.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.58 74.85) (end 117.465 74.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 164.58 78.85) (end 164.58 74.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.465 105.25) (end 121.465 109.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Copyright\nAleph Objects Inc.\nGNU GPLv3" (at 142.76 104.5) (layer B.SilkS))
  (gr_text v0.7 (at 119.5 76) (layer B.SilkS))
  (gr_text COUPLE (at 132 99.8) (layer F.SilkS))
  (gr_text + (at 140.48 97.5) (layer F.SilkS))
  (gr_text + (at 153.72 97.5) (layer F.SilkS))
  (zone (net 19) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 169.5 110) (xy 116.5 110) (xy 116.5 74) (xy 169.5 74)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 170 110.5) (xy 116 110.5) (xy 116 73.5) (xy 170 73.5)
      )
    )
  )
)
