(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 1711)
    (no_connects 475)
    (area 53.924999 24.924999 244.075001 160.075001)
    (thickness 1.6)
    (drawings 113)
    (tracks 5483)
    (zones 0)
    (modules 633)
    (nets 734)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (1 In1.Cu power)
    (2 In2.Cu signal)
    (3 In3.Cu signal)
    (4 In4.Cu power)
    (31 B.Cu mixed)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (user_trace_width 2.032)
    (trace_clearance 0.2)
    (zone_clearance 0.3048)
    (zone_45_only yes)
    (trace_min 0.1016)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.327)
    (via_min_drill 0.2)
    (user_via 0.45 0.3)
    (user_via 0.6 0.4)
    (user_via 0.66 0.4)
    (user_via 0.75 0.5)
    (user_via 0.9 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFD669)
    (pcbplotparams
      (layerselection 0x000b8_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/aleph/cim_gerb_test))
  )
  (net 0 "")
  (net 1 CGND)
  (net 2 /~SYS_RESET)
  (net 3 VCC)
  (net 4 +24V)
  (net 5 SYS_5V)
  (net 6 USB_DC)
  (net 7 /Ethernet/RD+)
  (net 8 /Ethernet/RD-)
  (net 9 /Ethernet/TD+)
  (net 10 /Ethernet/TD-)
  (net 11 /BED_THERM)
  (net 12 /ADC)
  (net 13 /X1_ENDSTOP)
  (net 14 /Y1_ENDSTOP)
  (net 15 /Z1_ENDSTOP)
  (net 16 /ENC_B)
  (net 17 "/Stepper Drivers/E Stepper Driver/5VOUT")
  (net 18 "/Stepper Drivers/E_A2")
  (net 19 "/Stepper Drivers/E_B2")
  (net 20 "/Stepper Drivers/E_A1")
  (net 21 "/Stepper Drivers/E_B1")
  (net 22 /Heaters/BED_HEAT)
  (net 23 /Heaters/E_HEAT)
  (net 24 /Heaters/DOCK0_HEAT)
  (net 25 /Heaters/H_HEAT)
  (net 26 /Heaters/DOCK1_HEAT)
  (net 27 /Fans/H_FAN)
  (net 28 /Fans/CASE_FAN)
  (net 29 VDD_1V8)
  (net 30 VDD_3V3AUX)
  (net 31 /Endstops/Z1_IN)
  (net 32 /~SS_DOCK0_T)
  (net 33 /~SS_DOCK0_NVM)
  (net 34 /~SS_DOCK1_T)
  (net 35 /~SS_DOCK1_NVM)
  (net 36 /SPI1_MISO)
  (net 37 /SPI1_SCLK)
  (net 38 /SPI1_MOSI)
  (net 39 /SPI0_MISO)
  (net 40 /SPI0_CS0)
  (net 41 /~DISP_INT)
  (net 42 /XDMA_EVENT_INTRO)
  (net 43 /CLKOUT2)
  (net 44 /USB/USB.B.VBUS)
  (net 45 /Thermistors/BED_THERM_IN)
  (net 46 /Thermistors/ADC_IN)
  (net 47 /Endstops/X1_IN)
  (net 48 /Endstops/Y1_IN)
  (net 49 /Endstops/ENC_A_IN)
  (net 50 /Endstops/ENC_B_IN)
  (net 51 /I2C0_SCL)
  (net 52 /I2C0_SDA)
  (net 53 /USB/UART0_RXD)
  (net 54 /USB/UART0_TXD)
  (net 55 /USB/USB.CLIENT.ID)
  (net 56 /USB/USB.CLIENT.D-)
  (net 57 /USB/USB.CLIENT.D+)
  (net 58 /USB/USB.HOST.D+)
  (net 59 /USB/USB.HOST.D-)
  (net 60 /MMC0_CLK)
  (net 61 /MMC0_CMD)
  (net 62 /MMC0_DAT0)
  (net 63 /MMC0_DAT3)
  (net 64 /MMC0_DAT1)
  (net 65 /MMC0_DAT2)
  (net 66 /SD.CD)
  (net 67 /Ethernet/YELA)
  (net 68 /Ethernet/GRNA)
  (net 69 /JTAG/JTAG_TMS)
  (net 70 /JTAG/~JTAG_TRST)
  (net 71 /JTAG/JTAG_TDI)
  (net 72 /JTAG/JTAG_TD0)
  (net 73 /TCK)
  (net 74 /JTAG/JTAG_EMU0)
  (net 75 /JTAG/JTAG_EMU1)
  (net 76 /SERVO_0)
  (net 77 VDD_3V3A)
  (net 78 /USR3)
  (net 79 /USR2)
  (net 80 /USR1)
  (net 81 /USR0)
  (net 82 "Net-(R15-Pad1)")
  (net 83 "Net-(R26-Pad2)")
  (net 84 "Net-(R28-Pad2)")
  (net 85 "Net-(R29-Pad2)")
  (net 86 "Net-(R30-Pad2)")
  (net 87 /Flash/GPIO1_16.SIP)
  (net 88 /Flash/EMMC_RSTN)
  (net 89 /Flash/MMC1_DAT0)
  (net 90 /Flash/MMC1_DAT1)
  (net 91 /Flash/MMC1_DAT2)
  (net 92 /Flash/MMC1_DAT3)
  (net 93 /Flash/MMC1_DAT4)
  (net 94 /Flash/MMC1_DAT5)
  (net 95 /Flash/MMC1_DAT6)
  (net 96 /Flash/MMC1_DAT7)
  (net 97 /Flash/MMC1_CMD)
  (net 98 /Flash/MMC1_CLK)
  (net 99 /USB/USB1_DRVVBUS)
  (net 100 /~USB1_OC)
  (net 101 /USB/USB1_VBUS)
  (net 102 /Ethernet/MII1_REFCLK)
  (net 103 /Ethernet/MII1_RXD3)
  (net 104 /Ethernet/MII1_RXD2)
  (net 105 /Ethernet/MII1_RXD1)
  (net 106 /Ethernet/MII1_RXD0)
  (net 107 /Ethernet/MII1_RXDV)
  (net 108 /Ethernet/MII1_RXCLK)
  (net 109 /Ethernet/MII1_RXERR)
  (net 110 /Ethernet/MII1_TXCLK)
  (net 111 /Ethernet/MII1_COL)
  (net 112 /Ethernet/MII1_CRS_DV)
  (net 113 /Ethernet/MDIO_DATA)
  (net 114 VDD_ADC)
  (net 115 /~SR_EN)
  (net 116 /E_FAULT)
  (net 117 /X2_ENDSTOP)
  (net 118 /X_FAULT)
  (net 119 /Z2_ENDSTOP)
  (net 120 /Z_FAULT)
  (net 121 /H_FAULT)
  (net 122 /Y2_ENDSTOP)
  (net 123 /Y_FAULT)
  (net 124 /Power/PWR_BUT)
  (net 125 /Power/BAT_TEMP)
  (net 126 /Power/BAT_VOLT)
  (net 127 /Power/VIN_BAT)
  (net 128 /USB/~UART0_RST)
  (net 129 GNDA)
  (net 130 /Power/PMIC_NWAKEUP)
  (net 131 /Power/PMIC_PGOOD)
  (net 132 /Power/LDO_PGOOD)
  (net 133 /Power/PMIC_INT)
  (net 134 "Net-(U1-PadC6)")
  (net 135 /SPI1_CS0)
  (net 136 /I2C2_SCL)
  (net 137 /I2C2_SDA)
  (net 138 /USB/UART0_RXD_IN)
  (net 139 /USB/UART0_TXD_OUT)
  (net 140 /Ethernet/MII1_TXEN)
  (net 141 /Ethernet/MII1_TXD3)
  (net 142 /Ethernet/MII1_TXD2)
  (net 143 /Ethernet/MII1_TXD1)
  (net 144 /Ethernet/MII1_TXD0)
  (net 145 /Ethernet/MDIO_CLK)
  (net 146 /H_STEP)
  (net 147 "Net-(U1-PadR14)")
  (net 148 /Z_DIR)
  (net 149 /Y_STEP)
  (net 150 /Z_STEP)
  (net 151 /E_DIR)
  (net 152 /X_STEP)
  (net 153 /Y_DIR)
  (net 154 /E_STEP)
  (net 155 /H_DIR)
  (net 156 /X_DIR)
  (net 157 "Net-(U14-Pad9)")
  (net 158 "Net-(U14-Pad10)")
  (net 159 "/Stepper Drivers/~E_EN")
  (net 160 "Net-(C2-Pad1)")
  (net 161 /Configuration/LCD.D15.R4--R7)
  (net 162 /Configuration/LCD.D14.R3--R6)
  (net 163 /Configuration/LCD.D13.R2--R5)
  (net 164 /Configuration/LCD.D12.R1--R4)
  (net 165 /Configuration/LCD.D11.R0--R3)
  (net 166 /Configuration/LCD.D10.G5--G7)
  (net 167 /Configuration/LCD.D9.G4--G6)
  (net 168 /Configuration/LCD.D8.G3--G5)
  (net 169 /Configuration/LCD.D7.G2--G4)
  (net 170 /Configuration/LCD.D6.G1--G3)
  (net 171 /Configuration/LCD.D5.G0--G2)
  (net 172 /Configuration/LCD.D4.B4--B7)
  (net 173 /Configuration/LCD.D3.B3--B6)
  (net 174 /Configuration/LCD.D2.B2--B5)
  (net 175 /Configuration/LCD.D1.B1--B4)
  (net 176 /Configuration/LCD.D0.B0--B3)
  (net 177 "Net-(U11-Pad9)")
  (net 178 "Net-(U14-Pad17)")
  (net 179 "Net-(U14-Pad19)")
  (net 180 "Net-(P15-Pad11)")
  (net 181 "Net-(P15-Pad10)")
  (net 182 "/Stepper Drivers/X0 Stepper Driver/5VOUT")
  (net 183 "/Stepper Drivers/X0_A2")
  (net 184 "/Stepper Drivers/X0_B2")
  (net 185 "/Stepper Drivers/X0_A1")
  (net 186 "/Stepper Drivers/X0_B1")
  (net 187 "/Stepper Drivers/~X0_EN")
  (net 188 "/Stepper Drivers/X1 Stepper Driver/5VOUT")
  (net 189 "/Stepper Drivers/X1_A2")
  (net 190 "/Stepper Drivers/X1_B2")
  (net 191 "/Stepper Drivers/X1_A1")
  (net 192 "/Stepper Drivers/X1_B1")
  (net 193 "/Stepper Drivers/~X1_EN")
  (net 194 "/Stepper Drivers/Z0 Stepper Driver/5VOUT")
  (net 195 "/Stepper Drivers/Z0_A2")
  (net 196 "/Stepper Drivers/Z0_B2")
  (net 197 "/Stepper Drivers/Z0_A1")
  (net 198 "/Stepper Drivers/Z0_B1")
  (net 199 "/Stepper Drivers/Y Stepper Driver/5VOUT")
  (net 200 "/Stepper Drivers/Y_A2")
  (net 201 "/Stepper Drivers/Y_B2")
  (net 202 "/Stepper Drivers/Y_A1")
  (net 203 "/Stepper Drivers/Y_B1")
  (net 204 "Net-(P15-Pad7)")
  (net 205 "Net-(P16-Pad6)")
  (net 206 "Net-(U1-PadA2)")
  (net 207 "Net-(U1-PadA3)")
  (net 208 /Microprocessor/AIN3)
  (net 209 "Net-(U1-PadB2)")
  (net 210 "Net-(U1-PadB3)")
  (net 211 "Net-(U1-PadB1)")
  (net 212 /Microprocessor/AIN0)
  (net 213 /Microprocessor/AIN2)
  (net 214 /Microprocessor/AIN5)
  (net 215 "Net-(U1-PadC2)")
  (net 216 "Net-(U1-PadC3)")
  (net 217 "Net-(U1-PadC4)")
  (net 218 "Net-(U1-PadC1)")
  (net 219 /Microprocessor/AIN1)
  (net 220 "Net-(U1-PadC10)")
  (net 221 "Net-(U1-PadD2)")
  (net 222 "Net-(U1-PadD5)")
  (net 223 "Net-(U1-PadD3)")
  (net 224 "Net-(U1-PadD4)")
  (net 225 "Net-(U1-PadD1)")
  (net 226 "Net-(U1-PadD6)")
  (net 227 "Net-(U1-PadD7)")
  (net 228 "Net-(U1-PadD9)")
  (net 229 "Net-(U1-PadD11)")
  (net 230 "Net-(U1-PadE2)")
  (net 231 "Net-(U1-PadE5)")
  (net 232 "Net-(U1-PadE3)")
  (net 233 "Net-(U1-PadE4)")
  (net 234 "Net-(U1-PadE1)")
  (net 235 "Net-(U1-PadE6)")
  (net 236 VDD_PLL)
  (net 237 "Net-(U1-PadE10)")
  (net 238 "Net-(U1-PadE11)")
  (net 239 "Net-(U1-PadE12)")
  (net 240 "Net-(U1-PadE13)")
  (net 241 "Net-(U1-PadE14)")
  (net 242 "Net-(U1-PadE18)")
  (net 243 "Net-(U1-PadF2)")
  (net 244 "Net-(U1-PadF5)")
  (net 245 "Net-(U1-PadF3)")
  (net 246 "Net-(U1-PadF4)")
  (net 247 "Net-(U1-PadF1)")
  (net 248 VDD_CORE)
  (net 249 "Net-(U1-PadF7)")
  (net 250 "Net-(U1-PadF9)")
  (net 251 VDD_MPU)
  (net 252 "Net-(U1-PadF11)")
  (net 253 "Net-(U1-PadF12)")
  (net 254 "Net-(U1-PadF13)")
  (net 255 "Net-(U1-PadF14)")
  (net 256 "Net-(U1-PadF16)")
  (net 257 "Net-(U1-PadG2)")
  (net 258 "Net-(U1-PadG5)")
  (net 259 "Net-(U1-PadG3)")
  (net 260 "Net-(U1-PadG4)")
  (net 261 "Net-(U1-PadG1)")
  (net 262 "Net-(U1-PadG6)")
  (net 263 "Net-(U1-PadG7)")
  (net 264 "Net-(U1-PadG10)")
  (net 265 "Net-(U1-PadG13)")
  (net 266 "Net-(U1-PadG14)")
  (net 267 "Net-(U1-PadH2)")
  (net 268 VDD_DDR)
  (net 269 "Net-(U1-PadH3)")
  (net 270 "Net-(U1-PadH4)")
  (net 271 "Net-(U1-PadH1)")
  (net 272 "Net-(U1-PadH11)")
  (net 273 "Net-(U1-PadH13)")
  (net 274 "Net-(U1-PadH14)")
  (net 275 "Net-(U1-PadH15)")
  (net 276 "Net-(U1-PadJ2)")
  (net 277 "Net-(U1-PadJ5)")
  (net 278 "Net-(U1-PadJ3)")
  (net 279 "Net-(U1-PadJ4)")
  (net 280 "Net-(U1-PadJ1)")
  (net 281 "Net-(U1-PadJ12)")
  (net 282 "Net-(U1-PadJ13)")
  (net 283 "Net-(U1-PadJ14)")
  (net 284 "Net-(U1-PadK2)")
  (net 285 "Net-(U1-PadK5)")
  (net 286 "Net-(U1-PadK3)")
  (net 287 "Net-(U1-PadK4)")
  (net 288 "Net-(U1-PadK1)")
  (net 289 "Net-(U1-PadK6)")
  (net 290 "Net-(U1-PadK8)")
  (net 291 "Net-(U1-PadK12)")
  (net 292 "Net-(U1-PadK13)")
  (net 293 "Net-(U1-PadK14)")
  (net 294 "Net-(U1-PadL8)")
  (net 295 "Net-(U1-PadL9)")
  (net 296 "Net-(U1-PadL7)")
  (net 297 "Net-(U1-PadL3)")
  (net 298 "Net-(U1-PadL1)")
  (net 299 "Net-(U1-PadL2)")
  (net 300 "Net-(U1-PadL4)")
  (net 301 "Net-(U1-PadL5)")
  (net 302 "Net-(U1-PadL6)")
  (net 303 "Net-(U1-PadL14)")
  (net 304 "Net-(U1-PadM13)")
  (net 305 "Net-(U1-PadM11)")
  (net 306 "Net-(U1-PadM3)")
  (net 307 "Net-(U1-PadM1)")
  (net 308 "Net-(U1-PadM2)")
  (net 309 "Net-(U1-PadM4)")
  (net 310 "Net-(U1-PadM5)")
  (net 311 "Net-(U1-PadM15)")
  (net 312 "Net-(U1-PadN13)")
  (net 313 "Net-(U1-PadN12)")
  (net 314 "Net-(U1-PadN8)")
  (net 315 "Net-(U1-PadN9)")
  (net 316 "Net-(U1-PadN3)")
  (net 317 "Net-(U1-PadN1)")
  (net 318 "Net-(U1-PadN2)")
  (net 319 "Net-(U1-PadN4)")
  (net 320 VDD_RTC)
  (net 321 "Net-(U1-PadN15)")
  (net 322 "Net-(U1-PadP13)")
  (net 323 "Net-(U1-PadP11)")
  (net 324 "Net-(U1-PadP12)")
  (net 325 "Net-(U1-PadP10)")
  (net 326 "Net-(U1-PadP8)")
  (net 327 "Net-(U1-PadP9)")
  (net 328 "Net-(U1-PadP3)")
  (net 329 "Net-(U1-PadP1)")
  (net 330 "Net-(U1-PadP2)")
  (net 331 "Net-(U1-PadP4)")
  (net 332 "Net-(U1-PadP14)")
  (net 333 "Net-(U1-PadP18)")
  (net 334 "Net-(U1-PadR11)")
  (net 335 "Net-(U1-PadR10)")
  (net 336 "Net-(U1-PadR5)")
  (net 337 "Net-(U1-PadR6)")
  (net 338 "Net-(U1-PadR15)")
  (net 339 "Net-(U1-PadU11)")
  (net 340 "Net-(U1-PadU5)")
  (net 341 /HDMI_INT)
  (net 342 "Net-(U1-PadV11)")
  (net 343 "Net-(U1-PadV10)")
  (net 344 "Net-(U1-PadV5)")
  (net 345 "Net-(U1-PadY16)")
  (net 346 "Net-(U1-PadY13)")
  (net 347 "Net-(U1-PadY14)")
  (net 348 "Net-(U1-PadY19)")
  (net 349 "Net-(U1-PadY17)")
  (net 350 "Net-(U1-PadY20)")
  (net 351 "Net-(U5-PadB1)")
  (net 352 "Net-(U5-PadF1)")
  (net 353 "Net-(U5-PadH1)")
  (net 354 "Net-(U5-PadJ1)")
  (net 355 "Net-(U5-PadK1)")
  (net 356 "Net-(U5-PadL1)")
  (net 357 "Net-(U5-PadM1)")
  (net 358 "Net-(U5-PadN1)")
  (net 359 "Net-(U5-PadP1)")
  (net 360 "Net-(U5-PadG2)")
  (net 361 "Net-(U5-PadH2)")
  (net 362 "Net-(U5-PadJ2)")
  (net 363 "Net-(U5-PadK2)")
  (net 364 "Net-(U5-PadL2)")
  (net 365 "Net-(U5-PadM2)")
  (net 366 "Net-(U5-PadF3)")
  (net 367 "Net-(U5-PadG3)")
  (net 368 "Net-(U5-PadH3)")
  (net 369 "Net-(U5-PadJ3)")
  (net 370 "Net-(U5-PadK3)")
  (net 371 "Net-(U5-PadL3)")
  (net 372 "Net-(U5-PadM3)")
  (net 373 "Net-(U5-PadN3)")
  (net 374 "Net-(U5-PadE5)")
  (net 375 "Net-(U5-PadH5)")
  (net 376 "Net-(U5-PadJ5)")
  (net 377 "Net-(U5-PadA6)")
  (net 378 "Net-(U5-PadK6)")
  (net 379 "Net-(U5-PadA7)")
  (net 380 "Net-(U5-PadK7)")
  (net 381 "Net-(U5-PadP7)")
  (net 382 "Net-(U5-PadC8)")
  (net 383 "Net-(U5-PadE8)")
  (net 384 "Net-(U5-PadM8)")
  (net 385 "Net-(U5-PadB9)")
  (net 386 "Net-(U5-PadC9)")
  (net 387 "Net-(U5-PadE9)")
  (net 388 "Net-(U5-PadM9)")
  (net 389 "Net-(U5-PadN9)")
  (net 390 "Net-(U5-PadA10)")
  (net 391 "Net-(U5-PadB10)")
  (net 392 "Net-(U5-PadC10)")
  (net 393 "Net-(U5-PadE10)")
  (net 394 "Net-(U5-PadF10)")
  (net 395 "Net-(U5-PadG10)")
  (net 396 "Net-(U5-PadK10)")
  (net 397 "Net-(U5-PadM10)")
  (net 398 "Net-(U5-PadN10)")
  (net 399 "Net-(U5-PadP10)")
  (net 400 "Net-(U5-PadA11)")
  (net 401 "Net-(U5-PadB11)")
  (net 402 "Net-(U5-PadC11)")
  (net 403 "Net-(U5-PadM11)")
  (net 404 "Net-(U5-PadN11)")
  (net 405 "Net-(U5-PadP11)")
  (net 406 "Net-(U5-PadA12)")
  (net 407 "Net-(U5-PadB12)")
  (net 408 "Net-(U5-PadC12)")
  (net 409 "Net-(U5-PadD12)")
  (net 410 "Net-(U5-PadE12)")
  (net 411 "Net-(U5-PadF12)")
  (net 412 "Net-(U5-PadG12)")
  (net 413 "Net-(U5-PadH12)")
  (net 414 "Net-(U5-PadJ12)")
  (net 415 "Net-(U5-PadK12)")
  (net 416 "Net-(U5-PadL12)")
  (net 417 "Net-(U5-PadM12)")
  (net 418 "Net-(U5-PadN12)")
  (net 419 "Net-(U5-PadP12)")
  (net 420 "Net-(U5-PadA13)")
  (net 421 "Net-(U5-PadB13)")
  (net 422 "Net-(U5-PadC13)")
  (net 423 "Net-(U5-PadD13)")
  (net 424 "Net-(U5-PadE13)")
  (net 425 "Net-(U5-PadF13)")
  (net 426 "Net-(U5-PadG13)")
  (net 427 "Net-(U5-PadH13)")
  (net 428 "Net-(U5-PadJ13)")
  (net 429 "Net-(U5-PadK13)")
  (net 430 "Net-(U5-PadL13)")
  (net 431 "Net-(U5-PadM13)")
  (net 432 "Net-(U5-PadN13)")
  (net 433 "Net-(U5-PadP13)")
  (net 434 "Net-(U5-PadA14)")
  (net 435 "Net-(U5-PadB14)")
  (net 436 "Net-(U5-PadC14)")
  (net 437 "Net-(U5-PadD14)")
  (net 438 "Net-(U5-PadE14)")
  (net 439 "Net-(U5-PadF14)")
  (net 440 "Net-(U5-PadG14)")
  (net 441 "Net-(U5-PadH14)")
  (net 442 "Net-(U5-PadJ14)")
  (net 443 "Net-(U5-PadK14)")
  (net 444 "Net-(U5-PadL14)")
  (net 445 "Net-(U5-PadM14)")
  (net 446 "Net-(U5-PadN14)")
  (net 447 "Net-(U5-PadP14)")
  (net 448 "/Stepper Drivers/~Y_EN")
  (net 449 "/Stepper Drivers/~Z0_EN")
  (net 450 "Net-(U15-Pad10)")
  (net 451 "Net-(U15-Pad9)")
  (net 452 "Net-(U15-Pad19)")
  (net 453 "Net-(U15-Pad17)")
  (net 454 "Net-(U16-Pad17)")
  (net 455 "Net-(U16-Pad19)")
  (net 456 "Net-(U16-Pad9)")
  (net 457 "Net-(U16-Pad10)")
  (net 458 "Net-(U20-Pad17)")
  (net 459 "Net-(U20-Pad19)")
  (net 460 "Net-(U20-Pad9)")
  (net 461 "Net-(U20-Pad10)")
  (net 462 "/Stepper Drivers/Z1 Stepper Driver/5VOUT")
  (net 463 "/Stepper Drivers/Z1_A2")
  (net 464 "/Stepper Drivers/Z1_B2")
  (net 465 "/Stepper Drivers/Z1_A1")
  (net 466 "/Stepper Drivers/Z1_B1")
  (net 467 "/Stepper Drivers/Z2 Stepper Driver/5VOUT")
  (net 468 "/Stepper Drivers/Z2_A2")
  (net 469 "/Stepper Drivers/Z2_B2")
  (net 470 "/Stepper Drivers/Z2_A1")
  (net 471 "/Stepper Drivers/Z2_B1")
  (net 472 "/Stepper Drivers/H Stepper Driver/5VOUT")
  (net 473 "/Stepper Drivers/H_A2")
  (net 474 "/Stepper Drivers/H_B2")
  (net 475 "/Stepper Drivers/H_A1")
  (net 476 "/Stepper Drivers/H_B1")
  (net 477 "Net-(D13-Pad1)")
  (net 478 "Net-(D15-Pad1)")
  (net 479 "Net-(D18-Pad1)")
  (net 480 "Net-(D20-Pad1)")
  (net 481 "Net-(Q5-Pad1)")
  (net 482 "Net-(Q5-Pad3)")
  (net 483 "Net-(Q6-Pad1)")
  (net 484 "Net-(Q7-Pad3)")
  (net 485 "Net-(Q7-Pad1)")
  (net 486 "Net-(Q9-Pad1)")
  (net 487 "/Stepper Drivers/~Z1_EN")
  (net 488 "/Stepper Drivers/~Z2_EN")
  (net 489 "/Stepper Drivers/~H_EN")
  (net 490 "Net-(U17-Pad10)")
  (net 491 "Net-(U17-Pad9)")
  (net 492 "Net-(U17-Pad19)")
  (net 493 "Net-(U17-Pad17)")
  (net 494 "Net-(U18-Pad17)")
  (net 495 "Net-(U18-Pad19)")
  (net 496 "Net-(U18-Pad9)")
  (net 497 "Net-(U18-Pad10)")
  (net 498 "Net-(U19-Pad10)")
  (net 499 "Net-(U19-Pad9)")
  (net 500 "Net-(U19-Pad19)")
  (net 501 "Net-(U19-Pad17)")
  (net 502 /Heaters/BED_HEAT_IN)
  (net 503 /Heaters/E_HEAT_IN)
  (net 504 "Net-(F2-Pad1)")
  (net 505 "Net-(F2-Pad2)")
  (net 506 /~SS_E_NVM)
  (net 507 /~SS_H_NVM)
  (net 508 /SPI1_CS1)
  (net 509 "/Stepper Drivers/Z2_MISO")
  (net 510 "/Stepper Drivers/E_MISO")
  (net 511 "/Stepper Drivers/Y_MISO")
  (net 512 "/Stepper Drivers/X0_MISO")
  (net 513 "/Stepper Drivers/X1_MISO")
  (net 514 "/Stepper Drivers/Z0_MISO")
  (net 515 "/Stepper Drivers/Z1_MISO")
  (net 516 "Net-(U13-Pad17)")
  (net 517 "Net-(U13-Pad19)")
  (net 518 "Net-(U13-Pad9)")
  (net 519 "Net-(U13-Pad10)")
  (net 520 /Fans/E_FAN)
  (net 521 VDD_5V)
  (net 522 /Heaters/DOCK0_HEAT_IN)
  (net 523 /Heaters/H_HEAT_IN)
  (net 524 /Heaters/DOCK1_HEAT_IN)
  (net 525 /Fans/E_FAN_IN)
  (net 526 /Fans/H_FAN_IN)
  (net 527 /Fans/CASE_FAN_IN)
  (net 528 "Net-(U21-Pad1)")
  (net 529 "Net-(U21-Pad17)")
  (net 530 "Net-(U21-Pad18)")
  (net 531 "Net-(U21-Pad19)")
  (net 532 "Net-(U21-Pad20)")
  (net 533 "Net-(U21-Pad21)")
  (net 534 "Net-(U21-Pad22)")
  (net 535 "Net-(U21-Pad25)")
  (net 536 "Net-(D21-Pad1)")
  (net 537 "Net-(D24-Pad1)")
  (net 538 "Net-(D25-Pad1)")
  (net 539 "Net-(D27-Pad2)")
  (net 540 /SPI0_SCLK)
  (net 541 /SPI0_MOSI)
  (net 542 "Net-(FB35-Pad2)")
  (net 543 "Net-(FB36-Pad2)")
  (net 544 "Net-(FB43-Pad2)")
  (net 545 "Net-(FB44-Pad2)")
  (net 546 "Net-(Q8-Pad3)")
  (net 547 "Net-(Q8-Pad1)")
  (net 548 "Net-(Q10-Pad1)")
  (net 549 "Net-(Q11-Pad3)")
  (net 550 "Net-(Q11-Pad1)")
  (net 551 "Net-(Q12-Pad1)")
  (net 552 "Net-(Q12-Pad3)")
  (net 553 "Net-(Q13-Pad1)")
  (net 554 "Net-(Q14-Pad1)")
  (net 555 "Net-(C41-Pad1)")
  (net 556 "Net-(F1-Pad2)")
  (net 557 "Net-(FB46-Pad1)")
  (net 558 "Net-(D15-Pad2)")
  (net 559 "Net-(D19-Pad2)")
  (net 560 "Net-(D22-Pad2)")
  (net 561 "Net-(D23-Pad2)")
  (net 562 "Net-(D26-Pad2)")
  (net 563 "Net-(D28-Pad1)")
  (net 564 "Net-(D29-Pad2)")
  (net 565 "Net-(D30-Pad1)")
  (net 566 "Net-(D31-Pad2)")
  (net 567 "Net-(D32-Pad1)")
  (net 568 "Net-(D33-Pad2)")
  (net 569 "Net-(Q15-Pad3)")
  (net 570 "Net-(Q15-Pad1)")
  (net 571 "Net-(Q16-Pad1)")
  (net 572 "Net-(Q17-Pad3)")
  (net 573 "Net-(Q17-Pad1)")
  (net 574 "Net-(Q18-Pad1)")
  (net 575 "Net-(Q19-Pad1)")
  (net 576 "Net-(Q19-Pad3)")
  (net 577 "Net-(Q20-Pad1)")
  (net 578 "Net-(C42-Pad1)")
  (net 579 "Net-(D7-Pad1)")
  (net 580 /~SS_E_T)
  (net 581 /~SS_H_T)
  (net 582 "Net-(FB1-Pad2)")
  (net 583 "Net-(FB2-Pad2)")
  (net 584 "Net-(FB3-Pad2)")
  (net 585 "Net-(FB4-Pad2)")
  (net 586 "Net-(FB5-Pad2)")
  (net 587 "Net-(FB6-Pad2)")
  (net 588 "Net-(FB7-Pad2)")
  (net 589 "Net-(FB8-Pad2)")
  (net 590 "Net-(FB9-Pad2)")
  (net 591 "Net-(FB10-Pad2)")
  (net 592 "Net-(FB11-Pad2)")
  (net 593 "Net-(FB12-Pad2)")
  (net 594 "Net-(FB13-Pad2)")
  (net 595 "Net-(FB14-Pad2)")
  (net 596 "Net-(FB15-Pad2)")
  (net 597 "Net-(FB16-Pad2)")
  (net 598 "Net-(FB17-Pad2)")
  (net 599 "Net-(FB18-Pad2)")
  (net 600 "Net-(FB19-Pad2)")
  (net 601 "Net-(FB20-Pad2)")
  (net 602 "Net-(FB21-Pad2)")
  (net 603 "Net-(FB22-Pad2)")
  (net 604 "Net-(FB23-Pad2)")
  (net 605 "Net-(FB24-Pad2)")
  (net 606 "Net-(FB25-Pad2)")
  (net 607 "Net-(FB26-Pad2)")
  (net 608 "Net-(FB27-Pad2)")
  (net 609 "Net-(FB28-Pad2)")
  (net 610 "Net-(FB29-Pad2)")
  (net 611 "Net-(FB30-Pad2)")
  (net 612 "Net-(FB31-Pad2)")
  (net 613 "Net-(FB32-Pad2)")
  (net 614 "Net-(FB33-Pad2)")
  (net 615 "Net-(FB34-Pad2)")
  (net 616 "Net-(FB51-Pad1)")
  (net 617 "Net-(FB52-Pad1)")
  (net 618 "Net-(FB53-Pad1)")
  (net 619 "Net-(FB54-Pad1)")
  (net 620 "Net-(FB55-Pad1)")
  (net 621 VDD_PHYA)
  (net 622 /Ethernet/PHY_VDDCR)
  (net 623 "Net-(IC1-Pad5)")
  (net 624 "Net-(R32-Pad2)")
  (net 625 "Net-(R45-Pad1)")
  (net 626 "Net-(R51-Pad2)")
  (net 627 "Net-(R53-Pad1)")
  (net 628 /Ethernet/REFCLKO)
  (net 629 /Ethernet/RXD3/PHYAD2)
  (net 630 /Ethernet/RXD2/RMIISEL)
  (net 631 /Ethernet/RXD1/MODE1)
  (net 632 /Ethernet/RXD0/MODE0)
  (net 633 /Ethernet/RXDV)
  (net 634 /Ethernet/RXER/PHYAD0)
  (net 635 /Ethernet/TXCLK)
  (net 636 /Ethernet/MODE2)
  (net 637 /Ethernet/CRS)
  (net 638 /Ethernet/RCLKIN)
  (net 639 /Ethernet/RBIAS)
  (net 640 /Ethernet/ETH_TXD4)
  (net 641 "Net-(R117-Pad2)")
  (net 642 "Net-(U7-Pad3)")
  (net 643 "Net-(U7-Pad5)")
  (net 644 "Net-(U9-Pad5)")
  (net 645 "Net-(U1-PadV17)")
  (net 646 "Net-(C43-Pad1)")
  (net 647 "Net-(FB56-Pad1)")
  (net 648 "Net-(C5-Pad1)")
  (net 649 "Net-(C7-Pad1)")
  (net 650 "Net-(C18-Pad1)")
  (net 651 "Net-(C27-Pad1)")
  (net 652 "Net-(FB41-Pad1)")
  (net 653 "Net-(FB42-Pad2)")
  (net 654 "Net-(FB45-Pad1)")
  (net 655 "Net-(C23-Pad1)")
  (net 656 "Net-(C28-Pad1)")
  (net 657 "Net-(C41-Pad2)")
  (net 658 "Net-(C43-Pad2)")
  (net 659 "Net-(C44-Pad1)")
  (net 660 "Net-(C57-Pad1)")
  (net 661 "Net-(C60-Pad1)")
  (net 662 "Net-(C60-Pad2)")
  (net 663 "Net-(C63-Pad2)")
  (net 664 "Net-(C68-Pad1)")
  (net 665 "Net-(C71-Pad1)")
  (net 666 "Net-(C73-Pad1)")
  (net 667 "Net-(C76-Pad2)")
  (net 668 "Net-(C76-Pad1)")
  (net 669 "Net-(C79-Pad2)")
  (net 670 "Net-(C84-Pad1)")
  (net 671 "Net-(C87-Pad1)")
  (net 672 "Net-(C89-Pad1)")
  (net 673 "Net-(C92-Pad1)")
  (net 674 "Net-(C92-Pad2)")
  (net 675 "Net-(C95-Pad2)")
  (net 676 "Net-(C100-Pad1)")
  (net 677 "Net-(C103-Pad1)")
  (net 678 "Net-(C105-Pad1)")
  (net 679 "Net-(C108-Pad2)")
  (net 680 "Net-(C108-Pad1)")
  (net 681 "Net-(C111-Pad2)")
  (net 682 "Net-(C116-Pad1)")
  (net 683 "Net-(C119-Pad1)")
  (net 684 "Net-(C121-Pad1)")
  (net 685 "Net-(C124-Pad1)")
  (net 686 "Net-(C124-Pad2)")
  (net 687 "Net-(C127-Pad2)")
  (net 688 "Net-(C132-Pad1)")
  (net 689 "Net-(C135-Pad1)")
  (net 690 "Net-(C137-Pad1)")
  (net 691 "Net-(C140-Pad2)")
  (net 692 "Net-(C140-Pad1)")
  (net 693 "Net-(C143-Pad2)")
  (net 694 "Net-(C148-Pad1)")
  (net 695 "Net-(C151-Pad1)")
  (net 696 "Net-(C153-Pad1)")
  (net 697 "Net-(C156-Pad2)")
  (net 698 "Net-(C156-Pad1)")
  (net 699 "Net-(C159-Pad2)")
  (net 700 "Net-(C164-Pad1)")
  (net 701 "Net-(C167-Pad1)")
  (net 702 "Net-(C169-Pad1)")
  (net 703 "Net-(C172-Pad1)")
  (net 704 "Net-(C172-Pad2)")
  (net 705 "Net-(C175-Pad2)")
  (net 706 "Net-(C180-Pad1)")
  (net 707 "Net-(C183-Pad1)")
  (net 708 /SIP_I2C0_SCL)
  (net 709 "Net-(FB48-Pad2)")
  (net 710 "Net-(FB57-Pad1)")
  (net 711 "Net-(U21-Pad15)")
  (net 712 "Net-(U21-Pad16)")
  (net 713 "Net-(R109-Pad2)")
  (net 714 "Net-(R111-Pad2)")
  (net 715 "Net-(R124-Pad2)")
  (net 716 "Net-(R131-Pad2)")
  (net 717 "Net-(R136-Pad2)")
  (net 718 "Net-(R141-Pad2)")
  (net 719 "Net-(R147-Pad2)")
  (net 720 "Net-(R154-Pad2)")
  (net 721 "Net-(R159-Pad2)")
  (net 722 /ENC_A)
  (net 723 "Net-(D3-Pad2)")
  (net 724 "Net-(D4-Pad2)")
  (net 725 "Net-(D5-Pad2)")
  (net 726 "Net-(D6-Pad2)")
  (net 727 "Net-(D9-Pad1)")
  (net 728 "Net-(D9-Pad3)")
  (net 729 "Net-(D11-Pad1)")
  (net 730 "Net-(D12-Pad1)")
  (net 731 "Net-(D12-Pad3)")
  (net 732 "Net-(R213-Pad1)")
  (net 733 "Net-(U12-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net /ADC)
    (add_net /BED_THERM)
    (add_net /CLKOUT2)
    (add_net /Configuration/LCD.D0.B0--B3)
    (add_net /Configuration/LCD.D1.B1--B4)
    (add_net /Configuration/LCD.D10.G5--G7)
    (add_net /Configuration/LCD.D11.R0--R3)
    (add_net /Configuration/LCD.D12.R1--R4)
    (add_net /Configuration/LCD.D13.R2--R5)
    (add_net /Configuration/LCD.D14.R3--R6)
    (add_net /Configuration/LCD.D15.R4--R7)
    (add_net /Configuration/LCD.D2.B2--B5)
    (add_net /Configuration/LCD.D3.B3--B6)
    (add_net /Configuration/LCD.D4.B4--B7)
    (add_net /Configuration/LCD.D5.G0--G2)
    (add_net /Configuration/LCD.D6.G1--G3)
    (add_net /Configuration/LCD.D7.G2--G4)
    (add_net /Configuration/LCD.D8.G3--G5)
    (add_net /Configuration/LCD.D9.G4--G6)
    (add_net /ENC_A)
    (add_net /ENC_B)
    (add_net /E_STEP)
    (add_net /Endstops/ENC_A_IN)
    (add_net /Endstops/ENC_B_IN)
    (add_net /Endstops/X1_IN)
    (add_net /Endstops/Y1_IN)
    (add_net /Endstops/Z1_IN)
    (add_net /Ethernet/CRS)
    (add_net /Ethernet/ETH_TXD4)
    (add_net /Ethernet/GRNA)
    (add_net /Ethernet/MDIO_CLK)
    (add_net /Ethernet/MDIO_DATA)
    (add_net /Ethernet/MII1_COL)
    (add_net /Ethernet/MII1_CRS_DV)
    (add_net /Ethernet/MII1_REFCLK)
    (add_net /Ethernet/MII1_RXCLK)
    (add_net /Ethernet/MII1_RXD0)
    (add_net /Ethernet/MII1_RXD1)
    (add_net /Ethernet/MII1_RXD2)
    (add_net /Ethernet/MII1_RXD3)
    (add_net /Ethernet/MII1_RXDV)
    (add_net /Ethernet/MII1_RXERR)
    (add_net /Ethernet/MII1_TXCLK)
    (add_net /Ethernet/MII1_TXD0)
    (add_net /Ethernet/MII1_TXD1)
    (add_net /Ethernet/MII1_TXD2)
    (add_net /Ethernet/MII1_TXD3)
    (add_net /Ethernet/MII1_TXEN)
    (add_net /Ethernet/MODE2)
    (add_net /Ethernet/PHY_VDDCR)
    (add_net /Ethernet/RBIAS)
    (add_net /Ethernet/RCLKIN)
    (add_net /Ethernet/RD+)
    (add_net /Ethernet/RD-)
    (add_net /Ethernet/REFCLKO)
    (add_net /Ethernet/RXD0/MODE0)
    (add_net /Ethernet/RXD1/MODE1)
    (add_net /Ethernet/RXD2/RMIISEL)
    (add_net /Ethernet/RXD3/PHYAD2)
    (add_net /Ethernet/RXDV)
    (add_net /Ethernet/RXER/PHYAD0)
    (add_net /Ethernet/TD+)
    (add_net /Ethernet/TD-)
    (add_net /Ethernet/TXCLK)
    (add_net /Ethernet/YELA)
    (add_net /Fans/CASE_FAN)
    (add_net /Fans/CASE_FAN_IN)
    (add_net /Fans/E_FAN)
    (add_net /Fans/E_FAN_IN)
    (add_net /Fans/H_FAN)
    (add_net /Fans/H_FAN_IN)
    (add_net /Flash/GPIO1_16.SIP)
    (add_net /HDMI_INT)
    (add_net /H_FAULT)
    (add_net /H_STEP)
    (add_net /Heaters/BED_HEAT)
    (add_net /Heaters/BED_HEAT_IN)
    (add_net /Heaters/DOCK0_HEAT)
    (add_net /Heaters/DOCK0_HEAT_IN)
    (add_net /Heaters/DOCK1_HEAT)
    (add_net /Heaters/DOCK1_HEAT_IN)
    (add_net /Heaters/E_HEAT)
    (add_net /Heaters/E_HEAT_IN)
    (add_net /Heaters/H_HEAT)
    (add_net /Heaters/H_HEAT_IN)
    (add_net /JTAG/JTAG_EMU0)
    (add_net /JTAG/JTAG_EMU1)
    (add_net /JTAG/JTAG_TD0)
    (add_net /JTAG/JTAG_TDI)
    (add_net /JTAG/JTAG_TMS)
    (add_net /JTAG/~JTAG_TRST)
    (add_net /MMC0_CLK)
    (add_net /MMC0_CMD)
    (add_net /MMC0_DAT0)
    (add_net /MMC0_DAT1)
    (add_net /MMC0_DAT2)
    (add_net /MMC0_DAT3)
    (add_net /Microprocessor/AIN0)
    (add_net /Microprocessor/AIN1)
    (add_net /Microprocessor/AIN2)
    (add_net /Microprocessor/AIN3)
    (add_net /Microprocessor/AIN5)
    (add_net /Power/BAT_TEMP)
    (add_net /Power/BAT_VOLT)
    (add_net /Power/LDO_PGOOD)
    (add_net /Power/PMIC_INT)
    (add_net /Power/PMIC_NWAKEUP)
    (add_net /Power/PMIC_PGOOD)
    (add_net /Power/PWR_BUT)
    (add_net /Power/VIN_BAT)
    (add_net /SD.CD)
    (add_net /SERVO_0)
    (add_net /SIP_I2C0_SCL)
    (add_net /SPI0_CS0)
    (add_net /SPI0_MISO)
    (add_net /SPI0_MOSI)
    (add_net /SPI0_SCLK)
    (add_net /SPI1_CS0)
    (add_net /SPI1_CS1)
    (add_net /SPI1_MISO)
    (add_net /SPI1_MOSI)
    (add_net /SPI1_SCLK)
    (add_net "/Stepper Drivers/E Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/E_A1")
    (add_net "/Stepper Drivers/E_A2")
    (add_net "/Stepper Drivers/E_B1")
    (add_net "/Stepper Drivers/E_B2")
    (add_net "/Stepper Drivers/E_MISO")
    (add_net "/Stepper Drivers/H Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/H_A1")
    (add_net "/Stepper Drivers/H_A2")
    (add_net "/Stepper Drivers/H_B1")
    (add_net "/Stepper Drivers/H_B2")
    (add_net "/Stepper Drivers/X0 Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/X0_A1")
    (add_net "/Stepper Drivers/X0_A2")
    (add_net "/Stepper Drivers/X0_B1")
    (add_net "/Stepper Drivers/X0_B2")
    (add_net "/Stepper Drivers/X0_MISO")
    (add_net "/Stepper Drivers/X1 Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/X1_A1")
    (add_net "/Stepper Drivers/X1_A2")
    (add_net "/Stepper Drivers/X1_B1")
    (add_net "/Stepper Drivers/X1_B2")
    (add_net "/Stepper Drivers/X1_MISO")
    (add_net "/Stepper Drivers/Y Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/Y_A1")
    (add_net "/Stepper Drivers/Y_A2")
    (add_net "/Stepper Drivers/Y_B1")
    (add_net "/Stepper Drivers/Y_B2")
    (add_net "/Stepper Drivers/Y_MISO")
    (add_net "/Stepper Drivers/Z0 Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/Z0_A1")
    (add_net "/Stepper Drivers/Z0_A2")
    (add_net "/Stepper Drivers/Z0_B1")
    (add_net "/Stepper Drivers/Z0_B2")
    (add_net "/Stepper Drivers/Z0_MISO")
    (add_net "/Stepper Drivers/Z1 Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/Z1_A1")
    (add_net "/Stepper Drivers/Z1_A2")
    (add_net "/Stepper Drivers/Z1_B1")
    (add_net "/Stepper Drivers/Z1_B2")
    (add_net "/Stepper Drivers/Z1_MISO")
    (add_net "/Stepper Drivers/Z2 Stepper Driver/5VOUT")
    (add_net "/Stepper Drivers/Z2_A1")
    (add_net "/Stepper Drivers/Z2_A2")
    (add_net "/Stepper Drivers/Z2_B1")
    (add_net "/Stepper Drivers/Z2_B2")
    (add_net "/Stepper Drivers/Z2_MISO")
    (add_net "/Stepper Drivers/~E_EN")
    (add_net "/Stepper Drivers/~H_EN")
    (add_net "/Stepper Drivers/~X0_EN")
    (add_net "/Stepper Drivers/~X1_EN")
    (add_net "/Stepper Drivers/~Y_EN")
    (add_net "/Stepper Drivers/~Z0_EN")
    (add_net "/Stepper Drivers/~Z1_EN")
    (add_net "/Stepper Drivers/~Z2_EN")
    (add_net /TCK)
    (add_net /Thermistors/ADC_IN)
    (add_net /Thermistors/BED_THERM_IN)
    (add_net /USB/UART0_RXD)
    (add_net /USB/UART0_RXD_IN)
    (add_net /USB/UART0_TXD)
    (add_net /USB/UART0_TXD_OUT)
    (add_net /USB/USB.B.VBUS)
    (add_net /USB/USB.CLIENT.D+)
    (add_net /USB/USB.CLIENT.D-)
    (add_net /USB/USB.CLIENT.ID)
    (add_net /USB/USB.HOST.D+)
    (add_net /USB/USB.HOST.D-)
    (add_net /USB/USB1_DRVVBUS)
    (add_net /USB/USB1_VBUS)
    (add_net /USB/~UART0_RST)
    (add_net /USR1)
    (add_net /USR2)
    (add_net /USR3)
    (add_net /X1_ENDSTOP)
    (add_net /X2_ENDSTOP)
    (add_net /XDMA_EVENT_INTRO)
    (add_net /X_DIR)
    (add_net /X_FAULT)
    (add_net /Y2_ENDSTOP)
    (add_net /Y_DIR)
    (add_net /Y_FAULT)
    (add_net /Z1_ENDSTOP)
    (add_net /Z2_ENDSTOP)
    (add_net /Z_FAULT)
    (add_net /~DISP_INT)
    (add_net /~SR_EN)
    (add_net /~SS_DOCK0_NVM)
    (add_net /~SS_DOCK0_T)
    (add_net /~SS_DOCK1_NVM)
    (add_net /~SS_DOCK1_T)
    (add_net /~SS_E_NVM)
    (add_net /~SS_E_T)
    (add_net /~SS_H_NVM)
    (add_net /~SS_H_T)
    (add_net /~SYS_RESET)
    (add_net /~USB1_OC)
    (add_net GNDA)
    (add_net "Net-(C100-Pad1)")
    (add_net "Net-(C103-Pad1)")
    (add_net "Net-(C105-Pad1)")
    (add_net "Net-(C108-Pad1)")
    (add_net "Net-(C108-Pad2)")
    (add_net "Net-(C111-Pad2)")
    (add_net "Net-(C116-Pad1)")
    (add_net "Net-(C119-Pad1)")
    (add_net "Net-(C121-Pad1)")
    (add_net "Net-(C124-Pad1)")
    (add_net "Net-(C124-Pad2)")
    (add_net "Net-(C127-Pad2)")
    (add_net "Net-(C132-Pad1)")
    (add_net "Net-(C135-Pad1)")
    (add_net "Net-(C137-Pad1)")
    (add_net "Net-(C140-Pad1)")
    (add_net "Net-(C140-Pad2)")
    (add_net "Net-(C143-Pad2)")
    (add_net "Net-(C148-Pad1)")
    (add_net "Net-(C151-Pad1)")
    (add_net "Net-(C153-Pad1)")
    (add_net "Net-(C156-Pad1)")
    (add_net "Net-(C156-Pad2)")
    (add_net "Net-(C159-Pad2)")
    (add_net "Net-(C164-Pad1)")
    (add_net "Net-(C167-Pad1)")
    (add_net "Net-(C169-Pad1)")
    (add_net "Net-(C172-Pad1)")
    (add_net "Net-(C172-Pad2)")
    (add_net "Net-(C175-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C180-Pad1)")
    (add_net "Net-(C183-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C41-Pad2)")
    (add_net "Net-(C42-Pad1)")
    (add_net "Net-(C43-Pad1)")
    (add_net "Net-(C43-Pad2)")
    (add_net "Net-(C44-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C57-Pad1)")
    (add_net "Net-(C60-Pad1)")
    (add_net "Net-(C60-Pad2)")
    (add_net "Net-(C63-Pad2)")
    (add_net "Net-(C68-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C71-Pad1)")
    (add_net "Net-(C73-Pad1)")
    (add_net "Net-(C76-Pad1)")
    (add_net "Net-(C76-Pad2)")
    (add_net "Net-(C79-Pad2)")
    (add_net "Net-(C84-Pad1)")
    (add_net "Net-(C87-Pad1)")
    (add_net "Net-(C89-Pad1)")
    (add_net "Net-(C92-Pad1)")
    (add_net "Net-(C92-Pad2)")
    (add_net "Net-(C95-Pad2)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D12-Pad3)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D20-Pad1)")
    (add_net "Net-(D21-Pad1)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D23-Pad2)")
    (add_net "Net-(D24-Pad1)")
    (add_net "Net-(D25-Pad1)")
    (add_net "Net-(D26-Pad2)")
    (add_net "Net-(D27-Pad2)")
    (add_net "Net-(D28-Pad1)")
    (add_net "Net-(D29-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D30-Pad1)")
    (add_net "Net-(D31-Pad2)")
    (add_net "Net-(D32-Pad1)")
    (add_net "Net-(D33-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad3)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(F2-Pad2)")
    (add_net "Net-(FB1-Pad2)")
    (add_net "Net-(FB10-Pad2)")
    (add_net "Net-(FB11-Pad2)")
    (add_net "Net-(FB12-Pad2)")
    (add_net "Net-(FB13-Pad2)")
    (add_net "Net-(FB14-Pad2)")
    (add_net "Net-(FB15-Pad2)")
    (add_net "Net-(FB16-Pad2)")
    (add_net "Net-(FB17-Pad2)")
    (add_net "Net-(FB18-Pad2)")
    (add_net "Net-(FB19-Pad2)")
    (add_net "Net-(FB2-Pad2)")
    (add_net "Net-(FB20-Pad2)")
    (add_net "Net-(FB21-Pad2)")
    (add_net "Net-(FB22-Pad2)")
    (add_net "Net-(FB23-Pad2)")
    (add_net "Net-(FB24-Pad2)")
    (add_net "Net-(FB25-Pad2)")
    (add_net "Net-(FB26-Pad2)")
    (add_net "Net-(FB27-Pad2)")
    (add_net "Net-(FB28-Pad2)")
    (add_net "Net-(FB29-Pad2)")
    (add_net "Net-(FB3-Pad2)")
    (add_net "Net-(FB30-Pad2)")
    (add_net "Net-(FB31-Pad2)")
    (add_net "Net-(FB32-Pad2)")
    (add_net "Net-(FB33-Pad2)")
    (add_net "Net-(FB34-Pad2)")
    (add_net "Net-(FB35-Pad2)")
    (add_net "Net-(FB36-Pad2)")
    (add_net "Net-(FB4-Pad2)")
    (add_net "Net-(FB41-Pad1)")
    (add_net "Net-(FB42-Pad2)")
    (add_net "Net-(FB43-Pad2)")
    (add_net "Net-(FB45-Pad1)")
    (add_net "Net-(FB46-Pad1)")
    (add_net "Net-(FB48-Pad2)")
    (add_net "Net-(FB5-Pad2)")
    (add_net "Net-(FB51-Pad1)")
    (add_net "Net-(FB52-Pad1)")
    (add_net "Net-(FB53-Pad1)")
    (add_net "Net-(FB54-Pad1)")
    (add_net "Net-(FB55-Pad1)")
    (add_net "Net-(FB56-Pad1)")
    (add_net "Net-(FB57-Pad1)")
    (add_net "Net-(FB6-Pad2)")
    (add_net "Net-(FB7-Pad2)")
    (add_net "Net-(FB8-Pad2)")
    (add_net "Net-(FB9-Pad2)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(P15-Pad10)")
    (add_net "Net-(P15-Pad11)")
    (add_net "Net-(P15-Pad7)")
    (add_net "Net-(P16-Pad6)")
    (add_net "Net-(Q10-Pad1)")
    (add_net "Net-(Q11-Pad1)")
    (add_net "Net-(Q11-Pad3)")
    (add_net "Net-(Q12-Pad1)")
    (add_net "Net-(Q12-Pad3)")
    (add_net "Net-(Q13-Pad1)")
    (add_net "Net-(Q14-Pad1)")
    (add_net "Net-(Q15-Pad1)")
    (add_net "Net-(Q15-Pad3)")
    (add_net "Net-(Q16-Pad1)")
    (add_net "Net-(Q17-Pad1)")
    (add_net "Net-(Q17-Pad3)")
    (add_net "Net-(Q18-Pad1)")
    (add_net "Net-(Q19-Pad1)")
    (add_net "Net-(Q19-Pad3)")
    (add_net "Net-(Q20-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q7-Pad3)")
    (add_net "Net-(Q8-Pad1)")
    (add_net "Net-(Q8-Pad3)")
    (add_net "Net-(Q9-Pad1)")
    (add_net "Net-(R109-Pad2)")
    (add_net "Net-(R111-Pad2)")
    (add_net "Net-(R117-Pad2)")
    (add_net "Net-(R124-Pad2)")
    (add_net "Net-(R131-Pad2)")
    (add_net "Net-(R136-Pad2)")
    (add_net "Net-(R141-Pad2)")
    (add_net "Net-(R147-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R154-Pad2)")
    (add_net "Net-(R159-Pad2)")
    (add_net "Net-(R213-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R30-Pad2)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R45-Pad1)")
    (add_net "Net-(R51-Pad2)")
    (add_net "Net-(R53-Pad1)")
    (add_net "Net-(U1-PadV17)")
    (add_net "Net-(U11-Pad9)")
    (add_net "Net-(U12-Pad9)")
    (add_net "Net-(U13-Pad10)")
    (add_net "Net-(U13-Pad17)")
    (add_net "Net-(U13-Pad19)")
    (add_net "Net-(U13-Pad9)")
    (add_net "Net-(U14-Pad10)")
    (add_net "Net-(U14-Pad17)")
    (add_net "Net-(U14-Pad19)")
    (add_net "Net-(U14-Pad9)")
    (add_net "Net-(U15-Pad10)")
    (add_net "Net-(U15-Pad17)")
    (add_net "Net-(U15-Pad19)")
    (add_net "Net-(U15-Pad9)")
    (add_net "Net-(U16-Pad10)")
    (add_net "Net-(U16-Pad17)")
    (add_net "Net-(U16-Pad19)")
    (add_net "Net-(U16-Pad9)")
    (add_net "Net-(U17-Pad10)")
    (add_net "Net-(U17-Pad17)")
    (add_net "Net-(U17-Pad19)")
    (add_net "Net-(U17-Pad9)")
    (add_net "Net-(U18-Pad10)")
    (add_net "Net-(U18-Pad17)")
    (add_net "Net-(U18-Pad19)")
    (add_net "Net-(U18-Pad9)")
    (add_net "Net-(U19-Pad10)")
    (add_net "Net-(U19-Pad17)")
    (add_net "Net-(U19-Pad19)")
    (add_net "Net-(U19-Pad9)")
    (add_net "Net-(U20-Pad10)")
    (add_net "Net-(U20-Pad17)")
    (add_net "Net-(U20-Pad19)")
    (add_net "Net-(U20-Pad9)")
    (add_net "Net-(U21-Pad1)")
    (add_net "Net-(U21-Pad15)")
    (add_net "Net-(U21-Pad16)")
    (add_net "Net-(U21-Pad17)")
    (add_net "Net-(U21-Pad18)")
    (add_net "Net-(U21-Pad19)")
    (add_net "Net-(U21-Pad20)")
    (add_net "Net-(U21-Pad21)")
    (add_net "Net-(U21-Pad22)")
    (add_net "Net-(U21-Pad25)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U9-Pad5)")
    (add_net SYS_5V)
    (add_net USB_DC)
    (add_net VDD_1V8)
    (add_net VDD_3V3A)
    (add_net VDD_3V3AUX)
    (add_net VDD_5V)
    (add_net VDD_ADC)
    (add_net VDD_CORE)
    (add_net VDD_DDR)
    (add_net VDD_MPU)
    (add_net VDD_PHYA)
    (add_net VDD_PLL)
    (add_net VDD_RTC)
  )
  (net_class BGA_PWR ""
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CGND)
    (add_net VCC)
  )
  (net_class OSD335x ""
    (clearance 0.2)
    (trace_width 0.1524)
    (via_dia 0.66)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /I2C0_SCL)
    (add_net /I2C0_SDA)
    (add_net /I2C2_SCL)
    (add_net /I2C2_SDA)
    (add_net "Net-(FB44-Pad2)")
    (add_net "Net-(U1-PadA2)")
    (add_net "Net-(U1-PadA3)")
    (add_net "Net-(U1-PadB1)")
    (add_net "Net-(U1-PadB2)")
    (add_net "Net-(U1-PadB3)")
    (add_net "Net-(U1-PadC1)")
    (add_net "Net-(U1-PadC10)")
    (add_net "Net-(U1-PadC2)")
    (add_net "Net-(U1-PadC3)")
    (add_net "Net-(U1-PadC4)")
    (add_net "Net-(U1-PadC6)")
    (add_net "Net-(U1-PadD1)")
    (add_net "Net-(U1-PadD11)")
    (add_net "Net-(U1-PadD2)")
    (add_net "Net-(U1-PadD3)")
    (add_net "Net-(U1-PadD4)")
    (add_net "Net-(U1-PadD5)")
    (add_net "Net-(U1-PadD6)")
    (add_net "Net-(U1-PadD7)")
    (add_net "Net-(U1-PadD9)")
    (add_net "Net-(U1-PadE1)")
    (add_net "Net-(U1-PadE10)")
    (add_net "Net-(U1-PadE11)")
    (add_net "Net-(U1-PadE12)")
    (add_net "Net-(U1-PadE13)")
    (add_net "Net-(U1-PadE14)")
    (add_net "Net-(U1-PadE18)")
    (add_net "Net-(U1-PadE2)")
    (add_net "Net-(U1-PadE3)")
    (add_net "Net-(U1-PadE4)")
    (add_net "Net-(U1-PadE5)")
    (add_net "Net-(U1-PadE6)")
    (add_net "Net-(U1-PadF1)")
    (add_net "Net-(U1-PadF11)")
    (add_net "Net-(U1-PadF12)")
    (add_net "Net-(U1-PadF13)")
    (add_net "Net-(U1-PadF14)")
    (add_net "Net-(U1-PadF16)")
    (add_net "Net-(U1-PadF2)")
    (add_net "Net-(U1-PadF3)")
    (add_net "Net-(U1-PadF4)")
    (add_net "Net-(U1-PadF5)")
    (add_net "Net-(U1-PadF7)")
    (add_net "Net-(U1-PadF9)")
    (add_net "Net-(U1-PadG1)")
    (add_net "Net-(U1-PadG10)")
    (add_net "Net-(U1-PadG13)")
    (add_net "Net-(U1-PadG14)")
    (add_net "Net-(U1-PadG2)")
    (add_net "Net-(U1-PadG3)")
    (add_net "Net-(U1-PadG4)")
    (add_net "Net-(U1-PadG5)")
    (add_net "Net-(U1-PadG6)")
    (add_net "Net-(U1-PadG7)")
    (add_net "Net-(U1-PadH1)")
    (add_net "Net-(U1-PadH11)")
    (add_net "Net-(U1-PadH13)")
    (add_net "Net-(U1-PadH14)")
    (add_net "Net-(U1-PadH15)")
    (add_net "Net-(U1-PadH2)")
    (add_net "Net-(U1-PadH3)")
    (add_net "Net-(U1-PadH4)")
    (add_net "Net-(U1-PadJ1)")
    (add_net "Net-(U1-PadJ12)")
    (add_net "Net-(U1-PadJ13)")
    (add_net "Net-(U1-PadJ14)")
    (add_net "Net-(U1-PadJ2)")
    (add_net "Net-(U1-PadJ3)")
    (add_net "Net-(U1-PadJ4)")
    (add_net "Net-(U1-PadJ5)")
    (add_net "Net-(U1-PadK1)")
    (add_net "Net-(U1-PadK12)")
    (add_net "Net-(U1-PadK13)")
    (add_net "Net-(U1-PadK14)")
    (add_net "Net-(U1-PadK2)")
    (add_net "Net-(U1-PadK3)")
    (add_net "Net-(U1-PadK4)")
    (add_net "Net-(U1-PadK5)")
    (add_net "Net-(U1-PadK6)")
    (add_net "Net-(U1-PadK8)")
    (add_net "Net-(U1-PadL1)")
    (add_net "Net-(U1-PadL14)")
    (add_net "Net-(U1-PadL2)")
    (add_net "Net-(U1-PadL3)")
    (add_net "Net-(U1-PadL4)")
    (add_net "Net-(U1-PadL5)")
    (add_net "Net-(U1-PadL6)")
    (add_net "Net-(U1-PadL7)")
    (add_net "Net-(U1-PadL8)")
    (add_net "Net-(U1-PadL9)")
    (add_net "Net-(U1-PadM1)")
    (add_net "Net-(U1-PadM11)")
    (add_net "Net-(U1-PadM13)")
    (add_net "Net-(U1-PadM15)")
    (add_net "Net-(U1-PadM2)")
    (add_net "Net-(U1-PadM3)")
    (add_net "Net-(U1-PadM4)")
    (add_net "Net-(U1-PadM5)")
    (add_net "Net-(U1-PadN1)")
    (add_net "Net-(U1-PadN12)")
    (add_net "Net-(U1-PadN13)")
    (add_net "Net-(U1-PadN15)")
    (add_net "Net-(U1-PadN2)")
    (add_net "Net-(U1-PadN3)")
    (add_net "Net-(U1-PadN4)")
    (add_net "Net-(U1-PadN8)")
    (add_net "Net-(U1-PadN9)")
    (add_net "Net-(U1-PadP1)")
    (add_net "Net-(U1-PadP10)")
    (add_net "Net-(U1-PadP11)")
    (add_net "Net-(U1-PadP12)")
    (add_net "Net-(U1-PadP13)")
    (add_net "Net-(U1-PadP14)")
    (add_net "Net-(U1-PadP18)")
    (add_net "Net-(U1-PadP2)")
    (add_net "Net-(U1-PadP3)")
    (add_net "Net-(U1-PadP4)")
    (add_net "Net-(U1-PadP8)")
    (add_net "Net-(U1-PadP9)")
    (add_net "Net-(U1-PadR10)")
    (add_net "Net-(U1-PadR11)")
    (add_net "Net-(U1-PadR14)")
    (add_net "Net-(U1-PadR15)")
    (add_net "Net-(U1-PadR5)")
    (add_net "Net-(U1-PadR6)")
    (add_net "Net-(U1-PadU11)")
    (add_net "Net-(U1-PadU5)")
    (add_net "Net-(U1-PadV10)")
    (add_net "Net-(U1-PadV11)")
    (add_net "Net-(U1-PadV5)")
    (add_net "Net-(U1-PadY13)")
    (add_net "Net-(U1-PadY14)")
    (add_net "Net-(U1-PadY16)")
    (add_net "Net-(U1-PadY17)")
    (add_net "Net-(U1-PadY19)")
    (add_net "Net-(U1-PadY20)")
  )
  (net_class eMMC ""
    (clearance 0.1)
    (trace_width 0.1524)
    (via_dia 0.66)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /E_DIR)
    (add_net /E_FAULT)
    (add_net /Flash/MMC1_CLK)
    (add_net /Flash/MMC1_CMD)
    (add_net /Flash/MMC1_DAT0)
    (add_net /Flash/MMC1_DAT1)
    (add_net /Flash/MMC1_DAT2)
    (add_net /Flash/MMC1_DAT3)
    (add_net /Flash/MMC1_DAT4)
    (add_net /Flash/MMC1_DAT5)
    (add_net /Flash/MMC1_DAT6)
    (add_net /Flash/MMC1_DAT7)
    (add_net /H_DIR)
    (add_net /USR0)
    (add_net /X_STEP)
    (add_net /Y1_ENDSTOP)
    (add_net /Y_STEP)
    (add_net /Z_DIR)
    (add_net /Z_STEP)
    (add_net "Net-(U5-PadA10)")
    (add_net "Net-(U5-PadA11)")
    (add_net "Net-(U5-PadA12)")
    (add_net "Net-(U5-PadA13)")
    (add_net "Net-(U5-PadA14)")
    (add_net "Net-(U5-PadA6)")
    (add_net "Net-(U5-PadA7)")
    (add_net "Net-(U5-PadB1)")
    (add_net "Net-(U5-PadB10)")
    (add_net "Net-(U5-PadB11)")
    (add_net "Net-(U5-PadB12)")
    (add_net "Net-(U5-PadB13)")
    (add_net "Net-(U5-PadB14)")
    (add_net "Net-(U5-PadB9)")
    (add_net "Net-(U5-PadC10)")
    (add_net "Net-(U5-PadC11)")
    (add_net "Net-(U5-PadC12)")
    (add_net "Net-(U5-PadC13)")
    (add_net "Net-(U5-PadC14)")
    (add_net "Net-(U5-PadC8)")
    (add_net "Net-(U5-PadC9)")
    (add_net "Net-(U5-PadD12)")
    (add_net "Net-(U5-PadD13)")
    (add_net "Net-(U5-PadD14)")
    (add_net "Net-(U5-PadE10)")
    (add_net "Net-(U5-PadE12)")
    (add_net "Net-(U5-PadE13)")
    (add_net "Net-(U5-PadE14)")
    (add_net "Net-(U5-PadE5)")
    (add_net "Net-(U5-PadE8)")
    (add_net "Net-(U5-PadE9)")
    (add_net "Net-(U5-PadF1)")
    (add_net "Net-(U5-PadF10)")
    (add_net "Net-(U5-PadF12)")
    (add_net "Net-(U5-PadF13)")
    (add_net "Net-(U5-PadF14)")
    (add_net "Net-(U5-PadF3)")
    (add_net "Net-(U5-PadG10)")
    (add_net "Net-(U5-PadG12)")
    (add_net "Net-(U5-PadG13)")
    (add_net "Net-(U5-PadG14)")
    (add_net "Net-(U5-PadG2)")
    (add_net "Net-(U5-PadG3)")
    (add_net "Net-(U5-PadH1)")
    (add_net "Net-(U5-PadH12)")
    (add_net "Net-(U5-PadH13)")
    (add_net "Net-(U5-PadH14)")
    (add_net "Net-(U5-PadH2)")
    (add_net "Net-(U5-PadH3)")
    (add_net "Net-(U5-PadH5)")
    (add_net "Net-(U5-PadJ1)")
    (add_net "Net-(U5-PadJ12)")
    (add_net "Net-(U5-PadJ13)")
    (add_net "Net-(U5-PadJ14)")
    (add_net "Net-(U5-PadJ2)")
    (add_net "Net-(U5-PadJ3)")
    (add_net "Net-(U5-PadJ5)")
    (add_net "Net-(U5-PadK1)")
    (add_net "Net-(U5-PadK10)")
    (add_net "Net-(U5-PadK12)")
    (add_net "Net-(U5-PadK13)")
    (add_net "Net-(U5-PadK14)")
    (add_net "Net-(U5-PadK2)")
    (add_net "Net-(U5-PadK3)")
    (add_net "Net-(U5-PadK6)")
    (add_net "Net-(U5-PadK7)")
    (add_net "Net-(U5-PadL1)")
    (add_net "Net-(U5-PadL12)")
    (add_net "Net-(U5-PadL13)")
    (add_net "Net-(U5-PadL14)")
    (add_net "Net-(U5-PadL2)")
    (add_net "Net-(U5-PadL3)")
    (add_net "Net-(U5-PadM1)")
    (add_net "Net-(U5-PadM10)")
    (add_net "Net-(U5-PadM11)")
    (add_net "Net-(U5-PadM12)")
    (add_net "Net-(U5-PadM13)")
    (add_net "Net-(U5-PadM14)")
    (add_net "Net-(U5-PadM2)")
    (add_net "Net-(U5-PadM3)")
    (add_net "Net-(U5-PadM8)")
    (add_net "Net-(U5-PadM9)")
    (add_net "Net-(U5-PadN1)")
    (add_net "Net-(U5-PadN10)")
    (add_net "Net-(U5-PadN11)")
    (add_net "Net-(U5-PadN12)")
    (add_net "Net-(U5-PadN13)")
    (add_net "Net-(U5-PadN14)")
    (add_net "Net-(U5-PadN3)")
    (add_net "Net-(U5-PadN9)")
    (add_net "Net-(U5-PadP1)")
    (add_net "Net-(U5-PadP10)")
    (add_net "Net-(U5-PadP11)")
    (add_net "Net-(U5-PadP12)")
    (add_net "Net-(U5-PadP13)")
    (add_net "Net-(U5-PadP14)")
    (add_net "Net-(U5-PadP7)")
  )
  (net_class eMMC_RSTN ""
    (clearance 0.05)
    (trace_width 0.1524)
    (via_dia 0.66)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Flash/EMMC_RSTN)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5942FDA5)
    (at 213.63 38.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C48 (at 0.25 2.19 360) (layer F.SilkS))
    (fp_text value 39nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 /Y1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5942FDA0)
    (at 215.43 38.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R98 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /Y1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5942FD98)
    (at 214.38 36.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R97 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /Y1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 619 "Net-(FB54-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5942E6C6)
    (at 200.61 38.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R94 (at 0 -2.15 360) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 617 "Net-(FB52-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /ADC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5942E6CC)
    (at 198.06 39.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C46 (at 0.4 1.55) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 /ADC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5942E6D4)
    (at 198.61 35.95 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R93 (at -1.15 -2.21 180) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 VDD_ADC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 /Thermistors/ADC_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:MountingHole_3mm_Pad locked (layer F.Cu) (tedit 592EEE90)
    (at 58 156)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (zone_connect 2))
  )
  (module KiMBo:Crystal_C_0402 (layer F.Cu) (tedit 5925F278)
    (at 163.605 88.94451 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C41 (at -1.25549 -0.005 180) (layer F.SilkS))
    (fp_text value 18pF (at 0 1.7 90) (layer F.Fab))
    (pad 2 smd rect (at 0.5 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 657 "Net-(C41-Pad2)") (solder_mask_margin 0.1))
    (pad 1 smd rect (at -0.5 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 555 "Net-(C41-Pad1)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Crystal_C_0402 (layer F.Cu) (tedit 5925F269)
    (at 163.605 87.16549 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C42 (at -0.66549 -1.195 360) (layer F.SilkS))
    (fp_text value 18pF (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.5 0 270) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 657 "Net-(C41-Pad2)") (solder_mask_margin 0.1))
    (pad 1 smd rect (at -0.5 0 270) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 578 "Net-(C42-Pad1)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Crystal_C_0402 (layer F.Cu) (tedit 5925F25E)
    (at 163.605 92.24549 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C44 (at -1.24549 0.005 360) (layer F.SilkS))
    (fp_text value 18pF (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 659 "Net-(C44-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.5 0 270) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 658 "Net-(C43-Pad2)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Crystal_C_0402 (layer F.Cu) (tedit 5925F28B)
    (at 163.605 94.02451 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C43 (at -1.37549 -0.105 180) (layer F.SilkS))
    (fp_text value 18pF (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 646 "Net-(C43-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.5 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 658 "Net-(C43-Pad2)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5925F263)
    (at 165.05 88.055 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R89 (at -1.645 0.25 180) (layer F.SilkS))
    (fp_text value DNP-1MΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 578 "Net-(C42-Pad1)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 555 "Net-(C41-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232273)
    (at 168.51 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB24 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 605 "Net-(FB24-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923226E)
    (at 163.43 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB26 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI1_MOSI))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 607 "Net-(FB26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232271)
    (at 165.97 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB25 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 606 "Net-(FB25-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI1_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232275)
    (at 171.05 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB23 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 604 "Net-(FB23-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923226C)
    (at 160.89 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB27 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 /~SS_DOCK1_T))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 608 "Net-(FB27-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232269)
    (at 158.35 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB28 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 /~SS_DOCK1_NVM))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 609 "Net-(FB28-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232278)
    (at 173.59 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB22 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 603 "Net-(FB22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232261)
    (at 147.65 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB16 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 597 "Net-(FB16-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923225C)
    (at 142.57 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB18 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI1_MISO))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 599 "Net-(FB18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232259)
    (at 140.03 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB19 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 600 "Net-(FB19-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI1_MOSI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232254)
    (at 134.95 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB21 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 602 "Net-(FB21-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 /~SS_DOCK0_NVM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232256)
    (at 137.49 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB20 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 601 "Net-(FB20-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /~SS_DOCK0_T))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923225E)
    (at 145.11 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB17 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 598 "Net-(FB17-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232264)
    (at 150.19 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB15 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 596 "Net-(FB15-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923223B)
    (at 111.55 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB14 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 507 /~SS_H_NVM))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 595 "Net-(FB14-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232249)
    (at 121.71 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB10 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 591 "Net-(FB10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232246)
    (at 119.17 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB11 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 592 "Net-(FB11-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI1_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232240)
    (at 114.09 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB13 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 581 /~SS_H_T))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 594 "Net-(FB13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923224E)
    (at 126.79 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB8 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 589 "Net-(FB8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923224B)
    (at 124.25 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB9 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 590 "Net-(FB9-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232243)
    (at 116.63 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB12 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI1_MOSI))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 593 "Net-(FB12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F09F4)
    (at 72.5 59.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R196 (at -1.8 0 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 571 "Net-(Q16-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F09CC)
    (at 76.5 60.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R198 (at 1.85 -1 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 563 "Net-(D28-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 564 "Net-(D29-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 78.5 64.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R194 (at 0 2.6 180) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 570 "Net-(Q15-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 525 /Fans/E_FAN_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 78 58.5507 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D29 (at -0.7 1.2507 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 564 "Net-(D29-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 65.5 57.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C190 (at 1.4 1.2 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 520 /Fans/E_FAN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:MBR-DO-214AC (layer F.Cu) (tedit 58F78FAA)
    (at 69 63.8)
    (attr smd)
    (fp_text reference D28 (at 2.2 -1.7) (layer F.SilkS))
    (fp_text value MBRA340T3 (at 0 3.29946) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 563 "Net-(D28-Pad1)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 591F09AA)
    (at 65.5 59.8 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB64 (at -0.9 -1.5 180) (layer F.SilkS))
    (fp_text value CIM21J202NE (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 563 "Net-(D28-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 520 /Fans/E_FAN))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57FE9788)
    (at 69.5 60.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q16 (at 0.4 2.2 180) (layer F.SilkS))
    (fp_text value DMP3098L-7 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 571 "Net-(Q16-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 563 "Net-(D28-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57FE9788)
    (at 75.50178 64.3 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q15 (at -1.4 -2.20178 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 569 "Net-(Q15-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 570 "Net-(Q15-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F09C1)
    (at 74.5 61.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R197 (at -1.6 0 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 571 "Net-(Q16-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 569 "Net-(Q15-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F0A01)
    (at 64.5 62.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R199 (at 1.9 0.3 360) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 520 /Fans/E_FAN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 57FE9780)
    (at 61.2 62.34 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P31 (at 3 4.44 180) (layer F.SilkS))
    (fp_text value E_FAN (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 520 /Fans/E_FAN))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 78.5 61.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R195 (at 0 -2.6 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 525 /Fans/E_FAN_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 591F3C95)
    (at 61.2 53.34 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P32 (at 3 4.44 180) (layer F.SilkS))
    (fp_text value H_FAN (at 0 -3.1 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /Fans/H_FAN))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 591F3CAD)
    (at 65.5 50.8 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB65 (at -0.9 -1.5 180) (layer F.SilkS))
    (fp_text value CIM21J202NE (at 0 2.1 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /Fans/H_FAN))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 565 "Net-(D30-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3D21)
    (at 72.5 50.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at -1.8 0 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 574 "Net-(Q18-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 591F3CB7)
    (at 65.5 48.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C191 (at 1.4 1.2 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 /Fans/H_FAN))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:MBR-DO-214AC (layer F.Cu) (tedit 591F3CF8)
    (at 69 54.8)
    (attr smd)
    (fp_text reference D30 (at 2.2 -1.7) (layer F.SilkS))
    (fp_text value MBRA340T3 (at 0 3.29946) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 565 "Net-(D30-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3D0E)
    (at 78.5 55.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R200 (at 0 2.6 180) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 526 /Fans/H_FAN_IN))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 573 "Net-(Q17-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3D12)
    (at 78.5 52.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at 0 -2.6 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 526 /Fans/H_FAN_IN))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3D2E)
    (at 76.5 51.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.85 -1 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 566 "Net-(D31-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 565 "Net-(D30-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3CBF)
    (at 64.5 53.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R205 (at 1.9 0.3 360) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /Fans/H_FAN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3D25)
    (at 74.5 52.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R203 (at -1.6 0 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 572 "Net-(Q17-Pad3)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 574 "Net-(Q18-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 591F3CEF)
    (at 78 49.5507 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D31 (at -0.7 1.2507 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 566 "Net-(D31-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591F3CCB)
    (at 69.5 51.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q18 (at 0.4 2.2 180) (layer F.SilkS))
    (fp_text value DMP3098L-7 (at 0 2.3 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 565 "Net-(D30-Pad1)"))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 574 "Net-(Q18-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591F3CD9)
    (at 75.50178 55.3 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q17 (at -1.4 -2.20178 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 573 "Net-(Q17-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 572 "Net-(Q17-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 591F3C99)
    (at 61.2 44.34 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P33 (at 3 4.44 180) (layer F.SilkS))
    (fp_text value CASE_FAN (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /Fans/CASE_FAN))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 591F3D79)
    (at 65.5 41.8 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB66 (at -0.9 -1.5 180) (layer F.SilkS))
    (fp_text value CIM21J202NE (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 567 "Net-(D32-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /Fans/CASE_FAN))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3DA5)
    (at 72.5 41.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R208 (at -1.8 0 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 577 "Net-(Q20-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 591F3DE8)
    (at 65.5 39.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C192 (at 1.4 1.2 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 /Fans/CASE_FAN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3D8B)
    (at 78.5 46.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R206 (at 0 2.6 180) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 575 "Net-(Q19-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 527 /Fans/CASE_FAN_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 591F3D97)
    (at 78 40.5507 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D33 (at -0.7 1.2507 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 568 "Net-(D33-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module KiMBo:MBR-DO-214AC (layer F.Cu) (tedit 591F3E3B)
    (at 69 45.8)
    (attr smd)
    (fp_text reference D32 (at 2.2 -1.7) (layer F.SilkS))
    (fp_text value MBRA340T3 (at 0 3.29946) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 567 "Net-(D32-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3DA9)
    (at 74.5 43.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R209 (at -1.6 0 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 577 "Net-(Q20-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 576 "Net-(Q19-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3E49)
    (at 64.5 44.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R211 (at 1.9 0.3 360) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /Fans/CASE_FAN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3D8F)
    (at 78.5 43.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R207 (at 0 -2.6 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 527 /Fans/CASE_FAN_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591F3E09)
    (at 75.50178 46.3 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q19 (at -1.4 -2.20178 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 576 "Net-(Q19-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 575 "Net-(Q19-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591F3E1A)
    (at 69.5 42.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q20 (at 0.4 2.2 180) (layer F.SilkS))
    (fp_text value DMP3098L-7 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 577 "Net-(Q20-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 567 "Net-(D32-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591F3DF5)
    (at 76.5 42.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R210 (at 1.85 -1 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 567 "Net-(D32-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 568 "Net-(D33-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:IHLP_Inductor (layer F.Cu) (tedit 591345CF)
    (at 114.15 119)
    (descr "Neosid, Inductor, SM-NE56, SMD2220, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM-NE56, SMD2220, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference L1 (at 0.1 -5.7) (layer F.SilkS))
    (fp_text value 47μH (at 0 4.20116) (layer F.Fab))
    (pad 1 smd rect (at -4.4705 0) (size 3.124 3.251) (layers F.Cu F.Paste F.Mask)
      (net 477 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 4.4705 0) (size 3.124 3.251) (layers F.Cu F.Paste F.Mask)
      (net 649 "Net-(C7-Pad1)"))
  )
  (module KiMBo:c_elec_16x16.5 (layer F.Cu) (tedit 5913566B)
    (at 98.15 110.15)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (attr smd)
    (fp_text reference C6 (at 0 -9.35) (layer F.SilkS))
    (fp_text value 470μF (at 0 6.35) (layer F.Fab))
    (pad 2 smd rect (at -6.25 0) (size 6.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 3.5))
    (pad 1 smd rect (at 6.25 0) (size 6.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.6 1.6 1.6191))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 143.45 108.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.25 -1.75 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 648 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:MBR-DO-214AC (layer F.Cu) (tedit 591C86CB)
    (at 70.9 76.01)
    (attr smd)
    (fp_text reference D25 (at 1 -2.5) (layer F.SilkS))
    (fp_text value MBRA340T3 (at 0 3.29946) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 538 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C86A2)
    (at 79.9 75.51 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R183 (at 0 2.5 180) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 551 "Net-(Q12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 524 /Heaters/DOCK1_HEAT_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C8760)
    (at 63.9 75.51 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R193 (at 1.9 -0.4 540) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /Heaters/DOCK1_HEAT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C871C)
    (at 77.9 71.51 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R191 (at 2 -0.5 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 538 "Net-(D25-Pad1)") (thermal_gap 0.3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 539 "Net-(D27-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C86FF)
    (at 75.9 72.51 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R189 (at 1.25 2.5 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 552 "Net-(Q12-Pad3)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 554 "Net-(Q14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C86F6)
    (at 75.9 69.51 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R188 (at -2 0 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.432))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 554 "Net-(Q14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_1812 (layer F.Cu) (tedit 591C8758)
    (at 66.525 71.57 180)
    (descr "Resistor SMD 1812, flow soldering, Panasonic (see ERJ12)")
    (tags "resistor 1812")
    (attr smd)
    (fp_text reference FB63 (at 0.625 -2.94 180) (layer F.SilkS))
    (fp_text value FBMH4532HM132-T (at 0 3.175 180) (layer F.Fab))
    (pad 1 smd rect (at -2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 538 "Net-(D25-Pad1)") (thermal_width 0.939) (thermal_gap 0.26))
    (pad 2 smd rect (at 2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 26 /Heaters/DOCK1_HEAT) (thermal_width 0.939) (thermal_gap 0.26))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591C873B)
    (at 72.90076 71.46 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q14 (at 0 2.45 180) (layer F.SilkS))
    (fp_text value DMP3098L-7 (at 0 2.3 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.3))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 538 "Net-(D25-Pad1)"))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 554 "Net-(Q14-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 591C8749)
    (at 66.525 68.51 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C189 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 /Heaters/DOCK1_HEAT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591C870A)
    (at 76.9 75.51 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q12 (at 2.5 1 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 552 "Net-(Q12-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.391))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 551 "Net-(Q12-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 591C86D6)
    (at 78.9 69.31 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D27 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 539 "Net-(D27-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C86B3)
    (at 79.9 72.51 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R185 (at -1.8 -1 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 524 /Heaters/DOCK1_HEAT_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_1812 (layer F.Cu) (tedit 591C838D)
    (at 66.525 83.9 180)
    (descr "Resistor SMD 1812, flow soldering, Panasonic (see ERJ12)")
    (tags "resistor 1812")
    (attr smd)
    (fp_text reference FB61 (at 0.625 -2.94 180) (layer F.SilkS))
    (fp_text value FBMH4532HM132-T (at 0 3.175 180) (layer F.Fab))
    (pad 2 smd rect (at 2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 24 /Heaters/DOCK0_HEAT) (thermal_width 0.939) (thermal_gap 0.26))
    (pad 1 smd rect (at -2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 536 "Net-(D21-Pad1)") (thermal_width 0.939) (thermal_gap 0.26))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 591C8387)
    (at 66.525 80.84 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C187 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 /Heaters/DOCK0_HEAT))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C8354)
    (at 75.9 81.84 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R176 (at -2 0 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 548 "Net-(Q10-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.432))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:MBR-DO-214AC (layer F.Cu) (tedit 591C8381)
    (at 70.9 88.34)
    (attr smd)
    (fp_text reference D21 (at 1 -2.5) (layer F.SilkS))
    (fp_text value MBRA340T3 (at 0 3.29946) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.3))
    (pad 1 smd rect (at -2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 536 "Net-(D21-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C8361)
    (at 77.9 83.84 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R179 (at 2 -0.5 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 561 "Net-(D23-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 536 "Net-(D21-Pad1)") (thermal_gap 0.3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591C8348)
    (at 76.9 87.84 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 2.5 1 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 547 "Net-(Q8-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.391))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 546 "Net-(Q8-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591C837C)
    (at 72.90076 83.79 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q10 (at 0 2.45 180) (layer F.SilkS))
    (fp_text value DMP3098L-7 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 548 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 536 "Net-(D21-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C8343)
    (at 79.9 84.84 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R173 (at -1.8 -1 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 522 /Heaters/DOCK0_HEAT_IN))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C8370)
    (at 75.9 84.84 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R177 (at 1.25 2.5 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 548 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 546 "Net-(Q8-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C836A)
    (at 63.9 87.84 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R181 (at 1.9 -0.4 540) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /Heaters/DOCK0_HEAT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C833A)
    (at 79.9 87.84 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R171 (at 0 2.5 180) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 522 /Heaters/DOCK0_HEAT_IN))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 547 "Net-(Q8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 591C83A1)
    (at 78.9 81.64 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D23 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 561 "Net-(D23-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module KiMBo:MBR-DO-214AC (layer F.Cu) (tedit 591C806F)
    (at 70.9 100.67)
    (attr smd)
    (fp_text reference D24 (at 1 -2.5) (layer F.SilkS))
    (fp_text value MBRA340T3 (at 0 3.29946) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 537 "Net-(D24-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C7FA3)
    (at 77.9 96.17 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R190 (at 2 -0.5 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 537 "Net-(D24-Pad1)") (thermal_gap 0.3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 562 "Net-(D26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C7FBB)
    (at 75.9 97.17 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R187 (at 1.25 2.5 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 549 "Net-(Q11-Pad3)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 553 "Net-(Q13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C7F87)
    (at 75.9 94.17 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R186 (at -2 0 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.432))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 553 "Net-(Q13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C7F5D)
    (at 79.9 97.17 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R184 (at -1.8 -1 540) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 523 /Heaters/H_HEAT_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591C7FAE)
    (at 72.90076 96.12 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q13 (at 0 2.45 180) (layer F.SilkS))
    (fp_text value DMP3098L-7 (at 0 2.3 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.3))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 537 "Net-(D24-Pad1)"))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 553 "Net-(Q13-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591C8286)
    (at 76.9 100.17 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q11 (at 2.5 1 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 549 "Net-(Q11-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.391))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 550 "Net-(Q11-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 591C7F73)
    (at 78.9 93.97 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D26 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 562 "Net-(D26-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 591C8062)
    (at 66.525 93.17 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C188 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 /Heaters/H_HEAT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C803E)
    (at 63.9 100.17 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R192 (at 1.9 -0.4 540) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /Heaters/H_HEAT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591C7F4C)
    (at 79.9 100.17 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R182 (at 0 2.5 180) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 550 "Net-(Q11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 523 /Heaters/H_HEAT_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_1812 (layer F.Cu) (tedit 591C8054)
    (at 66.525 96.23 180)
    (descr "Resistor SMD 1812, flow soldering, Panasonic (see ERJ12)")
    (tags "resistor 1812")
    (attr smd)
    (fp_text reference FB62 (at 0.625 -2.94 180) (layer F.SilkS))
    (fp_text value FBMH4532HM132-T (at 0 3.175 180) (layer F.Fab))
    (pad 1 smd rect (at -2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 537 "Net-(D24-Pad1)") (thermal_width 0.939) (thermal_gap 0.26))
    (pad 2 smd rect (at 2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 25 /Heaters/H_HEAT) (thermal_width 0.939) (thermal_gap 0.26))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_1812 (layer F.Cu) (tedit 591626F8)
    (at 66.525 108.56 180)
    (descr "Resistor SMD 1812, flow soldering, Panasonic (see ERJ12)")
    (tags "resistor 1812")
    (attr smd)
    (fp_text reference FB60 (at 0.625 -2.94 180) (layer F.SilkS))
    (fp_text value FBMH4532HM132-T (at 0 3.175 180) (layer F.Fab))
    (pad 2 smd rect (at 2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 23 /Heaters/E_HEAT) (thermal_width 0.939) (thermal_gap 0.26))
    (pad 1 smd rect (at -2.625 0 180) (size 1.75 3.7) (layers F.Cu F.Paste F.Mask)
      (net 480 "Net-(D20-Pad1)") (thermal_width 0.939) (thermal_gap 0.26))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:MBR-DO-214AC (layer F.Cu) (tedit 59132099)
    (at 70.9 113)
    (attr smd)
    (fp_text reference D20 (at 1 -2.5) (layer F.SilkS))
    (fp_text value MBRA340T3 (at 0 3.29946) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.3))
    (pad 1 smd rect (at -2 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 480 "Net-(D20-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 79.9 112.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R170 (at 0 2.5 180) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 503 /Heaters/E_HEAT_IN))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 485 "Net-(Q7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591626E4)
    (at 65.9 119.39 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference FB58 (at -2.9 1.89 180) (layer F.SilkS))
    (fp_text value BLM31SN500SN1L (at 0 2.3 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 /Heaters/BED_HEAT))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 479 "Net-(D18-Pad1)") (thermal_width 3.5) (thermal_gap 0.254))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591626E8)
    (at 65.9 122.39 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference FB59 (at -1.3 -1.9 180) (layer F.SilkS))
    (fp_text value BLM31SN500SN1L (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 479 "Net-(D18-Pad1)") (thermal_width 3.5) (thermal_gap 0.254))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 /Heaters/BED_HEAT) (thermal_width 3.5) (thermal_gap 0.254))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 57FE9788)
    (at 79.9 120.89 90)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q6 (at 4.2 -2.6 180) (layer F.SilkS))
    (fp_text value IPD90P03P4-04 (at 0 -2.413 90) (layer F.Fab))
    (pad 1 smd rect (at -2.286 0 90) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 483 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0 -6.35 90) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 479 "Net-(D18-Pad1)"))
    (pad 3 smd rect (at 2.286 0 90) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:3557-2-Fuseholder (layer F.Cu) (tedit 5911F62D)
    (at 64.56 140.83 270)
    (descr "Fuseholder, 5x20, open, horizontal, Type-II, lateral,")
    (tags "Fuseholder, 5x20, open, horizontal, Type-II, lateral, Sicherungshalter, offen,")
    (fp_text reference F2 (at -9.13 0.16 540) (layer F.SilkS))
    (fp_text value 0891020.NXS (at -1.27 6.35 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.735 -1.7 270) (size 2.1 2.1) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 505 "Net-(F2-Pad2)") (thermal_width 3.5) (thermal_gap 0.254))
    (pad 2 thru_hole circle (at 6.735 1.7 270) (size 2.1 2.1) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 505 "Net-(F2-Pad2)") (thermal_width 3.5) (thermal_gap 0.254))
    (pad 1 thru_hole circle (at -6.735 -1.7 270) (size 2.1 2.1) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 504 "Net-(F2-Pad1)") (thermal_width 3.5) (thermal_gap 0.254))
    (pad 1 thru_hole circle (at -6.735 1.7 270) (size 2.1 2.1) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 504 "Net-(F2-Pad1)") (thermal_width 3.5) (thermal_gap 0.254))
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5911FC76)
    (at 214.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C150 (at -6 0 540) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 590B580C)
    (at 78.9 147.7 90)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q4 (at 4.3 -5 180) (layer F.SilkS))
    (fp_text value IPD90P03P4-04 (at 0 -2.413 90) (layer F.Fab))
    (pad 1 smd rect (at -2.286 0 90) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 558 "Net-(D15-Pad2)"))
    (pad 2 smd rect (at 0 -6.35 90) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 505 "Net-(F2-Pad2)") (thermal_width 3.5))
    (pad 3 smd rect (at 2.286 0 90) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 478 "Net-(D15-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A010)
    (at 218.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C145 (at 2.05 -0.09 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 476 "/Stepper Drivers/H_B1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5908A0CE)
    (at 215.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C149 (at -0.00868 2.755376 540) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A04A)
    (at 220.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C136 (at 2.65 0.21 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B1FC)
    (at 215.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C142 (at 1.19 0.9 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 474 "/Stepper Drivers/H_B2"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 5908B3BF)
    (at 225.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P19 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value H_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 473 "/Stepper Drivers/H_A2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 475 "/Stepper Drivers/H_A1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 474 "/Stepper Drivers/H_B2"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 476 "/Stepper Drivers/H_B1"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5908A0B7)
    (at 218.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R148 (at 2 -0.19 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 719 "Net-(R147-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A08B)
    (at 228.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C141 (at 3.31 0.05) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 473 "/Stepper Drivers/H_A2"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A09D)
    (at 228.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C146 (at 3.31 0.05) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5908A0FF)
    (at 220.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R147 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 472 "/Stepper Drivers/H Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 719 "Net-(R147-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A10A)
    (at 224.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C137 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 690 "Net-(C137-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A02E)
    (at 225.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C144 (at 2 -0.2 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 475 "/Stepper Drivers/H_A1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A096)
    (at 216.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C147 (at -0.01 -1.35 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A0C2)
    (at 222.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C139 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 472 "/Stepper Drivers/H Stepper Driver/5VOUT"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B817)
    (at 215.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C148 (at 1.64 0.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 694 "Net-(C148-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908A066)
    (at 228.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R150 (at -3.55 0.05 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 695 "Net-(C151-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A0E6)
    (at 228.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C143 (at 0.05 -2.61 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 693 "Net-(C143-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908B102)
    (at 215.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R149 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 694 "Net-(C148-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A03E)
    (at 228.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C151 (at 3.31 0.05) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 695 "Net-(C151-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A0B0)
    (at 228.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C138 (at -3.31 -0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A0F6)
    (at 226.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C140 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 691 "Net-(C140-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 692 "Net-(C140-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5908A119)
    (at 222.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R146 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 690 "Net-(C137-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 472 "/Stepper Drivers/H Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076F42)
    (at 118.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C76 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 667 "Net-(C76-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 668 "Net-(C76-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076DA0)
    (at 112.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C72 (at 1.95 -0.19 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A9B1)
    (at 120.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C87 (at 0.01 -1.25) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 671 "Net-(C87-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076D90)
    (at 107.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C84 (at 2.9 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 670 "Net-(C84-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A651)
    (at 120.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C77 (at 1.06 -0.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 183 "/Stepper Drivers/X0_A2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076E66)
    (at 107.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C78 (at 2.39 -0.05 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 184 "/Stepper Drivers/X0_B2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076F4B)
    (at 120.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C79 (at 0.05 -2.35 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 669 "Net-(C79-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 591085A3)
    (at 107.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R126 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 670 "Net-(C84-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59076EE2)
    (at 110.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R125 (at 1.95 -0.44 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 715 "Net-(R124-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076EF0)
    (at 114.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C75 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 182 "/Stepper Drivers/X0 Stepper Driver/5VOUT"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076F74)
    (at 116.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C73 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 666 "Net-(C73-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076E9F)
    (at 108.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C83 (at 3.05 -0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908A804)
    (at 120.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R127 (at 2.29 -1.1 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 671 "Net-(C87-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59076F22)
    (at 112.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R124 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 182 "/Stepper Drivers/X0 Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 715 "Net-(R124-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076D75)
    (at 117.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C80 (at 2 -0.2 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 185 "/Stepper Drivers/X0_A1"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5907724E)
    (at 114.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R123 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 182 "/Stepper Drivers/X0 Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 666 "Net-(C73-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 591356C4)
    (at 106.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C86 (at -6 0.5 540) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076E8D)
    (at 120.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C82 (at 2.61 -0.55) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076EB3)
    (at 120.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C74 (at -2.66 -0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59076D64)
    (at 110.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C81 (at 2.05 -0.54 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 186 "/Stepper Drivers/X0_B1"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59076F16)
    (at 107.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C85 (at 0.04132 2.405376 360) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 590B5DC6)
    (at 117.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P20 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value X0_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 183 "/Stepper Drivers/X0_A2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 185 "/Stepper Drivers/X0_A1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 184 "/Stepper Drivers/X0_B2"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 186 "/Stepper Drivers/X0_B1"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5907950D)
    (at 125.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C181 (at 0.04132 2.805376 360) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 5908B3D4)
    (at 135.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P21 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value X1_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 192 "/Stepper Drivers/X1_B1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 190 "/Stepper Drivers/X1_B2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 191 "/Stepper Drivers/X1_A1"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 189 "/Stepper Drivers/X1_A2"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079535)
    (at 136.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C172 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 703 "Net-(C172-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 704 "Net-(C172-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079336)
    (at 130.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C168 (at 2.8 0.31 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079547)
    (at 138.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C170 (at -2.91 -1.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079839)
    (at 138.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C183 (at 0.01 -1.25) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 707 "Net-(C183-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 590795CF)
    (at 132.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R158 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 702 "Net-(C169-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 "/Stepper Drivers/X1 Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 591356AD)
    (at 124.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C182 (at -6 0 540) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590793A6)
    (at 126.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C179 (at -0.26 -1.3 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B4D5)
    (at 138.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C178 (at 1.41 -0.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590792CF)
    (at 128.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C177 (at 2.05 -0.09 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 192 "/Stepper Drivers/X1_B1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590792E1)
    (at 135.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C176 (at 1.95 -0.74 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 191 "/Stepper Drivers/X1_A1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A662)
    (at 125.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C174 (at 1.19 0.9 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 190 "/Stepper Drivers/X1_B2"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908A7FE)
    (at 125.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R161 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 706 "Net-(C180-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908AAA6)
    (at 138.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R162 (at 2.29 -1.1 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 707 "Net-(C183-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 590796B2)
    (at 130.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R159 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 721 "Net-(R159-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 "/Stepper Drivers/X1 Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079517)
    (at 134.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C169 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 702 "Net-(C169-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907942D)
    (at 138.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C175 (at 0.05 -2.35 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 705 "Net-(C175-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079411)
    (at 132.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C171 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 188 "/Stepper Drivers/X1 Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 590793FA)
    (at 128.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R160 (at 2 -0.49 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 721 "Net-(R159-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A9CF)
    (at 125.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C180 (at 1.64 0.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 706 "Net-(C180-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B138)
    (at 138.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C173 (at 1.21 -0.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 189 "/Stepper Drivers/X1_A2"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908B0CB)
    (at 89.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R156 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 700 "Net-(C164-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908AAC1)
    (at 102.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R157 (at 2.29 -1.1 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 701 "Net-(C167-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5907A74B)
    (at 94.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R154 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/Stepper Drivers/Y Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 720 "Net-(R154-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079AE2)
    (at 102.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C154 (at -3.01 -1.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907A7B7)
    (at 98.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C153 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 696 "Net-(C153-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079B04)
    (at 96.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C155 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 199 "/Stepper Drivers/Y Stepper Driver/5VOUT"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079BD8)
    (at 102.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C159 (at 0.05 -2.41 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 699 "Net-(C159-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5907A9C3)
    (at 96.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R153 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/Stepper Drivers/Y Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 696 "Net-(C153-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079A16)
    (at 102.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C167 (at -0.04 -1.25) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 701 "Net-(C167-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B4F7)
    (at 102.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C162 (at 1.41 -0.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59079AA1)
    (at 90.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C163 (at -0.41 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5911FC52)
    (at 88.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C166 (at -6 -1 540) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5907A738)
    (at 89.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C165 (at 1.84132 -2.594624 540) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590799C2)
    (at 92.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C161 (at 2.05 -0.09 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 203 "/Stepper Drivers/Y_B1"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 5908B3D1)
    (at 99.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P22 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value Y_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 200 "/Stepper Drivers/Y_A2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 202 "/Stepper Drivers/Y_A1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 201 "/Stepper Drivers/Y_B2"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 203 "/Stepper Drivers/Y_B1"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590799DB)
    (at 94.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C152 (at 2.55 -0.14 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B1CA)
    (at 89.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C158 (at 1.19 0.9 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 201 "/Stepper Drivers/Y_B2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907A78A)
    (at 100.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C156 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 697 "Net-(C156-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 698 "Net-(C156-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590799CB)
    (at 99.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C160 (at 1.95 -0.74 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 202 "/Stepper Drivers/Y_A1"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59079AF1)
    (at 92.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R155 (at 2 -0.49 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 720 "Net-(R154-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B7AD)
    (at 89.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C164 (at 1.54 0.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 700 "Net-(C164-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B146)
    (at 102.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C157 (at 1.21 -0.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 200 "/Stepper Drivers/Y_A2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B0F9)
    (at 154.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C92 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 673 "Net-(C92-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 674 "Net-(C92-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B054)
    (at 153.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C96 (at 1.95 -0.39 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 197 "/Stepper Drivers/Z0_A1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B187)
    (at 156.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C95 (at 0.05 -2.35 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 675 "Net-(C95-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5907B08D)
    (at 146.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R132 (at 2 -0.49 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 716 "Net-(R131-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B083)
    (at 144.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C99 (at 0.89 -1.3 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B159)
    (at 156.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C93 (at 1.06 -0.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 195 "/Stepper Drivers/Z0_A2"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5911FC60)
    (at 142.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C102 (at -6 0 540) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B505)
    (at 156.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C98 (at 1.41 -0.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B7C0)
    (at 143.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C100 (at 1.49 0.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 676 "Net-(C100-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B0D5)
    (at 150.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C91 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 194 "/Stepper Drivers/Z0 Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5907B0DE)
    (at 150.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R130 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 672 "Net-(C89-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 "/Stepper Drivers/Z0 Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5907B097)
    (at 143.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C101 (at -0.00868 2.705376 540) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B0EB)
    (at 152.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C89 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 672 "Net-(C89-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B145)
    (at 156.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C103 (at -0.04 -1.25) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 677 "Net-(C103-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B212)
    (at 143.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C94 (at 1.19 0.9 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 196 "/Stepper Drivers/Z0_B2"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B04C)
    (at 146.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C97 (at 2.05 -0.09 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 198 "/Stepper Drivers/Z0_B1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5907B09E)
    (at 148.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R131 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 716 "Net-(R131-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 "/Stepper Drivers/Z0 Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 59108F77)
    (at 153.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P23 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value Z0_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 198 "/Stepper Drivers/Z0_B1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 196 "/Stepper Drivers/Z0_B2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 197 "/Stepper Drivers/Z0_A1"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 195 "/Stepper Drivers/Z0_A2"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B106)
    (at 156.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C90 (at -2.66 -0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5907B158)
    (at 148.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C88 (at 2.6 -0.09 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908AACE)
    (at 156.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R134 (at 2.29 -1.1 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 677 "Net-(C103-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908B0D6)
    (at 143.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R133 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 676 "Net-(C100-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59088FB5)
    (at 162.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C115 (at -0.31 -1.3 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908AADD)
    (at 174.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R139 (at 2.29 -1.1 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 683 "Net-(C119-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B7CE)
    (at 161.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C116 (at 1.49 0.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 682 "Net-(C116-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B510)
    (at 174.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C114 (at 1.41 -0.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089004)
    (at 174.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C111 (at 0.05 -2.41 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 681 "Net-(C111-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59088FDE)
    (at 164.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R137 (at 2 -0.24 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 717 "Net-(R136-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5911FC66)
    (at 160.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C118 (at -6 0 540) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B164)
    (at 174.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C109 (at 1.21 -0.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 463 "/Stepper Drivers/Z1_A2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B1D7)
    (at 161.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C110 (at 1.19 0.9 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 464 "/Stepper Drivers/Z1_B2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 59108F7C)
    (at 171.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P24 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value Z1_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 463 "/Stepper Drivers/Z1_A2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 465 "/Stepper Drivers/Z1_A1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 464 "/Stepper Drivers/Z1_B2"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 466 "/Stepper Drivers/Z1_B1"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590898DB)
    (at 166.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C104 (at 2.6 0.21 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59089028)
    (at 166.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R136 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 462 "/Stepper Drivers/Z1 Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 717 "Net-(R136-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089C90)
    (at 174.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C119 (at -0.04 -1.3) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 683 "Net-(C119-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089034)
    (at 170.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C105 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 678 "Net-(C105-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59088FCF)
    (at 174.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C106 (at -2.81 -1.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59088D91)
    (at 164.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C113 (at 2.05 -0.09 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 466 "/Stepper Drivers/Z1_B1"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089021)
    (at 172.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C108 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 679 "Net-(C108-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 680 "Net-(C108-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59088DA9)
    (at 171.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C112 (at 2 -0.69 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 465 "/Stepper Drivers/Z1_A1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59089015)
    (at 161.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C117 (at -0.00868 2.755376 540) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908B0E2)
    (at 161.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R138 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 682 "Net-(C116-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59089047)
    (at 168.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R135 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 462 "/Stepper Drivers/Z1 Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 678 "Net-(C105-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59088FF3)
    (at 168.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C107 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 462 "/Stepper Drivers/Z1 Stepper Driver/5VOUT"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089AB3)
    (at 184.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C120 (at 2.55 -0.09 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B7DF)
    (at 179.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C132 (at 1.64 0.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 688 "Net-(C132-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908B0EE)
    (at 179.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R143 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 688 "Net-(C132-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089B0B)
    (at 180.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C131 (at -0.31 -1.45 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59089B36)
    (at 182.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R142 (at 2 -0.54 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 718 "Net-(R141-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089A97)
    (at 182.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C129 (at 2.05 -0.09 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 471 "/Stepper Drivers/Z2_B1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089D08)
    (at 189.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C128 (at 1.95 -0.29 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 470 "/Stepper Drivers/Z2_A1"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59089B8B)
    (at 179.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C133 (at -0.00868 2.755376 540) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089ABD)
    (at 192.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C135 (at 0.51 -1.25) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 689 "Net-(C135-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908AAEA)
    (at 192.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R144 (at 2.29 -1.1 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 689 "Net-(C135-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089B50)
    (at 186.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C123 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 467 "/Stepper Drivers/Z2 Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B16F)
    (at 192.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C125 (at 1.21 -0.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 468 "/Stepper Drivers/Z2_A2"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59089BBB)
    (at 186.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R140 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 684 "Net-(C121-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 467 "/Stepper Drivers/Z2 Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B51B)
    (at 192.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C130 (at 1.41 -0.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B1E5)
    (at 179.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C126 (at 1.19 0.9 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 469 "/Stepper Drivers/Z2_B2"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089BA2)
    (at 190.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C124 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 685 "Net-(C124-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 686 "Net-(C124-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59089B98)
    (at 184.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R141 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 718 "Net-(R141-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 467 "/Stepper Drivers/Z2 Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089B6B)
    (at 192.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C127 (at 0.05 -2.35 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 687 "Net-(C127-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089B23)
    (at 192.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C122 (at -2.96 -1.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5911FC6B)
    (at 178.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C134 (at -6 0 540) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59089BB1)
    (at 188.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C121 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 684 "Net-(C121-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 59108F85)
    (at 189.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P25 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value Z2_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 471 "/Stepper Drivers/Z2_B1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 469 "/Stepper Drivers/Z2_B2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 470 "/Stepper Drivers/Z2_A1"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 468 "/Stepper Drivers/Z2_A2"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59020DA8)
    (at 200.24 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R118 (at 2 -0.44 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 641 "Net-(R117-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B17B)
    (at 210.59 140.95)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C61 (at 1.06 -0.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "/Stepper Drivers/E_A2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908A0A9)
    (at 210.49 144.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C138 (at -3.11 -0.95 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59011468)
    (at 200.19 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C65 (at 2.05 -0.54 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "/Stepper Drivers/E_B1"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5911FC71)
    (at 196.79 130.25 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C70 (at -6 0 360) (layer F.SilkS))
    (fp_text value 100μF (at 0 5.08 270) (layer F.Fab))
    (pad 2 smd rect (at -3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2))
    (pad 1 smd rect (at 3.2512 0 270) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590113EF)
    (at 208.69 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C60 (at 2.05 -0.45 540) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 661 "Net-(C60-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 662 "Net-(C60-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B7F0)
    (at 197.29 136.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C68 (at 1.24 0.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 664 "Net-(C68-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59022C79)
    (at 204.59 147.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C59 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Stepper Drivers/E Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590113BF)
    (at 198.19 143.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C67 (at -0.31 -1.35 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59020D5C)
    (at 204.59 149.15)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R116 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.2Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Stepper Drivers/E Stepper Driver/5VOUT"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 660 "Net-(C57-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59011446)
    (at 207.99 137.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C64 (at 2 -0.2 360) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "/Stepper Drivers/E_A1"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59011517)
    (at 206.99 147.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C57 (at 2.45 -0.65 540) (layer F.SilkS))
    (fp_text value 470nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 660 "Net-(C57-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590113E0)
    (at 210.39 146.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C63 (at 0.05 -2.35 540) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 663 "Net-(C63-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908AAF8)
    (at 210.89 138.65 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R120 (at 2.29 -1.1 180) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 665 "Net-(C71-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 590113C9)
    (at 197.505376 149.15868 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C69 (at 0.04132 2.405376 360) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59020D83)
    (at 202.14 147.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R117 (at -1.95 -0.75 180) (layer F.SilkS))
    (fp_text value 5.23kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 641 "Net-(R117-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Stepper Drivers/E Stepper Driver/5VOUT"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B45C)
    (at 210.49 142.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C66 (at 2.61 -0.55) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5908B1F2)
    (at 197.59 140.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C62 (at 1.19 0.9 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "/Stepper Drivers/E_B2"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59011718)
    (at 202.59 136.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C56 (at 2.6 -0.29 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 5908B3C3)
    (at 207.9 152.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P18 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value E_MOTOR (at 0 -3.1 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "/Stepper Drivers/E_B1"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "/Stepper Drivers/E_B2"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "/Stepper Drivers/E_A1"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "/Stepper Drivers/E_A2"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590114C0)
    (at 210.89 136.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C71 (at -0.09 -1.25) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 665 "Net-(C71-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5908B0F9)
    (at 197.29 138.65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R119 (at 2.21 1.1) (layer F.SilkS))
    (fp_text value 220mΩ (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 664 "Net-(C68-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57FE9780)
    (at 161.08 65 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value Serial (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /USB/UART0_RXD))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /USB/UART0_TXD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiMBo:USB_MICRO_B_ST-USB-001E (layer F.Cu) (tedit 58F8DBB3)
    (at 239.2 111 90)
    (descr "USB Micro-B 5-pin SMD connector")
    (tags "USB, Micro-B, connector")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference P12 (at 4.5274 1.3716 90) (layer F.SilkS))
    (fp_text value μUSB (at 0 3.5 90) (layer F.SilkS) hide)
    (pad 11 smd rect (at 3.1 -2.55 90) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 10 smd rect (at -3.1 -2.55 90) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 4 smd rect (at 0.65 -2.675 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 55 /USB/USB.CLIENT.ID))
    (pad 2 smd rect (at -0.65 -2.675 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 56 /USB/USB.CLIENT.D-))
    (pad 3 smd rect (at 0 -2.675 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 57 /USB/USB.CLIENT.D+))
    (pad 1 smd rect (at -1.3 -2.675 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 USB_DC))
    (pad 5 smd rect (at 1.3 -2.675 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 6 smd rect (at 3.8 0 90) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 7 smd rect (at 1.2 0 90) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 8 smd rect (at -1.2 0 90) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 9 smd rect (at -3.8 0 90) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
  )
  (module Connect:USB_A (layer F.Cu) (tedit 5543E289)
    (at 226.60212 78.77286 90)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P13 (at 0 -2.35 90) (layer F.SilkS))
    (fp_text value USB_Type_A (at 3.83794 7.43458 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11286 -0.00212) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 3 thru_hole circle (at 4.57286 -0.00212) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 58 /USB/USB.HOST.D+))
    (pad 2 thru_hole circle (at 2.54086 -0.00212) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 59 /USB/USB.HOST.D-))
    (pad 1 thru_hole circle (at 0.00086 -0.00212) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 44 /USB/USB.B.VBUS))
    (pad 5 thru_hole circle (at 10.16086 2.66488) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 5 thru_hole circle (at -3.55514 2.66488) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (model Connect.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiMBo:euro_header_2_angled (layer F.Cu) (tedit 591C813C)
    (at 58 111.1 270)
    (descr "Euro header 4 pins")
    (tags DEV)
    (fp_text reference P27 (at -3.6 8.6 360) (layer F.SilkS))
    (fp_text value E_HEAT (at 0 5.334 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 23 /Heaters/E_HEAT) (thermal_width 0.939))
    (model /home/aleph/workspace/Lulzbot_Custom_PCB/layout/modules/packages3d/euro_header_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:euro_header_2_angled (layer F.Cu) (tedit 591C812B)
    (at 58 98.77 270)
    (descr "Euro header 4 pins")
    (tags DEV)
    (fp_text reference P28 (at 0 -5.334 270) (layer F.SilkS))
    (fp_text value H_HEAT (at 0 5.334 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 25 /Heaters/H_HEAT))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (model /home/aleph/workspace/Lulzbot_Custom_PCB/layout/modules/packages3d/euro_header_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:euro_header_2_angled (layer F.Cu) (tedit 591C8143)
    (at 58 86.44 270)
    (descr "Euro header 4 pins")
    (tags DEV)
    (fp_text reference P29 (at 0 -5.334 270) (layer F.SilkS))
    (fp_text value DOCK0_HEAT (at 0 5.334 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 24 /Heaters/DOCK0_HEAT))
    (model /home/aleph/workspace/Lulzbot_Custom_PCB/layout/modules/packages3d/euro_header_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:euro_header_2_angled (layer F.Cu) (tedit 591C8149)
    (at 58 74.11 270)
    (descr "Euro header 4 pins")
    (tags DEV)
    (fp_text reference P30 (at 0 -5.334 270) (layer F.SilkS))
    (fp_text value DOCK1_HEAT (at 0 5.334 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 26 /Heaters/DOCK1_HEAT))
    (model /home/aleph/workspace/Lulzbot_Custom_PCB/layout/modules/packages3d/euro_header_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x07 (layer F.Cu) (tedit 57FE9780)
    (at 64.75 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P17 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value LCD (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 615 "Net-(FB34-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 614 "Net-(FB33-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 613 "Net-(FB32-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 612 "Net-(FB31-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 611 "Net-(FB30-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 610 "Net-(FB29-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiMBo:euro_header_2_angled (layer F.Cu) (tedit 5911F644)
    (at 58 123.43 270)
    (descr "Euro header 4 pins")
    (tags DEV)
    (fp_text reference P26 (at -0.03 7 270) (layer F.SilkS))
    (fp_text value BED_HEAT (at 0 5.334 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (thermal_width 3.5) (thermal_gap 0.254))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 22 /Heaters/BED_HEAT) (thermal_width 3.5) (thermal_gap 0.254))
    (model /home/aleph/workspace/Lulzbot_Custom_PCB/layout/modules/packages3d/euro_header_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:euro_header_4_angled (layer F.Cu) (tedit 5910E584)
    (at 58 140.84 270)
    (descr "Euro header 4 pins")
    (tags DEV)
    (fp_text reference P35 (at 0 -5.334 270) (layer F.SilkS))
    (fp_text value PWR_Input (at 0 5.334 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (thermal_width 3.5) (thermal_gap 0.254))
    (pad 1 thru_hole oval (at -7.62 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 504 "Net-(F2-Pad1)") (thermal_width 3.5) (thermal_gap 0.254))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (thermal_width 3.5) (thermal_gap 0.254))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 2.1 4.2) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 504 "Net-(F2-Pad1)") (thermal_width 3.5) (thermal_gap 0.254))
    (model /home/aleph/workspace/Lulzbot_Custom_PCB/layout/modules/packages3d/euro_header_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:DGN-MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 58F8EF66)
    (at 212.5 73.575)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U6 (at 0 -2.6) (layer F.SilkS))
    (fp_text value TPS2051B (at 0 2.6) (layer F.Fab))
    (pad 8 smd rect (at 2.1 -0.975) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(C23-Pad1)") (solder_mask_margin 0.07))
    (pad 7 smd rect (at 2.1 -0.325) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(C23-Pad1)") (solder_mask_margin 0.07))
    (pad 6 smd rect (at 2.1 0.325) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(C23-Pad1)") (solder_mask_margin 0.07))
    (pad 5 smd rect (at 2.1 0.975) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 100 /~USB1_OC) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -2.1 0.975) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 99 /USB/USB1_DRVVBUS) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.1 0.325) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 SYS_5V) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.1 -0.325) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 SYS_5V) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -2.1 -0.975) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 0 0) (size 1.57 1.89) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 57FE977A)
    (at 146 69 270)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U11 (at 0 -3.55 270) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 3.55 270) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 /~SS_DOCK1_NVM))
    (pad 2 smd rect (at -2.95 -1.625 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 /~SS_DOCK0_T))
    (pad 3 smd rect (at -2.95 -0.975 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /~SS_DOCK0_NVM))
    (pad 4 smd rect (at -2.95 -0.325 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 713 "Net-(R109-Pad2)"))
    (pad 5 smd rect (at -2.95 0.325 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 507 /~SS_H_NVM))
    (pad 6 smd rect (at -2.95 0.975 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 714 "Net-(R111-Pad2)"))
    (pad 7 smd rect (at -2.95 1.625 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 506 /~SS_E_NVM))
    (pad 8 smd rect (at -2.95 2.275 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 9 smd rect (at 2.95 2.275 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U11-Pad9)"))
    (pad 10 smd rect (at 2.95 1.625 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 115 /~SR_EN))
    (pad 11 smd rect (at 2.95 0.975 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 12 smd rect (at 2.95 0.325 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 135 /SPI1_CS0))
    (pad 13 smd rect (at 2.95 -0.325 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 115 /~SR_EN))
    (pad 14 smd rect (at 2.95 -0.975 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI1_MOSI))
    (pad 15 smd rect (at 2.95 -1.625 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 /~SS_DOCK1_T))
    (pad 16 smd rect (at 2.95 -2.275 270) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:SCHA5B0200 (layer F.Cu) (tedit 58F8DD59)
    (at 241.2 125.4 90)
    (solder_mask_margin 0.1)
    (fp_text reference P14 (at -10.16 0 90) (layer F.SilkS))
    (fp_text value μSD (at 0 -16.51 90) (layer F.Fab))
    (pad 15 smd rect (at 7.1875 0 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 14 smd rect (at -7.1875 0 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 4 smd rect (at -7.1875 -1.265 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 5 smd rect (at 7.1875 -1.265 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 /MMC0_CLK))
    (pad 3 smd rect (at -7.1875 -1.965 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 61 /MMC0_CMD))
    (pad 6 smd rect (at 7.1875 -1.965 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 7 smd rect (at 7.1875 -2.665 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 /MMC0_DAT0))
    (pad 2 smd rect (at -7.1875 -2.665 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 /MMC0_DAT3))
    (pad 8 smd rect (at 7.1875 -3.365 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 64 /MMC0_DAT1))
    (pad 1 smd rect (at -7.1875 -3.365 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 65 /MMC0_DAT2))
    (pad 16 smd rect (at 7.1875 -9.7 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -7.1875 -11 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 9 smd rect (at -5.975 -13.35 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -3.425 -13.925 90) (size 1.2 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 11 smd rect (at 2.575 -13.925 90) (size 1.2 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 10 smd rect (at 3.775 -13.35 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /SD.CD))
  )
  (module KiMBo:Ethernet-LPJ0011BBNL (layer F.Cu) (tedit 58FA76D4)
    (at 235.6 94.9 90)
    (fp_text reference P15 (at 0 -9 90) (layer F.SilkS))
    (fp_text value Ethernet (at 0 -10.5 90) (layer F.Fab))
    (pad "" thru_hole circle (at 5.715 0 90) (size 3.8 3.8) (drill 3.8) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.715 0 90) (size 3.8 3.8) (drill 3.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 7.875 -3.05 90) (size 2.357 2.357) (drill 2.28) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 13 thru_hole circle (at -7.875 -3.05 90) (size 2.357 2.357) (drill 2.28) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 12 thru_hole circle (at 6.325 3.38 90) (size 1.597 1.597) (drill 1.52) (layers *.Cu *.Mask)
      (net 67 /Ethernet/YELA))
    (pad 11 thru_hole circle (at 3.785 4.9 90) (size 1.597 1.597) (drill 1.52) (layers *.Cu *.Mask)
      (net 180 "Net-(P15-Pad11)"))
    (pad 10 thru_hole circle (at -3.785 3.38 90) (size 1.597 1.597) (drill 1.52) (layers *.Cu *.Mask)
      (net 181 "Net-(P15-Pad10)"))
    (pad 9 thru_hole circle (at -6.325 4.9 90) (size 1.597 1.597) (drill 1.52) (layers *.Cu *.Mask)
      (net 68 /Ethernet/GRNA))
    (pad 8 thru_hole circle (at 4.445 -7.27 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 7 thru_hole circle (at 3.175 -4.73 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 204 "Net-(P15-Pad7)"))
    (pad 6 thru_hole circle (at 1.905 -7.27 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 /Ethernet/TD-))
    (pad 5 thru_hole circle (at 0.635 -4.73 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 160 "Net-(C2-Pad1)"))
    (pad 4 thru_hole circle (at -0.635 -7.27 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 160 "Net-(C2-Pad1)"))
    (pad 3 thru_hole circle (at -1.905 -4.73 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 /Ethernet/TD+))
    (pad 2 thru_hole circle (at -3.175 -7.27 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 /Ethernet/RD-))
    (pad 1 thru_hole circle (at -4.445 -4.73 90) (size 1.577 1.577) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 /Ethernet/RD+))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 590B4DDB)
    (at 76.4 138.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -2.3 0.2 360) (layer F.SilkS))
    (fp_text value 22μF (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.372))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 590B4DD5)
    (at 74.15 138.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.3 0.05 360) (layer F.SilkS))
    (fp_text value 22μF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.372))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 590A3DED)
    (at 65.9 117.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C185 (at 0.25 1.25 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /Heaters/BED_HEAT))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:SMA-DO-214AC (layer F.Cu) (tedit 5909F587)
    (at 83.4 147.7 270)
    (attr smd)
    (fp_text reference D15 (at -3.7 -2.8 360) (layer F.SilkS))
    (fp_text value SMAZ10 (at 0 3.29946 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 558 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 478 "Net-(D15-Pad1)"))
  )
  (module KiMBo:SK-DO-214AC (layer F.Cu) (tedit 591084AE)
    (at 70.65 139.45 270)
    (attr smd)
    (fp_text reference D16 (at -4.85 0 540) (layer F.SilkS))
    (fp_text value SMAJ26A (at 0 3.29946 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.032 0 270) (size 1.778 2.159) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 1.5) (thermal_gap 0.27))
    (pad 1 smd rect (at -2.032 0 270) (size 1.778 2.159) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
  )
  (module KiMBo:SK-DO-214AB (layer F.Cu) (tedit 590B4C73)
    (at 72.4 128.5 180)
    (attr smd)
    (fp_text reference D18 (at 0 -3.8 180) (layer F.SilkS))
    (fp_text value SK1545-TP (at 0 3.8 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.302 0 180) (size 1.778 5.08) (layers F.Cu F.Paste F.Mask)
      (net 479 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 3.302 0 180) (size 1.778 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 3.5))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 79.9 126)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D19 (at 0 -1.1) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 559 "Net-(D19-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591626A8)
    (at 82.15 139.2 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference FB40 (at 4.5 0.55 180) (layer F.SilkS))
    (fp_text value BLM31SN500SN1L (at 0 2.3 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 478 "Net-(D15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591626A4)
    (at 79.15 139.2 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference FB39 (at 4.5 -0.45 180) (layer F.SilkS))
    (fp_text value BLM31SN500SN1L (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 478 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 59132108)
    (at 86.4 117.75 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at -2 -1.25 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 482 "Net-(Q5-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.331))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 481 "Net-(Q5-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 590B4CC7)
    (at 83.4 153 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 2 0 360) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 558 "Net-(D15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 86.4 115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R164 (at -3.5 -0.5) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 502 /Heaters/BED_HEAT_IN))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 481 "Net-(Q5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591083A7)
    (at 86.4 113)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R165 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 502 /Heaters/BED_HEAT_IN))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.282))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 83.15 121.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R166 (at 0.55 -2.45 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 483 "Net-(Q6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 85.65 120.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R167 (at -2.05 -1.5) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 483 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 482 "Net-(Q5-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 79.9 128)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R168 (at 0 1.5) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 479 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 559 "Net-(D19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 591324F4)
    (at 63.9 125.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R169 (at 2.1 -0.4 360) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.341))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /Heaters/BED_HEAT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-263-5Lead (layer F.Cu) (tedit 5913466F)
    (at 114.15 110.15 90)
    (descr "D2PAK / TO-263 3-lead smd package")
    (tags "D2PAK D2PAK-3 TO-263AB TO-263")
    (attr smd)
    (fp_text reference U3 (at 15.15 0.1 180) (layer F.SilkS))
    (fp_text value LM2592HVSX-5.0 (at 15.25 -0.25 180) (layer F.Fab))
    (pad 5 smd rect (at 0 3.4 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 1.06))
    (pad 4 smd rect (at 0 1.7 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 649 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0 -1.7 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 477 "Net-(D13-Pad1)"))
    (pad 3 smd rect (at 9.15 0 90) (size 9.4 10.8) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 3.5))
    (pad 3 smd rect (at 0 0 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 1.1))
    (pad 1 smd rect (at 0 -3.4 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model TO_SOT_Packages_SMD.3dshapes/TO-263-5Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59131B77)
    (at 66.525 105.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C186 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 /Heaters/E_HEAT))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 78.9 106.3 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D22 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 560 "Net-(D22-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 59131F39)
    (at 76.9 112.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at 2.5 1 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 485 "Net-(Q7-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.391))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 484 "Net-(Q7-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 591332B4)
    (at 72.90076 108.45 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q9 (at 0 2.45 180) (layer F.SilkS))
    (fp_text value DMP3098L-7 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 486 "Net-(Q9-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 480 "Net-(D20-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5912328E)
    (at 79.9 109.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R172 (at -1.8 -1 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 503 /Heaters/E_HEAT_IN))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59123DE5)
    (at 75.9 106.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R174 (at -2 0 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 486 "Net-(Q9-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V) (thermal_gap 0.432))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 75.9 109.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R175 (at 1.25 2.5 360) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 486 "Net-(Q9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 484 "Net-(Q7-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59131EAA)
    (at 77.9 108.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R178 (at 2 -0.5 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 560 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 480 "Net-(D20-Pad1)") (thermal_gap 0.3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5913362B)
    (at 63.9 112.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R180 (at 1.9 -0.4 360) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /Heaters/E_HEAT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_gap 0.432))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x03 (layer F.Cu) (tedit 57FE9780)
    (at 179.21 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P34 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value PWM (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 543 "Net-(FB36-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 542 "Net-(FB35-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiMBo:c_elec_8x10.2 (layer F.Cu) (tedit 591355E5)
    (at 126.15 114 180)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (attr smd)
    (fp_text reference C7 (at 0 5.08 180) (layer F.SilkS))
    (fp_text value 220μF (at 0 5.08 180) (layer F.Fab))
    (pad 1 smd rect (at 3.55 0 180) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 649 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -3.55 0 180) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 2.3))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:SK-DO-214AC (layer F.Cu) (tedit 59134957)
    (at 103.65 121 180)
    (attr smd)
    (fp_text reference D13 (at 4.6 0 180) (layer F.SilkS))
    (fp_text value SK54A-LTP (at 0 3.29946 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.032 0 180) (size 1.778 2.159) (layers F.Cu F.Paste F.Mask)
      (net 477 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 2.032 0 180) (size 1.778 2.159) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (thermal_width 1.5))
  )
  (module KiMBo:SOD-923 (layer F.Cu) (tedit 591355F6)
    (at 122.15 119.45 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D14 (at 0 -2.2 360) (layer F.SilkS))
    (fp_text value D5V0F1U2S9 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 649 "Net-(C7-Pad1)"))
  )
  (module Housings_SSOP:TSSOP-28_4.4x9.7mm_Pitch0.65mm (layer F.Cu) (tedit 57FE977A)
    (at 131 86.86)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U21 (at 0 -5.9) (layer F.SilkS))
    (fp_text value PCA9685 (at 0 5.9) (layer F.Fab))
    (pad 1 smd rect (at -2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 528 "Net-(U21-Pad1)"))
    (pad 2 smd rect (at -2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 528 "Net-(U21-Pad1)"))
    (pad 3 smd rect (at -2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 528 "Net-(U21-Pad1)"))
    (pad 4 smd rect (at -2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 528 "Net-(U21-Pad1)"))
    (pad 5 smd rect (at -2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 528 "Net-(U21-Pad1)"))
    (pad 6 smd rect (at -2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 527 /Fans/CASE_FAN_IN))
    (pad 7 smd rect (at -2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 526 /Fans/H_FAN_IN))
    (pad 8 smd rect (at -2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 525 /Fans/E_FAN_IN))
    (pad 9 smd rect (at -2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 524 /Heaters/DOCK1_HEAT_IN))
    (pad 10 smd rect (at -2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 522 /Heaters/DOCK0_HEAT_IN))
    (pad 11 smd rect (at -2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 523 /Heaters/H_HEAT_IN))
    (pad 12 smd rect (at -2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 503 /Heaters/E_HEAT_IN))
    (pad 13 smd rect (at -2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 502 /Heaters/BED_HEAT_IN))
    (pad 14 smd rect (at -2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 15 smd rect (at 2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 711 "Net-(U21-Pad15)"))
    (pad 16 smd rect (at 2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 712 "Net-(U21-Pad16)"))
    (pad 17 smd rect (at 2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 529 "Net-(U21-Pad17)"))
    (pad 18 smd rect (at 2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 530 "Net-(U21-Pad18)"))
    (pad 19 smd rect (at 2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 531 "Net-(U21-Pad19)"))
    (pad 20 smd rect (at 2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 532 "Net-(U21-Pad20)"))
    (pad 21 smd rect (at 2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 533 "Net-(U21-Pad21)"))
    (pad 22 smd rect (at 2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 534 "Net-(U21-Pad22)"))
    (pad 23 smd rect (at 2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 /CLKOUT2))
    (pad 24 smd rect (at 2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 528 "Net-(U21-Pad1)"))
    (pad 25 smd rect (at 2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 535 "Net-(U21-Pad25)"))
    (pad 26 smd rect (at 2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 136 /I2C2_SCL))
    (pad 27 smd rect (at 2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 137 /I2C2_SDA))
    (pad 28 smd rect (at 2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Housings_SSOP.3dshapes/TSSOP-28_4.4x9.7mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0805 (layer F.Cu) (tedit 59232475)
    (at 184.29 36.1 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB35 (at 1.95 0 180) (layer F.SilkS))
    (fp_text value MPZ2012S601AT000 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 542 "Net-(FB35-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 57FE9780)
    (at 189.91 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value BED_THERM (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /Thermistors/BED_THERM_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 57FE9780)
    (at 198.07 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value ADC (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /Thermistors/ADC_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 592321FD)
    (at 69.83 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB33 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 /SPI0_CS0))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 614 "Net-(FB33-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232202)
    (at 72.37 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB32 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 613 "Net-(FB32-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 541 /SPI0_MOSI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923220B)
    (at 74.91 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB31 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 612 "Net-(FB31-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 39 /SPI0_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232217)
    (at 77.45 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB30 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 540 /SPI0_SCLK))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 611 "Net-(FB30-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923221A)
    (at 79.99 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB29 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 610 "Net-(FB29-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x08 (layer F.Cu) (tedit 5922FECA)
    (at 109.01 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value TOOLHEAD1 (at 0 -3.1 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 589 "Net-(FB8-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 590 "Net-(FB9-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 591 "Net-(FB10-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 592 "Net-(FB11-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 593 "Net-(FB12-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 594 "Net-(FB13-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 595 "Net-(FB14-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x08 (layer F.Cu) (tedit 5922FED2)
    (at 85.61 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value TOOLHEAD0 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 588 "Net-(FB7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 587 "Net-(FB6-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 586 "Net-(FB5-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 585 "Net-(FB4-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 584 "Net-(FB3-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 583 "Net-(FB2-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 582 "Net-(FB1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x08 (layer F.Cu) (tedit 57FE9780)
    (at 132.41 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value DOCK0 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 602 "Net-(FB21-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 601 "Net-(FB20-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 600 "Net-(FB19-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 599 "Net-(FB18-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 598 "Net-(FB17-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 597 "Net-(FB16-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 596 "Net-(FB15-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x08 (layer F.Cu) (tedit 57FE9780)
    (at 155.81 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value DOCK1 (at 0 -3.1 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 603 "Net-(FB22-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 604 "Net-(FB23-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 605 "Net-(FB24-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 606 "Net-(FB25-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 607 "Net-(FB26-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 608 "Net-(FB27-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 609 "Net-(FB28-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 59232671)
    (at 214.39 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value Y1 (at 0 -3.1 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /Endstops/Y1_IN))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 59232678)
    (at 222.55 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value X1 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /Endstops/X1_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 59232681)
    (at 230.71 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value ENC (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /Endstops/ENC_A_IN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /Endstops/ENC_B_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 59232669)
    (at 206.23 32.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value Z1 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /Endstops/Z1_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232237)
    (at 103.39 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB1 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 582 "Net-(FB1-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232234)
    (at 100.85 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB2 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 583 "Net-(FB2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232231)
    (at 98.31 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB3 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 584 "Net-(FB3-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923222F)
    (at 95.77 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB4 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI1_MISO))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 585 "Net-(FB4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232229)
    (at 93.23 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB5 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 586 "Net-(FB5-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI1_MOSI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232226)
    (at 90.69 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB6 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 587 "Net-(FB6-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 580 /~SS_E_T))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 5923221E)
    (at 88.15 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB7 (at 1.75 0 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 588 "Net-(FB7-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 506 /~SS_E_NVM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:TPD_PX1SON (layer F.Cu) (tedit 58F78B3D)
    (at 211 35.9 270)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D17 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value TPD1E04U04DPYR (at 0 -1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.5 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.5 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /Endstops/Z1_IN))
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 59232469)
    (at 181.75 36.1 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB36 (at 1.95 0 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 579 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 543 "Net-(FB36-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 192.45 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB51 (at 0.3 2.65 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 616 "Net-(FB51-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 /Thermistors/BED_THERM_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 200.61 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB52 (at 0.3 2.59 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 617 "Net-(FB52-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 /Thermistors/ADC_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 225.09 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB53 (at 0 2.61 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 /Endstops/X1_IN))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 618 "Net-(FB53-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 216.93 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB54 (at 0 2.57 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 /Endstops/Y1_IN))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 619 "Net-(FB54-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 208.77 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB55 (at 0.09906 -2.30124 90) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 620 "Net-(FB55-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /Endstops/Z1_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 230.71 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB56 (at -2 -0.01 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 647 "Net-(FB56-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 /Endstops/ENC_A_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 233.25 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB57 (at -2 1.25 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 50 /Endstops/ENC_B_IN))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 710 "Net-(FB57-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5925F296)
    (at 165.05 93.135 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R90 (at -1.565 -0.05 180) (layer F.SilkS))
    (fp_text value 1MΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 646 "Net-(C43-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 659 "Net-(C44-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:DCT-MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 58F8E4CF)
    (at 157.27 70 270)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U8 (at 0 -2.6 270) (layer F.SilkS))
    (fp_text value 74LVC2G241 (at 0 2.6 270) (layer F.Fab))
    (pad 1 smd rect (at -1.7 -0.975 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.7 -0.325 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /USB/UART0_RXD) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.7 0.325 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 /USB/UART0_TXD) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -1.7 0.975 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.7 0.975 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 139 /USB/UART0_TXD_OUT) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 1.7 0.325 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 138 /USB/UART0_RXD_IN) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 1.7 -0.325 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 1.7 -0.975 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.07))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 158.755 76 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -2 -1.245 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 540 /SPI0_SCLK))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 151.475 76.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FE9765)
    (at 163.5 116.7)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.4 0) (layer F.SilkS))
    (fp_text value 2.2μF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 168.95 78 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0 -2.2 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57FE9783)
    (at 154 77.4 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference FB44 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value BLM15AG102SN1D (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /CLKOUT2))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 545 "Net-(FB44-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5939764A)
    (at 166.2 78 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference IC1 (at -1 -2.4 180) (layer F.SilkS))
    (fp_text value 24LC32AT-I/OT (at -0.05 2.35 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 51 /I2C0_SCL))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 52 /I2C0_SDA))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 623 "Net-(IC1-Pad5)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 165.25 74.35 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R38 (at 1.9 -0.4 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 623 "Net-(IC1-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57FE977C)
    (at 167.3 74.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP5 (at 0.4 -1.6) (layer F.SilkS))
    (fp_text value Test_Point (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 623 "Net-(IC1-Pad5)"))
  )
  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57FE9788)
    (at 164.4104 111.1964 180)
    (descr "SC70-5 SOT323-5")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U4 (at -1.2896 2.0964 180) (layer F.SilkS))
    (fp_text value 74LVC1G06 (at 0 2.3 180) (layer F.Fab))
    (pad 5 smd rect (at -0.6604 -1.016 180) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 4 smd rect (at 0.6604 -1.016 180) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 624 "Net-(R32-Pad2)"))
    (pad 2 smd rect (at 0 1.016 180) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U1-PadR14)"))
    (pad 3 smd rect (at 0.6604 1.016 180) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.6604 1.016 180) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:DRY-DFN-6-1EP_2x2mm_Pitch0.5mm (layer F.Cu) (tedit 58F8F373)
    (at 221.6 73.9)
    (descr "DC6 Package; 6-Lead Plastic DFN (2mm x 2mm) (see Linear Technology DFN_6_05-08-1703.pdf)")
    (tags "DFN 0.5")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U7 (at 0 -2.05) (layer F.SilkS))
    (fp_text value TPD4S012 (at 0 2.05) (layer F.Fab))
    (pad 1 smd rect (at -0.37 -0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 /USB/USB.HOST.D+))
    (pad 2 smd rect (at -0.37 0) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 /USB/USB.HOST.D-))
    (pad 3 smd rect (at -0.37 0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 642 "Net-(U7-Pad3)"))
    (pad 4 smd rect (at 0.37 0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 5 smd rect (at 0.37 0) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 643 "Net-(U7-Pad5)"))
    (pad 6 smd rect (at 0.37 -0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(C23-Pad1)"))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:DRY-DFN-6-1EP_2x2mm_Pitch0.5mm (layer F.Cu) (tedit 58F8F373)
    (at 227.97 111.4)
    (descr "DC6 Package; 6-Lead Plastic DFN (2mm x 2mm) (see Linear Technology DFN_6_05-08-1703.pdf)")
    (tags "DFN 0.5")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U9 (at 0 -2.05) (layer F.SilkS))
    (fp_text value TPD4S012 (at 0 2.05) (layer F.Fab))
    (pad 6 smd rect (at 0.37 -0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 USB_DC))
    (pad 5 smd rect (at 0.37 0) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 644 "Net-(U9-Pad5)"))
    (pad 4 smd rect (at 0.37 0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 3 smd rect (at -0.37 0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 /USB/USB.CLIENT.ID))
    (pad 2 smd rect (at -0.37 0) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 /USB/USB.CLIENT.D-))
    (pad 1 smd rect (at -0.37 -0.5) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 /USB/USB.CLIENT.D+))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 59306D01)
    (at 220.6 94.9)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference U10 (at 0 -3.75) (layer F.SilkS))
    (fp_text value LAN8710A (at 0 3.75) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA) (clearance 0.15))
    (pad 2 smd rect (at -2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 /Ethernet/YELA))
    (pad 3 smd rect (at -2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 /Ethernet/GRNA))
    (pad 4 smd rect (at -2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 627 "Net-(R53-Pad1)"))
    (pad 5 smd rect (at -2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 638 /Ethernet/RCLKIN))
    (pad 6 smd rect (at -2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 622 /Ethernet/PHY_VDDCR))
    (pad 7 smd rect (at -2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 628 /Ethernet/REFCLKO))
    (pad 8 smd rect (at -2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 629 /Ethernet/RXD3/PHYAD2) (clearance 0.15))
    (pad 9 smd rect (at -1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 630 /Ethernet/RXD2/RMIISEL) (clearance 0.15))
    (pad 10 smd rect (at -1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 631 /Ethernet/RXD1/MODE1))
    (pad 11 smd rect (at -0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 632 /Ethernet/RXD0/MODE0))
    (pad 12 smd rect (at -0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 13 smd rect (at 0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 634 /Ethernet/RXER/PHYAD0))
    (pad 14 smd rect (at 0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 637 /Ethernet/CRS))
    (pad 15 smd rect (at 1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 636 /Ethernet/MODE2))
    (pad 16 smd rect (at 1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 113 /Ethernet/MDIO_DATA) (clearance 0.15))
    (pad 17 smd rect (at 2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 145 /Ethernet/MDIO_CLK) (clearance 0.15))
    (pad 18 smd rect (at 2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 640 /Ethernet/ETH_TXD4))
    (pad 19 smd rect (at 2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
    (pad 20 smd rect (at 2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 635 /Ethernet/TXCLK))
    (pad 21 smd rect (at 2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 140 /Ethernet/MII1_TXEN))
    (pad 22 smd rect (at 2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 144 /Ethernet/MII1_TXD0))
    (pad 23 smd rect (at 2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 143 /Ethernet/MII1_TXD1))
    (pad 24 smd rect (at 2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 142 /Ethernet/MII1_TXD2) (clearance 0.15))
    (pad 25 smd rect (at 1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 141 /Ethernet/MII1_TXD3) (clearance 0.15))
    (pad 26 smd rect (at 1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 633 /Ethernet/RXDV))
    (pad 27 smd rect (at 0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 28 smd rect (at 0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Ethernet/TD-))
    (pad 29 smd rect (at -0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /Ethernet/TD+))
    (pad 30 smd rect (at -0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /Ethernet/RD-))
    (pad 31 smd rect (at -1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /Ethernet/RD+))
    (pad 32 smd rect (at -1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 639 /Ethernet/RBIAS) (clearance 0.15))
    (pad 33 smd rect (at 0.8625 0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:MountingHole_3mm_Pad locked (layer F.Cu) (tedit 592EEE90)
    (at 58 156)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (zone_connect 2))
  )
  (module KiMBo:MountingHole_3mm_Pad locked (layer F.Cu) (tedit 592EEEF2)
    (at 58 29)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (zone_connect 2))
  )
  (module KiMBo:MountingHole_3mm_Pad locked (layer F.Cu) (tedit 592EEF0B)
    (at 240 29)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (zone_connect 2))
  )
  (module KiMBo:MountingHole_3mm_Pad locked (layer F.Cu) (tedit 592EEF24)
    (at 240 156)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 CGND) (zone_connect 2))
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 151.475 77.7 180)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB46 (at 0.09906 -2.30124 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 557 "Net-(FB46-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 157.255 76 270)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB42 (at -2 0.755 360) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 653 "Net-(FB42-Pad2)"))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 540 /SPI0_SCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0805 (layer F.Cu) (tedit 59307EA4)
    (at 126.15 106.4)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB38 (at 0.09906 -2.30124) (layer F.SilkS))
    (fp_text value MPZ2012S601AT000 (at -0.20066 2.70002) (layer F.Fab))
    (pad 2 smd rect (at 0.9 0) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (pad 1 smd rect (at -0.9 0) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 556 "Net-(F1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:PTC_SMD0805_Reflow (layer F.Cu) (tedit 59161EBD)
    (at 122.6 107.5 90)
    (descr "PTC, SMD1206, Littlefuse, Reflow,")
    (tags "PTC, SMD1206,  Littlefuse, Reflow,")
    (attr smd)
    (fp_text reference F1 (at -0.09906 -2.75082 90) (layer F.SilkS))
    (fp_text value PTC (at -0.44958 3.2004 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 649 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 556 "Net-(F1-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 164.55 85.4 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at -2.95 0.1 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 136 /I2C2_SCL))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 164.5 83.9 180)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB48 (at -3.8 0 180) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 709 "Net-(FB48-Pad2)"))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 136 /I2C2_SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 223.6 53.45 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 223.6 59.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 166.8 111.1964 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 2.2 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 145.5 110.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 3.2 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FE9765)
    (at 145.5 112.3 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 3.2 0 180) (layer F.SilkS))
    (fp_text value 2.2μF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 145.5 116.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 3.2 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FE9765)
    (at 145.5 114.9 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 3.2 0 180) (layer F.SilkS))
    (fp_text value 2.2μF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FE9765)
    (at 164.9 105.7)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.6) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 650 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 163.4 107.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 2.9 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 650 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 164.5 80.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at -2.8 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 51 /I2C0_SCL))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer F.Cu) (tedit 57FE9765)
    (at 207.1 67.05 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C22 (at -0.20066 -3.29946 90) (layer F.SilkS))
    (fp_text value 220μF (at -0.09906 3.59918 90) (layer F.Fab))
    (pad 2 smd rect (at 3.12 0 90) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -3.12 0 90) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 5 SYS_5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 142 69 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C52 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 150 69 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C54 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 131.2 94.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C184 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 148 77 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB45 (at 0.09906 -2.30124 90) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI1_MOSI))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 654 "Net-(FB45-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 164.5 82.34)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB47 (at 3.2 0) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 51 /I2C0_SCL))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 708 /SIP_I2C0_SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57FE9788)
    (at 182 41)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 76 /SERVO_0))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 579 "Net-(D7-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 228.25 57.4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 /JTAG/JTAG_EMU0))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 218.95 53.95 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 /JTAG/JTAG_EMU1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 218.95 61.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 /JTAG/~JTAG_TRST))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 155.5 77 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 /CLKOUT2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R29-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 163 114.695)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at 2.7 0.005) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /Flash/EMMC_RSTN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 624 "Net-(R32-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CAC4)
    (at 145.515 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R42 (at 1.7 0.385 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /Flash/MMC1_CMD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CACB)
    (at 147.315 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R43 (at -1.9 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /Flash/MMC1_CLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CBC3)
    (at 149.115 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R40 (at 1.7 0.385 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CB5F)
    (at 150.915 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R39 (at -1.9 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 /Flash/MMC1_DAT5))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CE6C)
    (at 152.715 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at 1.75 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /Flash/MMC1_DAT3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CCD8)
    (at 154.515 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at -1.85 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 /Flash/MMC1_DAT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CE5B)
    (at 156.315 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 1.75 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /Flash/MMC1_DAT2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CCEB)
    (at 158.115 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R41 (at -1.95 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 /Flash/MMC1_DAT7))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CE61)
    (at 159.915 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 1.75 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 /Flash/MMC1_DAT1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935CCF6)
    (at 161.715 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at -1.95 0 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 /Flash/MMC1_DAT4))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5935C65A)
    (at 163.515 120.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R44 (at 1.75 0.485 180) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /Flash/EMMC_RSTN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 141.45 65.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R111 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 714 "Net-(R111-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 146.325 62.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R113 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 581 /~SS_H_T))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 713 "Net-(R109-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 144.605 62.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R114 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 580 /~SS_E_T))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 714 "Net-(R111-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57FE9788)
    (at 162 76.5)
    (descr "SC70-5 SOT323-5")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U2 (at 0.75 -2.3) (layer F.SilkS))
    (fp_text value 74LVC1G06 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.6604 1.016) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.6604 1.016) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0 1.016) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 131 /Power/PMIC_PGOOD))
    (pad 4 smd rect (at 0.6604 -1.016) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
    (pad 5 smd rect (at -0.6604 -1.016) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 141.15 107.3 180)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB37 (at 0.65 -1.5 180) (layer F.SilkS))
    (fp_text value MPZ1608S102ATA00 (at -0.20066 2.70002 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 648 "Net-(C5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 67.29 35.9 90)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB34 (at 0.09906 -2.30124 90) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 615 "Net-(FB34-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 41 /~DISP_INT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:JTAG (layer F.Cu) (tedit 58FA6A4B)
    (at 234.2 55.325 90)
    (descr "Molex Slimstack receptacle 02X10 contacts 0.5mm pitch 1.5mm height")
    (tags "Slimstack 1.5mm 02x10 0.5mm pitch")
    (attr smd)
    (fp_text reference P16 (at 0 5.75 90) (layer F.SilkS))
    (fp_text value JTAG (at 0 -5.25 90) (layer F.Fab))
    (pad 1 smd rect (at 5.715 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 69 /JTAG/JTAG_TMS))
    (pad 2 smd rect (at 5.715 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 70 /JTAG/~JTAG_TRST))
    (pad 3 smd rect (at 4.445 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 71 /JTAG/JTAG_TDI))
    (pad 4 smd rect (at 4.445 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 5 smd rect (at 3.175 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 6 smd rect (at 3.175 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(P16-Pad6)"))
    (pad 7 smd rect (at 1.905 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 72 /JTAG/JTAG_TD0))
    (pad 8 smd rect (at 1.905 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 9 smd rect (at 0.635 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 73 /TCK))
    (pad 10 smd rect (at 0.635 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 11 smd rect (at -0.635 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 73 /TCK))
    (pad 12 smd rect (at -0.635 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -1.905 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 74 /JTAG/JTAG_EMU0))
    (pad 14 smd rect (at -1.905 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 75 /JTAG/JTAG_EMU1))
    (pad 15 smd rect (at -3.175 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
    (pad 16 smd rect (at -3.175 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 17 smd rect (at -4.445 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 42 /XDMA_EVENT_INTRO))
    (pad 18 smd rect (at -4.445 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 43 /CLKOUT2))
    (pad 19 smd rect (at -5.715 -2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 66 /SD.CD))
    (pad 20 smd rect (at -5.715 2.7 90) (size 0.7 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
  )
  (module KiMBo:BGA-400-1-27mm (layer F.Cu) (tedit 59247C40)
    (at 149 92.5 270)
    (solder_mask_margin 0.1)
    (clearance 0.15)
    (fp_text reference U1 (at 0 14.605 270) (layer F.SilkS))
    (fp_text value OSD3358 (at 0 -14.478 270) (layer F.Fab))
    (pad Y20 smd circle (at 12.065 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 350 "Net-(U1-PadY20)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y17 smd circle (at 12.065 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 349 "Net-(U1-PadY17)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y18 smd circle (at 12.065 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y19 smd circle (at 12.065 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 348 "Net-(U1-PadY19)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y11 smd circle (at 12.065 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 VDD_3V3AUX) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y12 smd circle (at 12.065 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y14 smd circle (at 12.065 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 347 "Net-(U1-PadY14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y13 smd circle (at 12.065 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 346 "Net-(U1-PadY13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y15 smd circle (at 12.065 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y16 smd circle (at 12.065 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 345 "Net-(U1-PadY16)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y6 smd circle (at 12.065 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 648 "Net-(C5-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y7 smd circle (at 12.065 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y5 smd circle (at 12.065 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 648 "Net-(C5-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y3 smd circle (at 12.065 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 127 /Power/VIN_BAT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y4 smd circle (at 12.065 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 SYS_5V) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y2 smd circle (at 12.065 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 127 /Power/VIN_BAT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y1 smd circle (at 12.065 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 126 /Power/BAT_VOLT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y8 smd circle (at 12.065 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 USB_DC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y9 smd circle (at 12.065 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 USB_DC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad Y10 smd circle (at 12.065 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W20 smd circle (at 10.795 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W17 smd circle (at 10.795 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W18 smd circle (at 10.795 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W19 smd circle (at 10.795 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W11 smd circle (at 10.795 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W12 smd circle (at 10.795 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W14 smd circle (at 10.795 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W13 smd circle (at 10.795 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W15 smd circle (at 10.795 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W16 smd circle (at 10.795 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W6 smd circle (at 10.795 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W7 smd circle (at 10.795 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W5 smd circle (at 10.795 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W3 smd circle (at 10.795 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W4 smd circle (at 10.795 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 SYS_5V) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W2 smd circle (at 10.795 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W1 smd circle (at 10.795 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 125 /Power/BAT_TEMP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W8 smd circle (at 10.795 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W9 smd circle (at 10.795 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad W10 smd circle (at 10.795 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V20 smd circle (at 9.525 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V19 smd circle (at 9.525 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V18 smd circle (at 9.525 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V17 smd circle (at 9.525 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 645 "Net-(U1-PadV17)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V14 smd circle (at 9.525 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /Y1_ENDSTOP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V16 smd circle (at 9.525 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 78 /USR3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V15 smd circle (at 9.525 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 81 /USR0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V6 smd circle (at 9.525 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 156 /X_DIR) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V5 smd circle (at 9.525 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(U1-PadV5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V4 smd circle (at 9.525 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 162 /Configuration/LCD.D14.R3--R6) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V2 smd circle (at 9.525 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 164 /Configuration/LCD.D12.R1--R4) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V1 smd circle (at 9.525 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V3 smd circle (at 9.525 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 163 /Configuration/LCD.D13.R2--R5) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V7 smd circle (at 9.525 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 90 /Flash/MMC1_DAT1) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V9 smd circle (at 9.525 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 97 /Flash/MMC1_CMD) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V8 smd circle (at 9.525 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 94 /Flash/MMC1_DAT5) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V10 smd circle (at 9.525 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 343 "Net-(U1-PadV10)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V12 smd circle (at 9.525 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 116 /E_FAULT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V11 smd circle (at 9.525 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 342 "Net-(U1-PadV11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad V13 smd circle (at 9.525 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 155 /H_DIR) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U20 smd circle (at 8.255 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U19 smd circle (at 8.255 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U18 smd circle (at 8.255 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 154 /E_STEP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U17 smd circle (at 8.255 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /Z1_ENDSTOP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U14 smd circle (at 8.255 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 76 /SERVO_0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U16 smd circle (at 8.255 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 341 /HDMI_INT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U15 smd circle (at 8.255 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 80 /USR1) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U6 smd circle (at 8.255 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 118 /X_FAULT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U5 smd circle (at 8.255 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 "Net-(U1-PadU5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U4 smd circle (at 8.255 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 165 /Configuration/LCD.D11.R0--R3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U2 smd circle (at 8.255 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 167 /Configuration/LCD.D9.G4--G6) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U1 smd circle (at 8.255 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 168 /Configuration/LCD.D8.G3--G5) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U3 smd circle (at 8.255 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 166 /Configuration/LCD.D10.G5--G7) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U7 smd circle (at 8.255 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 89 /Flash/MMC1_DAT0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U9 smd circle (at 8.255 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 98 /Flash/MMC1_CLK) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U8 smd circle (at 8.255 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 93 /Flash/MMC1_DAT4) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U10 smd circle (at 8.255 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 153 /Y_DIR) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U12 smd circle (at 8.255 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 152 /X_STEP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U11 smd circle (at 8.255 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 339 "Net-(U1-PadU11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad U13 smd circle (at 8.255 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 151 /E_DIR) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T20 smd circle (at 6.985 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T19 smd circle (at 6.985 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T18 smd circle (at 6.985 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 101 /USB/USB1_VBUS) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T17 smd circle (at 6.985 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 117 /X2_ENDSTOP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T14 smd circle (at 6.985 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 122 /Y2_ENDSTOP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T16 smd circle (at 6.985 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 100 /~USB1_OC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T15 smd circle (at 6.985 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 79 /USR2) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T6 smd circle (at 6.985 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 123 /Y_FAULT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T5 smd circle (at 6.985 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 161 /Configuration/LCD.D15.R4--R7) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T4 smd circle (at 6.985 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 169 /Configuration/LCD.D7.G2--G4) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T2 smd circle (at 6.985 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 171 /Configuration/LCD.D5.G0--G2) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T1 smd circle (at 6.985 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 172 /Configuration/LCD.D4.B4--B7) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T3 smd circle (at 6.985 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 170 /Configuration/LCD.D6.G1--G3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T7 smd circle (at 6.985 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 121 /H_FAULT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T9 smd circle (at 6.985 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 96 /Flash/MMC1_DAT7) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T8 smd circle (at 6.985 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 92 /Flash/MMC1_DAT3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T10 smd circle (at 6.985 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 150 /Z_STEP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T12 smd circle (at 6.985 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 149 /Y_STEP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T11 smd circle (at 6.985 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 148 /Z_DIR) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad T13 smd circle (at 6.985 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 /~DISP_INT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R20 smd circle (at 5.715 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R19 smd circle (at 5.715 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R18 smd circle (at 5.715 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 59 /USB/USB.HOST.D-) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R17 smd circle (at 5.715 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 58 /USB/USB.HOST.D+) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R14 smd circle (at 5.715 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U1-PadR14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R16 smd circle (at 5.715 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R15 smd circle (at 5.715 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(U1-PadR15)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R6 smd circle (at 5.715 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(U1-PadR6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R5 smd circle (at 5.715 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 336 "Net-(U1-PadR5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R4 smd circle (at 5.715 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 173 /Configuration/LCD.D3.B3--B6) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R2 smd circle (at 5.715 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 175 /Configuration/LCD.D1.B1--B4) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R1 smd circle (at 5.715 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 176 /Configuration/LCD.D0.B0--B3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R3 smd circle (at 5.715 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 174 /Configuration/LCD.D2.B2--B5) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R7 smd circle (at 5.715 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /ENC_B) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R9 smd circle (at 5.715 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R8 smd circle (at 5.715 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 91 /Flash/MMC1_DAT2) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R10 smd circle (at 5.715 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 335 "Net-(U1-PadR10)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R12 smd circle (at 5.715 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 146 /H_STEP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R11 smd circle (at 5.715 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 334 "Net-(U1-PadR11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad R13 smd circle (at 5.715 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 87 /Flash/GPIO1_16.SIP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P20 smd circle (at 4.445 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P19 smd circle (at 4.445 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P18 smd circle (at 4.445 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 333 "Net-(U1-PadP18)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P17 smd circle (at 4.445 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 625 "Net-(R45-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P14 smd circle (at 4.445 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 332 "Net-(U1-PadP14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P16 smd circle (at 4.445 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 55 /USB/USB.CLIENT.ID) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P15 smd circle (at 4.445 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 626 "Net-(R51-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P6 smd circle (at 4.445 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 VDD_3V3A) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P5 smd circle (at 4.445 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 VDD_3V3A) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P4 smd circle (at 4.445 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 331 "Net-(U1-PadP4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P2 smd circle (at 4.445 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 330 "Net-(U1-PadP2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P1 smd circle (at 4.445 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 329 "Net-(U1-PadP1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P3 smd circle (at 4.445 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 328 "Net-(U1-PadP3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P7 smd circle (at 4.445 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 VDD_3V3A) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P9 smd circle (at 4.445 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 327 "Net-(U1-PadP9)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P8 smd circle (at 4.445 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 326 "Net-(U1-PadP8)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P10 smd circle (at 4.445 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 325 "Net-(U1-PadP10)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P12 smd circle (at 4.445 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 324 "Net-(U1-PadP12)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P11 smd circle (at 4.445 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 323 "Net-(U1-PadP11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad P13 smd circle (at 4.445 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 322 "Net-(U1-PadP13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N20 smd circle (at 3.175 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N19 smd circle (at 3.175 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N18 smd circle (at 3.175 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 56 /USB/USB.CLIENT.D-) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N17 smd circle (at 3.175 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 57 /USB/USB.CLIENT.D+) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N14 smd circle (at 3.175 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N16 smd circle (at 3.175 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N15 smd circle (at 3.175 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 321 "Net-(U1-PadN15)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N6 smd circle (at 3.175 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 320 VDD_RTC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N5 smd circle (at 3.175 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 VDD_3V3A) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N4 smd circle (at 3.175 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 319 "Net-(U1-PadN4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N2 smd circle (at 3.175 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 318 "Net-(U1-PadN2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N1 smd circle (at 3.175 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 317 "Net-(U1-PadN1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N3 smd circle (at 3.175 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 316 "Net-(U1-PadN3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N7 smd circle (at 3.175 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N9 smd circle (at 3.175 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 315 "Net-(U1-PadN9)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N8 smd circle (at 3.175 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 314 "Net-(U1-PadN8)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N10 smd circle (at 3.175 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N12 smd circle (at 3.175 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 313 "Net-(U1-PadN12)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N11 smd circle (at 3.175 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad N13 smd circle (at 3.175 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 312 "Net-(U1-PadN13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M20 smd circle (at 1.905 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 646 "Net-(C43-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M19 smd circle (at 1.905 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M18 smd circle (at 1.905 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 145 /Ethernet/MDIO_CLK) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M17 smd circle (at 1.905 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 113 /Ethernet/MDIO_DATA) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M14 smd circle (at 1.905 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M16 smd circle (at 1.905 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 106 /Ethernet/MII1_RXD0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M15 smd circle (at 1.905 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 311 "Net-(U1-PadM15)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M6 smd circle (at 1.905 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M5 smd circle (at 1.905 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 310 "Net-(U1-PadM5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M4 smd circle (at 1.905 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 309 "Net-(U1-PadM4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M2 smd circle (at 1.905 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 308 "Net-(U1-PadM2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M1 smd circle (at 1.905 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 307 "Net-(U1-PadM1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M3 smd circle (at 1.905 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 306 "Net-(U1-PadM3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M7 smd circle (at 1.905 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M9 smd circle (at 1.905 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M8 smd circle (at 1.905 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M10 smd circle (at 1.905 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M12 smd circle (at 1.905 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M11 smd circle (at 1.905 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 305 "Net-(U1-PadM11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad M13 smd circle (at 1.905 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 304 "Net-(U1-PadM13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L20 smd circle (at 0.635 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 658 "Net-(C43-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L19 smd circle (at 0.635 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L18 smd circle (at 0.635 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 108 /Ethernet/MII1_RXCLK) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L17 smd circle (at 0.635 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 103 /Ethernet/MII1_RXD3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L14 smd circle (at 0.635 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 303 "Net-(U1-PadL14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L16 smd circle (at 0.635 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 104 /Ethernet/MII1_RXD2) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L15 smd circle (at 0.635 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 105 /Ethernet/MII1_RXD1) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L6 smd circle (at 0.635 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 302 "Net-(U1-PadL6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L5 smd circle (at 0.635 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 301 "Net-(U1-PadL5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L4 smd circle (at 0.635 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 300 "Net-(U1-PadL4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L2 smd circle (at 0.635 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 299 "Net-(U1-PadL2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L1 smd circle (at 0.635 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 298 "Net-(U1-PadL1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L3 smd circle (at 0.635 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 297 "Net-(U1-PadL3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L7 smd circle (at 0.635 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 296 "Net-(U1-PadL7)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L9 smd circle (at 0.635 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 295 "Net-(U1-PadL9)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L8 smd circle (at 0.635 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 294 "Net-(U1-PadL8)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L10 smd circle (at 0.635 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L12 smd circle (at 0.635 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L11 smd circle (at 0.635 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad L13 smd circle (at 0.635 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K20 smd circle (at -0.635 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 659 "Net-(C44-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K19 smd circle (at -0.635 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K18 smd circle (at -0.635 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 110 /Ethernet/MII1_TXCLK) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K17 smd circle (at -0.635 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 144 /Ethernet/MII1_TXD0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K16 smd circle (at -0.635 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 143 /Ethernet/MII1_TXD1) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K15 smd circle (at -0.635 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 142 /Ethernet/MII1_TXD2) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K14 smd circle (at -0.635 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(U1-PadK14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K13 smd circle (at -0.635 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(U1-PadK13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K12 smd circle (at -0.635 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 291 "Net-(U1-PadK12)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K11 smd circle (at -0.635 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K10 smd circle (at -0.635 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K9 smd circle (at -0.635 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K8 smd circle (at -0.635 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(U1-PadK8)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K7 smd circle (at -0.635 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K6 smd circle (at -0.635 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(U1-PadK6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K1 smd circle (at -0.635 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 288 "Net-(U1-PadK1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K4 smd circle (at -0.635 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 287 "Net-(U1-PadK4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K3 smd circle (at -0.635 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(U1-PadK3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K5 smd circle (at -0.635 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 285 "Net-(U1-PadK5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad K2 smd circle (at -0.635 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(U1-PadK2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J20 smd circle (at -1.905 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J19 smd circle (at -1.905 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J18 smd circle (at -1.905 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 141 /Ethernet/MII1_TXD3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J17 smd circle (at -1.905 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 107 /Ethernet/MII1_RXDV) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J16 smd circle (at -1.905 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 140 /Ethernet/MII1_TXEN) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J15 smd circle (at -1.905 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 109 /Ethernet/MII1_RXERR) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J14 smd circle (at -1.905 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 283 "Net-(U1-PadJ14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J13 smd circle (at -1.905 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(U1-PadJ13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J12 smd circle (at -1.905 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 281 "Net-(U1-PadJ12)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J11 smd circle (at -1.905 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J10 smd circle (at -1.905 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J9 smd circle (at -1.905 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J8 smd circle (at -1.905 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J7 smd circle (at -1.905 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J6 smd circle (at -1.905 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J1 smd circle (at -1.905 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 280 "Net-(U1-PadJ1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J4 smd circle (at -1.905 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 279 "Net-(U1-PadJ4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J3 smd circle (at -1.905 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(U1-PadJ3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J5 smd circle (at -1.905 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 277 "Net-(U1-PadJ5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad J2 smd circle (at -1.905 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 276 "Net-(U1-PadJ2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H20 smd circle (at -3.175 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 555 "Net-(C41-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H19 smd circle (at -3.175 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H18 smd circle (at -3.175 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 102 /Ethernet/MII1_REFCLK) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H17 smd circle (at -3.175 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 112 /Ethernet/MII1_CRS_DV) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H16 smd circle (at -3.175 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 111 /Ethernet/MII1_COL) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H15 smd circle (at -3.175 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 275 "Net-(U1-PadH15)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H14 smd circle (at -3.175 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 274 "Net-(U1-PadH14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H13 smd circle (at -3.175 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(U1-PadH13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H12 smd circle (at -3.175 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H11 smd circle (at -3.175 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(U1-PadH11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H10 smd circle (at -3.175 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H9 smd circle (at -3.175 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H8 smd circle (at -3.175 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H7 smd circle (at -3.175 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H6 smd circle (at -3.175 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H1 smd circle (at -3.175 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(U1-PadH1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H4 smd circle (at -3.175 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 270 "Net-(U1-PadH4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H3 smd circle (at -3.175 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 269 "Net-(U1-PadH3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H5 smd circle (at -3.175 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 268 VDD_DDR) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad H2 smd circle (at -3.175 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(U1-PadH2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G20 smd circle (at -4.445 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 657 "Net-(C41-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G19 smd circle (at -4.445 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G18 smd circle (at -4.445 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 61 /MMC0_CMD) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G17 smd circle (at -4.445 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 /MMC0_CLK) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G16 smd circle (at -4.445 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 62 /MMC0_DAT0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G15 smd circle (at -4.445 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 /MMC0_DAT1) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G14 smd circle (at -4.445 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(U1-PadG14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G13 smd circle (at -4.445 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(U1-PadG13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G12 smd circle (at -4.445 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G11 smd circle (at -4.445 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G10 smd circle (at -4.445 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(U1-PadG10)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G9 smd circle (at -4.445 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G8 smd circle (at -4.445 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G7 smd circle (at -4.445 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(U1-PadG7)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G6 smd circle (at -4.445 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 262 "Net-(U1-PadG6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G1 smd circle (at -4.445 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(U1-PadG1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G4 smd circle (at -4.445 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(U1-PadG4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G3 smd circle (at -4.445 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(U1-PadG3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G5 smd circle (at -4.445 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 258 "Net-(U1-PadG5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad G2 smd circle (at -4.445 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(U1-PadG2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F20 smd circle (at -5.715 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 578 "Net-(C42-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F19 smd circle (at -5.715 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F18 smd circle (at -5.715 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 65 /MMC0_DAT2) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F17 smd circle (at -5.715 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 /MMC0_DAT3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F16 smd circle (at -5.715 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(U1-PadF16)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F15 smd circle (at -5.715 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 99 /USB/USB1_DRVVBUS) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F14 smd circle (at -5.715 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(U1-PadF14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F13 smd circle (at -5.715 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(U1-PadF13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F12 smd circle (at -5.715 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(U1-PadF12)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F11 smd circle (at -5.715 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(U1-PadF11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F10 smd circle (at -5.715 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 251 VDD_MPU) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F9 smd circle (at -5.715 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(U1-PadF9)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F8 smd circle (at -5.715 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F7 smd circle (at -5.715 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(U1-PadF7)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F6 smd circle (at -5.715 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 248 VDD_CORE) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F1 smd circle (at -5.715 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(U1-PadF1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F4 smd circle (at -5.715 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(U1-PadF4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F3 smd circle (at -5.715 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(U1-PadF3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F5 smd circle (at -5.715 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(U1-PadF5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad F2 smd circle (at -5.715 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(U1-PadF2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E20 smd circle (at -6.985 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E19 smd circle (at -6.985 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E18 smd circle (at -6.985 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(U1-PadE18)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E17 smd circle (at -6.985 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 128 /USB/~UART0_RST) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E16 smd circle (at -6.985 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 139 /USB/UART0_TXD_OUT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E15 smd circle (at -6.985 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 138 /USB/UART0_RXD_IN) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E14 smd circle (at -6.985 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(U1-PadE14)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E13 smd circle (at -6.985 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(U1-PadE13)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E12 smd circle (at -6.985 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(U1-PadE12)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E11 smd circle (at -6.985 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(U1-PadE11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E10 smd circle (at -6.985 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(U1-PadE10)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E9 smd circle (at -6.985 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E8 smd circle (at -6.985 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 129 GNDA) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E7 smd circle (at -6.985 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 236 VDD_PLL) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E6 smd circle (at -6.985 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(U1-PadE6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E1 smd circle (at -6.985 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(U1-PadE1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E4 smd circle (at -6.985 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(U1-PadE4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E3 smd circle (at -6.985 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(U1-PadE3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E5 smd circle (at -6.985 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(U1-PadE5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad E2 smd circle (at -6.985 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(U1-PadE2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D20 smd circle (at -8.255 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 124 /Power/PWR_BUT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D19 smd circle (at -8.255 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U1-PadC6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D18 smd circle (at -8.255 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 137 /I2C2_SDA) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D17 smd circle (at -8.255 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 709 "Net-(FB48-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D16 smd circle (at -8.255 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 115 /~SR_EN) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D15 smd circle (at -8.255 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 120 /Z_FAULT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D14 smd circle (at -8.255 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 545 "Net-(FB44-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D13 smd circle (at -8.255 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R29-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D12 smd circle (at -8.255 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 654 "Net-(FB45-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D11 smd circle (at -8.255 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(U1-PadD11)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D10 smd circle (at -8.255 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D9 smd circle (at -8.255 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(U1-PadD9)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D8 smd circle (at -8.255 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 114 VDD_ADC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D7 smd circle (at -8.255 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(U1-PadD7)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D6 smd circle (at -8.255 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(U1-PadD6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D1 smd circle (at -8.255 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(U1-PadD1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D4 smd circle (at -8.255 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(U1-PadD4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D3 smd circle (at -8.255 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(U1-PadD3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D5 smd circle (at -8.255 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(U1-PadD5)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad D2 smd circle (at -8.255 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(U1-PadD2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C20 smd circle (at -9.525 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 708 /SIP_I2C0_SCL) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C19 smd circle (at -9.525 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 /I2C0_SDA) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C18 smd circle (at -9.525 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R28-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C17 smd circle (at -9.525 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 /I2C0_SDA) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C16 smd circle (at -9.525 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 708 /SIP_I2C0_SCL) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C15 smd circle (at -9.525 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 66 /SD.CD) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C14 smd circle (at -9.525 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 74 /JTAG/JTAG_EMU0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C13 smd circle (at -9.525 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 119 /Z2_ENDSTOP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C12 smd circle (at -9.525 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 135 /SPI1_CS0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C11 smd circle (at -9.525 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 69 /JTAG/JTAG_TMS) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C10 smd circle (at -9.525 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(U1-PadC10)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C9 smd circle (at -9.525 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R26-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C8 smd circle (at -9.525 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /ADC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C7 smd circle (at -9.525 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 219 /Microprocessor/AIN1) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C6 smd circle (at -9.525 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U1-PadC6)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C1 smd circle (at -9.525 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(U1-PadC1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C4 smd circle (at -9.525 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(U1-PadC4)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C3 smd circle (at -9.525 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(U1-PadC3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C5 smd circle (at -9.525 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 130 /Power/PMIC_NWAKEUP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad C2 smd circle (at -9.525 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(U1-PadC2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B20 smd circle (at -10.795 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 132 /Power/LDO_PGOOD) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B19 smd circle (at -10.795 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 133 /Power/PMIC_INT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B18 smd circle (at -10.795 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 133 /Power/PMIC_INT) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B17 smd circle (at -10.795 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 /SPI0_MISO) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B16 smd circle (at -10.795 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 544 "Net-(FB43-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B15 smd circle (at -10.795 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 131 /Power/PMIC_PGOOD) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B14 smd circle (at -10.795 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 75 /JTAG/JTAG_EMU1) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B13 smd circle (at -10.795 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI1_MISO) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B12 smd circle (at -10.795 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R30-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B11 smd circle (at -10.795 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 /JTAG/JTAG_TDI) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B10 smd circle (at -10.795 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 70 /JTAG/~JTAG_TRST) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B9 smd circle (at -10.795 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 114 VDD_ADC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B8 smd circle (at -10.795 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 214 /Microprocessor/AIN5) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B7 smd circle (at -10.795 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 213 /Microprocessor/AIN2) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B6 smd circle (at -10.795 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 212 /Microprocessor/AIN0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B1 smd circle (at -10.795 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(U1-PadB1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B4 smd circle (at -10.795 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R15-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B3 smd circle (at -10.795 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(U1-PadB3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B5 smd circle (at -10.795 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 132 /Power/LDO_PGOOD) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad B2 smd circle (at -10.795 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(U1-PadB2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A20 smd circle (at -12.065 -12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 131 /Power/PMIC_PGOOD) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A19 smd circle (at -12.065 -10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 130 /Power/PMIC_NWAKEUP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A18 smd circle (at -12.065 -9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A17 smd circle (at -12.065 -8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 653 "Net-(FB42-Pad2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A16 smd circle (at -12.065 -6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 /SPI0_CS0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A15 smd circle (at -12.065 -5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 652 "Net-(FB41-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A14 smd circle (at -12.065 -4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /X1_ENDSTOP) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A13 smd circle (at -12.065 -3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 557 "Net-(FB46-Pad1)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A12 smd circle (at -12.065 -1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 73 /TCK) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A11 smd circle (at -12.065 -0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 72 /JTAG/JTAG_TD0) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A10 smd circle (at -12.065 0.635 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A9 smd circle (at -12.065 1.905 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 129 GNDA) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A8 smd circle (at -12.065 3.175 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /BED_THERM) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A7 smd circle (at -12.065 4.445 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 208 /Microprocessor/AIN3) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A6 smd circle (at -12.065 5.715 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 129 GNDA) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A5 smd circle (at -12.065 6.985 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 114 VDD_ADC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A4 smd circle (at -12.065 8.255 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 114 VDD_ADC) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A3 smd circle (at -12.065 9.525 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(U1-PadA3)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A2 smd circle (at -12.065 10.795 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(U1-PadA2)") (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (pad A1 smd circle (at -12.065 12.065 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1) (clearance 0.15) (thermal_width 0.25401) (thermal_gap 0.2535))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 5.4 5.4 3.11))
      (rotate (xyz 0 0 270))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 96.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U19 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 203 "/Stepper Drivers/Y_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 700 "Net-(C164-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 201 "/Stepper Drivers/Y_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 501 "Net-(U19-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 500 "Net-(U19-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 123 /Y_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 122 /Y2_ENDSTOP))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 448 "/Stepper Drivers/~Y_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 720 "Net-(R154-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 199 "/Stepper Drivers/Y Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 696 "Net-(C153-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 697 "Net-(C156-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 698 "Net-(C156-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 699 "Net-(C159-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 200 "/Stepper Drivers/Y_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 701 "Net-(C167-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 202 "/Stepper Drivers/Y_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI1_MOSI))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 511 "/Stepper Drivers/Y_MISO"))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 149 /Y_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 153 /Y_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 499 "Net-(U19-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 498 "Net-(U19-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 114.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U14 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 186 "/Stepper Drivers/X0_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 670 "Net-(C84-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 184 "/Stepper Drivers/X0_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U14-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U14-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 118 /X_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 117 /X2_ENDSTOP))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 187 "/Stepper Drivers/~X0_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 715 "Net-(R124-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 182 "/Stepper Drivers/X0 Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 666 "Net-(C73-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 667 "Net-(C76-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 668 "Net-(C76-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 669 "Net-(C79-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 183 "/Stepper Drivers/X0_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 671 "Net-(C87-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 185 "/Stepper Drivers/X0_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 511 "/Stepper Drivers/Y_MISO"))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 512 "/Stepper Drivers/X0_MISO"))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 152 /X_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 156 /X_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U14-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U14-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 132.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U20 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 192 "/Stepper Drivers/X1_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 706 "Net-(C180-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 190 "/Stepper Drivers/X1_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 458 "Net-(U20-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 459 "Net-(U20-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 118 /X_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 117 /X2_ENDSTOP))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 193 "/Stepper Drivers/~X1_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 721 "Net-(R159-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 188 "/Stepper Drivers/X1 Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 702 "Net-(C169-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 704 "Net-(C172-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 703 "Net-(C172-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 705 "Net-(C175-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 189 "/Stepper Drivers/X1_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 707 "Net-(C183-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 191 "/Stepper Drivers/X1_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 512 "/Stepper Drivers/X0_MISO"))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 513 "/Stepper Drivers/X1_MISO"))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 152 /X_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 156 /X_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 460 "Net-(U20-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 461 "Net-(U20-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 150.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U15 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 198 "/Stepper Drivers/Z0_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 676 "Net-(C100-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 196 "/Stepper Drivers/Z0_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 453 "Net-(U15-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 452 "Net-(U15-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 120 /Z_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 119 /Z2_ENDSTOP))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 449 "/Stepper Drivers/~Z0_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 716 "Net-(R131-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 194 "/Stepper Drivers/Z0 Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 672 "Net-(C89-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 674 "Net-(C92-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 673 "Net-(C92-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 675 "Net-(C95-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 195 "/Stepper Drivers/Z0_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 677 "Net-(C103-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 197 "/Stepper Drivers/Z0_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 513 "/Stepper Drivers/X1_MISO"))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 514 "/Stepper Drivers/Z0_MISO"))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 150 /Z_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 148 /Z_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 451 "Net-(U15-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 450 "Net-(U15-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 168.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U16 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 466 "/Stepper Drivers/Z1_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 682 "Net-(C116-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 464 "/Stepper Drivers/Z1_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 454 "Net-(U16-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 455 "Net-(U16-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 120 /Z_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 119 /Z2_ENDSTOP))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 487 "/Stepper Drivers/~Z1_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 717 "Net-(R136-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 462 "/Stepper Drivers/Z1 Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 678 "Net-(C105-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 679 "Net-(C108-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 680 "Net-(C108-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 681 "Net-(C111-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 463 "/Stepper Drivers/Z1_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 683 "Net-(C119-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 465 "/Stepper Drivers/Z1_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 514 "/Stepper Drivers/Z0_MISO"))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 515 "/Stepper Drivers/Z1_MISO"))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 150 /Z_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 148 /Z_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 456 "Net-(U16-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 457 "Net-(U16-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 186.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U17 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 471 "/Stepper Drivers/Z2_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 688 "Net-(C132-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 469 "/Stepper Drivers/Z2_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 493 "Net-(U17-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 492 "Net-(U17-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 120 /Z_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 119 /Z2_ENDSTOP))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 488 "/Stepper Drivers/~Z2_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 718 "Net-(R141-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 467 "/Stepper Drivers/Z2 Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 684 "Net-(C121-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 686 "Net-(C124-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 685 "Net-(C124-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 687 "Net-(C127-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 468 "/Stepper Drivers/Z2_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 689 "Net-(C135-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 470 "/Stepper Drivers/Z2_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 515 "/Stepper Drivers/Z1_MISO"))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 509 "/Stepper Drivers/Z2_MISO"))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 150 /Z_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 148 /Z_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 491 "Net-(U17-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 490 "Net-(U17-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 204.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U13 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 21 "/Stepper Drivers/E_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 664 "Net-(C68-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 19 "/Stepper Drivers/E_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 516 "Net-(U13-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 517 "Net-(U13-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 116 /E_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 159 "/Stepper Drivers/~E_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 641 "Net-(R117-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 17 "/Stepper Drivers/E Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 660 "Net-(C57-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 662 "Net-(C60-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 661 "Net-(C60-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 663 "Net-(C63-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 18 "/Stepper Drivers/E_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 665 "Net-(C71-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 20 "/Stepper Drivers/E_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 509 "/Stepper Drivers/Z2_MISO"))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 510 "/Stepper Drivers/E_MISO"))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 154 /E_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 151 /E_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 518 "Net-(U13-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 519 "Net-(U13-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:QFN36_5X6 (layer F.Cu) (tedit 5911DF04)
    (at 222.09 142.05 270)
    (solder_mask_margin 0.1)
    (fp_text reference U18 (at 0 0 270) (layer F.SilkS))
    (fp_text value TMC2130 (at 0 -0.75 270) (layer F.SilkS))
    (pad 11 smd rect (at -1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 12 smd rect (at -1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 13 smd rect (at -0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 476 "/Stepper Drivers/H_B1"))
    (pad 14 smd rect (at -0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 694 "Net-(C148-Pad1)"))
    (pad 15 smd rect (at 0.24892 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 474 "/Stepper Drivers/H_B2"))
    (pad 16 smd rect (at 0.7493 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 17 smd rect (at 1.24968 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 494 "Net-(U18-Pad17)"))
    (pad 18 smd rect (at 1.74752 3.19786 90) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 19 smd rect (at 2.69748 2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 495 "Net-(U18-Pad19)"))
    (pad 20 smd rect (at 2.69748 1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 121 /H_FAULT))
    (pad 21 smd rect (at 2.69748 1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 22 smd rect (at 2.69748 0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 489 "/Stepper Drivers/~H_EN"))
    (pad 23 smd rect (at 2.69748 0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 719 "Net-(R147-Pad2)"))
    (pad 24 smd rect (at 2.69748 -0.24892 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 25 smd rect (at 2.69748 -0.7493 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 472 "/Stepper Drivers/H Stepper Driver/5VOUT"))
    (pad 26 smd rect (at 2.69748 -1.24968 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 690 "Net-(C137-Pad1)"))
    (pad 27 smd rect (at 2.69748 -1.74752 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 691 "Net-(C140-Pad2)"))
    (pad 28 smd rect (at 2.69748 -2.2479 180) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 692 "Net-(C140-Pad1)"))
    (pad 29 smd rect (at 1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 693 "Net-(C143-Pad2)"))
    (pad 30 smd rect (at 1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 31 smd rect (at 0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (pad 32 smd rect (at 0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 473 "/Stepper Drivers/H_A2"))
    (pad 33 smd rect (at -0.24892 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 695 "Net-(C151-Pad1)"))
    (pad 34 smd rect (at -0.7493 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 475 "/Stepper Drivers/H_A1"))
    (pad 35 smd rect (at -1.24968 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 36 smd rect (at -1.74752 -3.19786 270) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.69748 -2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.69748 -1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 3 smd rect (at -2.69748 -1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 4 smd rect (at -2.69748 -0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 510 "/Stepper Drivers/E_MISO"))
    (pad 5 smd rect (at -2.69748 -0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI1_MISO))
    (pad 6 smd rect (at -2.69748 0.24892) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 146 /H_STEP))
    (pad 7 smd rect (at -2.69748 0.7493) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 155 /H_DIR))
    (pad 8 smd rect (at -2.69748 1.24968) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -2.69748 1.74752) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 496 "Net-(U18-Pad9)"))
    (pad 10 smd rect (at -2.69748 2.2479) (size 0.24892 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 497 "Net-(U18-Pad10)"))
    (pad 37 smd rect (at 0 0 270) (size 3.6 4.6) (layers *.Mask F.Cu F.Paste)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 -1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 -0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 0 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0.65 0.85 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at -1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 0 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (pad 37 thru_hole circle (at 1.3 1.7 270) (size 0.4 0.4) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 CGND))
    (model Housings_DFN_QFN.3dshapes/QFN-36-1EP_5x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:EMMCxxG-S100 locked (layer F.Cu) (tedit 5931879C)
    (at 157.765 109.595 180)
    (tags "153-Pin BGA")
    (attr smd)
    (fp_text reference U5 (at 10.965 2.695 360) (layer F.SilkS))
    (fp_text value EMMC**G-S100 (at 3.25 -10 180) (layer F.Fab))
    (pad A1 smd circle (at 0 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 92 /Flash/MMC1_DAT3) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B1 smd circle (at 0.5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 351 "Net-(U5-PadB1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C1 smd circle (at 1 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 650 "Net-(C18-Pad1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad D1 smd circle (at 1.5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 94 /Flash/MMC1_DAT5) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E1 smd circle (at 2 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015) (thermal_gap 0.0001))
    (pad F1 smd circle (at 2.5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 352 "Net-(U5-PadF1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G1 smd circle (at 3 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H1 smd circle (at 3.5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 353 "Net-(U5-PadH1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J1 smd circle (at 4 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 354 "Net-(U5-PadJ1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K1 smd circle (at 4.5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 355 "Net-(U5-PadK1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad L1 smd circle (at 5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 356 "Net-(U5-PadL1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M1 smd circle (at 5.5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 357 "Net-(U5-PadM1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N1 smd circle (at 6 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 358 "Net-(U5-PadN1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P1 smd circle (at 6.5 0) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 359 "Net-(U5-PadP1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A2 smd circle (at 0 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 93 /Flash/MMC1_DAT4) (solder_mask_margin 0.1015) (clearance 0.0015))
    (pad B2 smd circle (at 0.5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 92 /Flash/MMC1_DAT3) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C2 smd circle (at 1 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 650 "Net-(C18-Pad1)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad D2 smd circle (at 1.5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 94 /Flash/MMC1_DAT5) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E2 smd circle (at 2 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad F2 smd circle (at 2.5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G2 smd circle (at 3 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 360 "Net-(U5-PadG2)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H2 smd circle (at 3.5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 361 "Net-(U5-PadH2)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J2 smd circle (at 4 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 362 "Net-(U5-PadJ2)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K2 smd circle (at 4.5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 363 "Net-(U5-PadK2)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad L2 smd circle (at 5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 364 "Net-(U5-PadL2)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M2 smd circle (at 5.5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 365 "Net-(U5-PadM2)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N2 smd circle (at 6 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P2 smd circle (at 6.5 -0.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015) (thermal_gap 0.254))
    (pad A3 smd circle (at 0 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 89 /Flash/MMC1_DAT0) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B3 smd circle (at 0.5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 93 /Flash/MMC1_DAT4) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C3 smd circle (at 1 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 94 /Flash/MMC1_DAT5) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad D3 smd circle (at 1.5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E3 smd circle (at 2 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad F3 smd circle (at 2.5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 366 "Net-(U5-PadF3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G3 smd circle (at 3 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(U5-PadG3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H3 smd circle (at 3.5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 368 "Net-(U5-PadH3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J3 smd circle (at 4 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(U5-PadJ3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K3 smd circle (at 4.5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 370 "Net-(U5-PadK3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad L3 smd circle (at 5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(U5-PadL3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M3 smd circle (at 5.5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 372 "Net-(U5-PadM3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N3 smd circle (at 6 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 373 "Net-(U5-PadN3)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P3 smd circle (at 6.5 -1) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A4 smd circle (at 0 -1.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 90 /Flash/MMC1_DAT1) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B4 smd circle (at 0.5 -1.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 94 /Flash/MMC1_DAT5) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C4 smd circle (at 1 -1.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad D4 smd circle (at 1.5 -1.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M4 smd circle (at 5.5 -1.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N4 smd circle (at 6 -1.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P4 smd circle (at 6.5 -1.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015) (thermal_gap 0.254))
    (pad A5 smd circle (at 0 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 91 /Flash/MMC1_DAT2) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B5 smd circle (at 0.5 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C5 smd circle (at 1 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 95 /Flash/MMC1_DAT6) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E5 smd circle (at 2 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 374 "Net-(U5-PadE5)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad F5 smd circle (at 2.5 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G5 smd circle (at 3 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H5 smd circle (at 3.5 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 375 "Net-(U5-PadH5)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J5 smd circle (at 4 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(U5-PadJ5)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K5 smd circle (at 4.5 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 88 /Flash/EMMC_RSTN) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M5 smd circle (at 5.5 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 97 /Flash/MMC1_CMD) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N5 smd circle (at 6 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P5 smd circle (at 6.5 -2) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.05))
    (pad A6 smd circle (at 0 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 377 "Net-(U5-PadA6)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B6 smd circle (at 0.5 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 96 /Flash/MMC1_DAT7) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C6 smd circle (at 1 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E6 smd circle (at 2 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K6 smd circle (at 4.5 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 378 "Net-(U5-PadK6)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M6 smd circle (at 5.5 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 98 /Flash/MMC1_CLK) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N6 smd circle (at 6 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 97 /Flash/MMC1_CMD) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P6 smd circle (at 6.5 -2.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015) (thermal_gap 0.254))
    (pad A7 smd circle (at 0 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 379 "Net-(U5-PadA7)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B7 smd circle (at 0.5 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 96 /Flash/MMC1_DAT7) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C7 smd circle (at 1 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E7 smd circle (at 2 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K7 smd circle (at 4.5 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 380 "Net-(U5-PadK7)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M7 smd circle (at 5.5 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 98 /Flash/MMC1_CLK) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N7 smd circle (at 6 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 97 /Flash/MMC1_CMD) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P7 smd circle (at 6.5 -3) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 381 "Net-(U5-PadP7)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A8 smd circle (at 0 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 96 /Flash/MMC1_DAT7) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B8 smd circle (at 0.5 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C8 smd circle (at 1 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 382 "Net-(U5-PadC8)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E8 smd circle (at 2 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 383 "Net-(U5-PadE8)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K8 smd circle (at 4.5 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M8 smd circle (at 5.5 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 384 "Net-(U5-PadM8)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N8 smd circle (at 6 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 98 /Flash/MMC1_CLK) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P8 smd circle (at 6.5 -3.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 97 /Flash/MMC1_CMD) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A9 smd circle (at 0 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B9 smd circle (at 0.5 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 385 "Net-(U5-PadB9)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C9 smd circle (at 1 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 386 "Net-(U5-PadC9)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E9 smd circle (at 2 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 387 "Net-(U5-PadE9)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K9 smd circle (at 4.5 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M9 smd circle (at 5.5 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 388 "Net-(U5-PadM9)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N9 smd circle (at 6 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 389 "Net-(U5-PadN9)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P9 smd circle (at 6.5 -4) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 98 /Flash/MMC1_CLK) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A10 smd circle (at 0 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 390 "Net-(U5-PadA10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B10 smd circle (at 0.5 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 391 "Net-(U5-PadB10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C10 smd circle (at 1 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 392 "Net-(U5-PadC10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E10 smd circle (at 2 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 393 "Net-(U5-PadE10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad F10 smd circle (at 2.5 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 394 "Net-(U5-PadF10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G10 smd circle (at 3 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 395 "Net-(U5-PadG10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H10 smd circle (at 3.5 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J10 smd circle (at 4 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K10 smd circle (at 4.5 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 396 "Net-(U5-PadK10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M10 smd circle (at 5.5 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 397 "Net-(U5-PadM10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N10 smd circle (at 6 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 398 "Net-(U5-PadN10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P10 smd circle (at 6.5 -4.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 399 "Net-(U5-PadP10)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A11 smd circle (at 0 -5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 400 "Net-(U5-PadA11)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B11 smd circle (at 0.5 -5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 401 "Net-(U5-PadB11)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C11 smd circle (at 1 -5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 402 "Net-(U5-PadC11)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M11 smd circle (at 5.5 -5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 403 "Net-(U5-PadM11)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N11 smd circle (at 6 -5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 404 "Net-(U5-PadN11)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P11 smd circle (at 6.5 -5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 405 "Net-(U5-PadP11)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A12 smd circle (at 0 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 406 "Net-(U5-PadA12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B12 smd circle (at 0.5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 407 "Net-(U5-PadB12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C12 smd circle (at 1 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 408 "Net-(U5-PadC12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad D12 smd circle (at 1.5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 409 "Net-(U5-PadD12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E12 smd circle (at 2 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 410 "Net-(U5-PadE12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad F12 smd circle (at 2.5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 411 "Net-(U5-PadF12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G12 smd circle (at 3 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 412 "Net-(U5-PadG12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H12 smd circle (at 3.5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 413 "Net-(U5-PadH12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J12 smd circle (at 4 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 414 "Net-(U5-PadJ12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K12 smd circle (at 4.5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 415 "Net-(U5-PadK12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad L12 smd circle (at 5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 416 "Net-(U5-PadL12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M12 smd circle (at 5.5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 417 "Net-(U5-PadM12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N12 smd circle (at 6 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 418 "Net-(U5-PadN12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P12 smd circle (at 6.5 -5.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 419 "Net-(U5-PadP12)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A13 smd circle (at 0 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 420 "Net-(U5-PadA13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B13 smd circle (at 0.5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 421 "Net-(U5-PadB13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C13 smd circle (at 1 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(U5-PadC13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad D13 smd circle (at 1.5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 423 "Net-(U5-PadD13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E13 smd circle (at 2 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 424 "Net-(U5-PadE13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad F13 smd circle (at 2.5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 425 "Net-(U5-PadF13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G13 smd circle (at 3 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 426 "Net-(U5-PadG13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H13 smd circle (at 3.5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 427 "Net-(U5-PadH13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J13 smd circle (at 4 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 428 "Net-(U5-PadJ13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K13 smd circle (at 4.5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 429 "Net-(U5-PadK13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad L13 smd circle (at 5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 430 "Net-(U5-PadL13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M13 smd circle (at 5.5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 431 "Net-(U5-PadM13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N13 smd circle (at 6 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 432 "Net-(U5-PadN13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P13 smd circle (at 6.5 -6) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 433 "Net-(U5-PadP13)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad A14 smd circle (at 0 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 434 "Net-(U5-PadA14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad B14 smd circle (at 0.5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 435 "Net-(U5-PadB14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad C14 smd circle (at 1 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 436 "Net-(U5-PadC14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad D14 smd circle (at 1.5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 437 "Net-(U5-PadD14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad E14 smd circle (at 2 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 438 "Net-(U5-PadE14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad F14 smd circle (at 2.5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 439 "Net-(U5-PadF14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad G14 smd circle (at 3 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 440 "Net-(U5-PadG14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad H14 smd circle (at 3.5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 441 "Net-(U5-PadH14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad J14 smd circle (at 4 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 442 "Net-(U5-PadJ14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad K14 smd circle (at 4.5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 443 "Net-(U5-PadK14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad L14 smd circle (at 5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 444 "Net-(U5-PadL14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad M14 smd circle (at 5.5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 445 "Net-(U5-PadM14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad N14 smd circle (at 6 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 446 "Net-(U5-PadN14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (pad P14 smd circle (at 6.5 -6.5) (size 0.244 0.244) (layers F.Cu F.Paste F.Mask)
      (net 447 "Net-(U5-PadP14)") (solder_mask_margin 0.1015) (clearance 0.1015))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.127953 0.127953 0))
      (scale (xyz 2.3 2.6 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module KiMBo:Crystal_SMD_32.768kHz_2Pads (layer F.Cu) (tedit 59396355)
    (at 167.669 88.055 270)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 2 Pads")
    (tags "crystal oscillator quartz SMD SMT 5032")
    (attr smd)
    (fp_text reference Y2 (at 0 -2.25 360) (layer F.SilkS))
    (fp_text value AH-32.768KDZY-T (at 0 2.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 578 "Net-(C42-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 555 "Net-(C41-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_5032_4Pads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.55 0.55 0.55))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Crystal_SMD_7A_2Pads (layer F.Cu) (tedit 5939635C)
    (at 167.669 93.135 270)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 2 Pads")
    (tags "crystal oscillator quartz SMD SMT 5032")
    (attr smd)
    (fp_text reference Y3 (at 0 -3 360) (layer F.SilkS))
    (fp_text value 7A-24.000MAAJ-T (at 0 2.9 270) (layer F.Fab))
    (pad 2 smd rect (at 1.85 0 270) (size 1.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 646 "Net-(C43-Pad1)"))
    (pad 1 smd rect (at -1.85 0 270) (size 1.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 659 "Net-(C44-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_5032_2Pads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.34 0.34 0.34))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Crystal_SMD_7A_2Pads (layer F.Cu) (tedit 5924ADEC)
    (at 214.3 95.15 90)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 2 Pads")
    (tags "crystal oscillator quartz SMD SMT 5032")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.8 180) (layer F.SilkS))
    (fp_text value 7A-25.000MAAJ-T (at 0 2.9 90) (layer F.Fab))
    (pad 2 smd rect (at 1.85 0 90) (size 1.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 656 "Net-(C28-Pad1)"))
    (pad 1 smd rect (at -1.85 0 90) (size 1.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 651 "Net-(C27-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_5032_2Pads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.34 0.34 0.34))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 189.9 39.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C45 (at 0.4 1.55) (layer F.SilkS))
    (fp_text value 4.7μF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 /BED_THERM))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 172 83.225 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at -3 0 180) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R28-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 172 81.455 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at -3 0 180) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R30-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 190.45 35.95 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R91 (at 0 -2.35 180) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 VDD_ADC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /Thermistors/BED_THERM_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 192.45 38.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R92 (at 0 -2.15 360) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 616 "Net-(FB51-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /BED_THERM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 593EC847)
    (at 172 79.685)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R103 (at 3.5 0) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 508 /SPI1_CS1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 221.79 38.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C47 (at 0.25 2.19 360) (layer F.SilkS))
    (fp_text value 39nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 /X1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 222.54 36.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R95 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /X1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 618 "Net-(FB53-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 223.59 38.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R96 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /X1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 372.973333 76.815)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 348.662857 78.165)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 2.2μF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 385.869524 96.115)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 383.329524 101.965)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 USB_DC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 378.319524 101.965)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 350.703333 44.725)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 30pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 651 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 344.593333 50.575)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 30pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 656 "Net-(C28-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 332.219524 50.575)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 351.869524 38.875)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 335.539524 62.275)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 342.459524 38.875)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 622 /Ethernet/PHY_VDDCR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FE9765)
    (at 324.404762 44.925)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C33 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10μF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 316.875001 62.675)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1μF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 622 /Ethernet/PHY_VDDCR))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 309.77619 45.125)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-15pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /Ethernet/RD+))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 323.31619 38.875)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C36 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-15pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /Ethernet/RD-))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 309.77619 50.975)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C37 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-15pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 /Ethernet/TD+))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 318.12619 45.125)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C38 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-15pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 /Ethernet/TD-))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 414.034762 73.165)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C39 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10μF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 418.284762 67.315)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C40 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10μF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 344.159524 102.365)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C49 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /Z1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 339.149524 102.365)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C50 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 722 /ENC_A))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 334.419524 108.215)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C51 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /ENC_B))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 434.519524 38.875)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C53 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 429.789524 44.725)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C55 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 414.989524 92.015)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C58 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +24V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 400.258571 38.875)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C193 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 161 /Configuration/LCD.D15.R4--R7))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 375.208571 44.725)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C194 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 162 /Configuration/LCD.D14.R3--R6))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 368.618571 50.575)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C195 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 163 /Configuration/LCD.D13.R2--R5))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 385.608571 38.875)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C196 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 164 /Configuration/LCD.D12.R1--R4))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 368.618571 56.425)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C197 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 165 /Configuration/LCD.D11.R0--R3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 383.708571 44.725)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C198 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 166 /Configuration/LCD.D10.G5--G7))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 372.868571 56.425)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C199 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 167 /Configuration/LCD.D9.G4--G6))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 377.118571 50.575)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C200 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 168 /Configuration/LCD.D8.G3--G5))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 372.868571 50.575)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 169 /Configuration/LCD.D7.G2--G4))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 379.458571 44.725)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 170 /Configuration/LCD.D6.G1--G3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 363.418571 46.675)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 171 /Configuration/LCD.D5.G0--G2))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 382.318571 56.425)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 172 /Configuration/LCD.D4.B4--B7))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 386.568571 50.575)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 173 /Configuration/LCD.D3.B3--B6))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 376.158571 38.875)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 174 /Configuration/LCD.D2.B2--B5))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 370.958571 44.725)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C207 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 175 /Configuration/LCD.D1.B1--B4))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FE9765)
    (at 363.418571 58.375)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 176 /Configuration/LCD.D0.B0--B3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:TPD_PX1SON (layer F.Cu) (tedit 58F78B3D)
    (at 364.886667 71.165)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at 0 1.5) (layer F.SilkS))
    (fp_text value TPD1E04U04DPYR (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.5 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
  )
  (module KiMBo:SOD-923 (layer F.Cu) (tedit 58F783D3)
    (at 376.688095 71.165)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D2 (at 0 -1.5) (layer F.SilkS))
    (fp_text value D5V0F1U2S9 (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 390.795001 76.215)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.5) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 723 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 380.105001 82.865)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.5) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 724 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 384.325001 77.015)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 -1.5) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 725 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 390.795001 71.165)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.5) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 726 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module KiMBo:SOD-923 (layer F.Cu) (tedit 58F783D3)
    (at 362.958095 81.465)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D7 (at 0 -1.5) (layer F.SilkS))
    (fp_text value D5V0F1U2S9 (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 579 "Net-(D7-Pad1)"))
  )
  (module KiMBo:SOD-923 (layer F.Cu) (tedit 58F783D3)
    (at 362.958095 76.215)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D8 (at 0 -1.5) (layer F.SilkS))
    (fp_text value D5V0F1U2S9 (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57FE9788)
    (at 349.966667 71.915)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D9 (at 0 -2.25) (layer F.SilkS))
    (fp_text value TLVH431 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 727 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 728 "Net-(D9-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:TPD_PX1SON (layer F.Cu) (tedit 58F78B3D)
    (at 312.466667 71.165)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D10 (at 0 1.5) (layer F.SilkS))
    (fp_text value TPD1E04U04DPYR (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.5 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE977B)
    (at 317.222381 83.615)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D11 (at 0 -1.5) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 VDD_3V3AUX))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 729 "Net-(D11-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57FE9788)
    (at 324.839524 71.915)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D12 (at 0 -2.25) (layer F.SilkS))
    (fp_text value DNP-TLVH431 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 730 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 731 "Net-(D12-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57FE9783)
    (at 312.561905 109.315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference FB41 (at 0 -1.8) (layer F.SilkS))
    (fp_text value BLM15AG102SN1D (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 652 "Net-(FB41-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /XDMA_EVENT_INTRO))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:Ferrite_Bead_0603 (layer F.Cu) (tedit 58F67155)
    (at 313.643517 102.76624)
    (descr "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (tags "Neosid, Inductor, SM0603CG, Festinduktivitaet, SMD,")
    (attr smd)
    (fp_text reference FB43 (at 0.09906 -2.30124) (layer F.SilkS))
    (fp_text value MMZ1608A252BTA00 (at -0.20066 2.70002) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 544 "Net-(FB43-Pad2)"))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 541 /SPI0_MOSI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57FE9783)
    (at 364.791428 96.315)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB49 (at 0 -2.1) (layer F.SilkS))
    (fp_text value LI0805H151R-10 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /USB/USB.B.VBUS))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57FE9783)
    (at 312.371428 39.075)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB50 (at 0 -2.1) (layer F.SilkS))
    (fp_text value LI0805H151R-10 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57FE9788)
    (at 334.468571 71.915)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.25) (layer F.SilkS))
    (fp_text value MMBT2907 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 727 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 77 VDD_3V3A))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57FE9788)
    (at 311.871428 76.965)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.25) (layer F.SilkS))
    (fp_text value DNP-MMBT2907 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 730 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 359.672381 87.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 723 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 /USR3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 383.272381 71.565)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 724 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 /USR2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 362.972381 87.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 725 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 /USR1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 376.652381 76.815)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 726 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 /USR0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 380.5 77.415)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 470Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(P15-Pad10)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 387.048571 71.565)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /Ethernet/YELA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 376.28 83.265)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 470Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(P15-Pad11)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 369.415001 76.615)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 371.716666 82.665)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 /SERVO_0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 366.986666 87.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 521 VDD_5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 579 "Net-(D7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 339.358571 91.815)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 348.448571 84.015)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 335.03 91.815)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 499Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 VDD_3V3A))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 727 "Net-(D9-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 330.535238 90.265)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNPΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 728 "Net-(D9-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 727 "Net-(D9-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 332.428571 84.215)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 VDD_3V3A))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 728 "Net-(D9-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 343.482857 83.465)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 40.2kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 728 "Net-(D9-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 343.482857 77.615)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 729 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 309.942857 89.065)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-499Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 730 "Net-(D12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 336.845238 85.965)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNPΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 731 "Net-(D12-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 730 "Net-(D12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 322.411428 78.165)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 731 "Net-(D12-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 310.585714 83.215)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-40.2kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 731 "Net-(D12-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 VDD_1V8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 324.122857 102.365)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 322.362857 109.415)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.75kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 415.162381 82.635)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /Flash/GPIO1_16.SIP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 722 /ENC_A))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 359.672381 108.415)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R45 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 625 "Net-(R45-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 368.396666 102.365)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R46 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1.5kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 /I2C0_SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 373.688571 101.965)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R47 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 /USB/USB1_DRVVBUS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 363.686666 108.415)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R48 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1.5kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 708 /SIP_I2C0_SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 376.512381 96.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R49 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /~USB1_OC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 373.626666 107.815)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R50 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100mΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /USB/USB1_VBUS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(C23-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 373.212381 96.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R51 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 USB_DC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 626 "Net-(R51-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 380.764762 96.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R52 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 /USB/UART0_RXD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 340.843809 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R53 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 627 "Net-(R53-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 651 "Net-(C27-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 309.561904 56.825)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R54 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-1MΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 656 "Net-(C28-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 627 "Net-(R53-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 331.356666 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R55 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-10Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 628 /Ethernet/REFCLKO))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /Ethernet/MII1_REFCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 354.93 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R56 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 629 /Ethernet/RXD3/PHYAD2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 /Ethernet/MII1_RXD3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 325.15 62.675)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R57 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 630 /Ethernet/RXD2/RMIISEL))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 /Ethernet/MII1_RXD2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 347.16 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R58 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 631 /Ethernet/RXD1/MODE1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /Ethernet/MII1_RXD1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 328.95 56.825)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R59 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 632 /Ethernet/RXD0/MODE0))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 /Ethernet/MII1_RXD0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 342.22 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R60 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 633 /Ethernet/RXDV))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 107 /Ethernet/MII1_RXDV))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 333.35 56.425)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R61 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 628 /Ethernet/REFCLKO))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 108 /Ethernet/MII1_RXCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 336.92 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R62 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 634 /Ethernet/RXER/PHYAD0))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 109 /Ethernet/MII1_RXERR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 320.75 62.675)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R63 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 635 /Ethernet/TXCLK))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 110 /Ethernet/MII1_TXCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 328.7 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R64 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 636 /Ethernet/MODE2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 /Ethernet/MII1_COL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 342.62 56.425)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R65 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 637 /Ethernet/CRS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 /Ethernet/MII1_CRS_DV))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 356.022381 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R66 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 638 /Ethernet/RCLKIN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 656 "Net-(C28-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 317.340476 50.975)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R67 (at 0 -1.9) (layer F.SilkS))
    (fp_text value DNP-0Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 638 /Ethernet/RCLKIN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /Ethernet/MII1_REFCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 324.386666 56.825)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R68 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1.5kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 113 /Ethernet/MDIO_DATA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 349.058095 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R69 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 49.9Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /Ethernet/RD+))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 330.192857 62.675)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R70 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 12.1kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 639 /Ethernet/RBIAS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 315.648571 56.825)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R71 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 634 /Ethernet/RXER/PHYAD0))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 337.988095 56.425)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R72 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 49.9Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /Ethernet/RD-))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 322.858571 50.975)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R73 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 640 /Ethernet/ETH_TXD4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 308.038095 62.675)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R74 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 49.9Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /Ethernet/TD+))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 346.548571 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R75 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 629 /Ethernet/RXD3/PHYAD2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 337.588095 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R76 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 49.9Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 621 VDD_PHYA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /Ethernet/TD-))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 319.898571 56.825)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R77 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 630 /Ethernet/RXD2/RMIISEL))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 333.028571 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R78 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 628 /Ethernet/REFCLKO))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 327.346666 50.975)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R79 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1.5kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 636 /Ethernet/MODE2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 312.836666 62.675)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R80 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1.5kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 631 /Ethernet/RXD1/MODE1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 337.586666 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R81 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1.5kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 632 /Ethernet/RXD0/MODE0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 401.308571 67.315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R82 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /SD.CD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 401.308571 73.165)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R83 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 /MMC0_DAT3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 405.558571 67.315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R84 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /MMC0_DAT2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 409.808571 67.315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R85 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 /MMC0_DAT1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 405.558571 73.165)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R86 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 /MMC0_DAT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 409.808571 73.165)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R87 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 /MMC0_CMD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 414.058571 67.315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R88 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 /MMC0_CLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 348.86 102.365)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R99 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /Z1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 620 "Net-(FB55-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 334.276666 102.365)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R100 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /Z1_ENDSTOP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 339.286666 108.215)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 722 /ENC_A))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 647 "Net-(FB56-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 344.016666 108.215)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /ENC_B))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 710 "Net-(FB57-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 411.836666 48.025)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R104 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 115 /~SR_EN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 421.296666 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R105 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /~SS_DOCK1_T))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 416.566666 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R106 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /~SS_DOCK1_NVM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 429.646666 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R107 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /~SS_DOCK0_T))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 424.916666 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R108 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /~SS_DOCK0_NVM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 420.186666 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R109 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 713 "Net-(R109-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 424.916666 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R110 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 507 /~SS_H_NVM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 420.186666 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R112 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 506 /~SS_E_NVM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 410.116666 92.015)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R115 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 /E_FAULT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 406.276666 82.635)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R121 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 /X2_ENDSTOP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 401.546666 82.635)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R122 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 118 /X_FAULT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 400.516666 96.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R128 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 /Z2_ENDSTOP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 395.786666 96.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R129 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 /Z_FAULT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 395.786666 105.495)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R145 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 /H_FAULT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 426.416666 60.405)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R151 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 /Y2_ENDSTOP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 431.146666 60.405)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R152 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 123 /Y_FAULT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 426.416666 69.785)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R163 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 /CLKOUT2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 392.834762 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R212 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 176 /Configuration/LCD.D0.B0--B3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 388.03 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R213 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 732 "Net-(R213-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 174 /Configuration/LCD.D2.B2--B5))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 377.594762 56.425)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R214 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 /Configuration/LCD.D1.B1--B4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 395.534762 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R215 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 174 /Configuration/LCD.D2.B2--B5))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 391.294762 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R216 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 173 /Configuration/LCD.D3.B3--B6))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 381.844762 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R217 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 /Configuration/LCD.D4.B4--B7))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 390.334762 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R218 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 /Configuration/LCD.D5.G0--G2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 398.034762 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R219 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 170 /Configuration/LCD.D6.G1--G3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 387.044762 56.425)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R220 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 169 /Configuration/LCD.D7.G2--G4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 396.494762 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R221 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 168 /Configuration/LCD.D8.G3--G5))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 403.234762 44.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R222 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 167 /Configuration/LCD.D9.G4--G6))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 392.244762 56.425)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R223 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 166 /Configuration/LCD.D10.G5--G7))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 401.694762 50.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R224 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 /Configuration/LCD.D11.R0--R3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 397.444762 56.425)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R225 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 /Configuration/LCD.D12.R1--R4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 380.884762 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R226 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 /Configuration/LCD.D13.R2--R5))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 371.434762 38.875)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R227 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 /Configuration/LCD.D14.R3--R6))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FE9783)
    (at 363.894762 52.525)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R228 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 161 /Configuration/LCD.D15.R4--R7))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiMBo:KMR_SW_SPST_EVQP7A (layer F.Cu) (tedit 58F9179C)
    (at 337.665001 78.765)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value RESET (at 0 3.25) (layer F.Fab))
    (pad 3 smd rect (at 2.045 -0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.045 -0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 4 smd rect (at 2.045 0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
    (pad 2 smd rect (at -2.045 0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 2 /~SYS_RESET))
  )
  (module KiMBo:KMR_SW_SPST_EVQP7A (layer F.Cu) (tedit 58F9179C)
    (at 325.265001 90.865)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value Power (at 0 3.25) (layer F.Fab))
    (pad 3 smd rect (at 2.045 -0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 1 smd rect (at -2.045 -0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 4 smd rect (at 2.045 0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 124 /Power/PWR_BUT))
    (pad 2 smd rect (at -2.045 0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 124 /Power/PWR_BUT))
  )
  (module KiMBo:KMR_SW_SPST_EVQP7A (layer F.Cu) (tedit 58F9179C)
    (at 365.061429 39.475)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value μSD_Boot (at 0 3.25) (layer F.Fab))
    (pad 3 smd rect (at 2.045 -0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 732 "Net-(R213-Pad1)"))
    (pad 1 smd rect (at -2.045 -0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 732 "Net-(R213-Pad1)"))
    (pad 4 smd rect (at 2.045 0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 2 smd rect (at -2.045 0.8) (size 0.89 1.015) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57FE977C)
    (at 326.299524 84.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2) (layer F.SilkS))
    (fp_text value Test_Point (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 CGND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57FE977C)
    (at 342.599524 71.665)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP2 (at 0 -2) (layer F.SilkS))
    (fp_text value Test_Point (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 125 /Power/BAT_TEMP))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57FE977C)
    (at 330.689524 78.265)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP3 (at 0 -2) (layer F.SilkS))
    (fp_text value Test_Point (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 126 /Power/BAT_VOLT))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57FE977C)
    (at 318.289524 89.165)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP4 (at 0 -2) (layer F.SilkS))
    (fp_text value Test_Point (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 127 /Power/VIN_BAT))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57FE977C)
    (at 362.029524 102.465)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP6 (at 0 -2) (layer F.SilkS))
    (fp_text value Test_Point (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 128 /USB/~UART0_RST))
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 57FE977A)
    (at 413.645001 40.525)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U12 (at 0 -3.55) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 3.55) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 193 "/Stepper Drivers/~X1_EN"))
    (pad 2 smd rect (at -2.95 -1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 448 "/Stepper Drivers/~Y_EN"))
    (pad 3 smd rect (at -2.95 -0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 449 "/Stepper Drivers/~Z0_EN"))
    (pad 4 smd rect (at -2.95 -0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 487 "/Stepper Drivers/~Z1_EN"))
    (pad 5 smd rect (at -2.95 0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 488 "/Stepper Drivers/~Z2_EN"))
    (pad 6 smd rect (at -2.95 0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 159 "/Stepper Drivers/~E_EN"))
    (pad 7 smd rect (at -2.95 1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 489 "/Stepper Drivers/~H_EN"))
    (pad 8 smd rect (at -2.95 2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 9 smd rect (at 2.95 2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 733 "Net-(U12-Pad9)"))
    (pad 10 smd rect (at 2.95 1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 115 /~SR_EN))
    (pad 11 smd rect (at 2.95 0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI1_SCLK))
    (pad 12 smd rect (at 2.95 0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 135 /SPI1_CS0))
    (pad 13 smd rect (at 2.95 -0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 CGND))
    (pad 14 smd rect (at 2.95 -0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U11-Pad9)"))
    (pad 15 smd rect (at 2.95 -1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 187 "/Stepper Drivers/~X0_EN"))
    (pad 16 smd rect (at 2.95 -2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text X0 (at 105.6 153.5) (layer F.SilkS))
  (gr_text H (at 213.9 153.5) (layer F.SilkS))
  (gr_text X1 (at 123.6 153.5) (layer F.SilkS))
  (gr_text Y (at 87.9 153.5) (layer F.SilkS))
  (gr_text Z0 (at 141.6 153.5) (layer F.SilkS))
  (gr_text Z1 (at 159.6 153.5) (layer F.SilkS))
  (gr_text Z2 (at 177.6 153.5) (layer F.SilkS))
  (gr_text X0 (at 110 174) (layer Eco2.User))
  (gr_text X1 (at 128 174) (layer Eco2.User))
  (gr_text Y (at 146 174) (layer Eco2.User))
  (gr_text Z0 (at 165 174) (layer Eco2.User))
  (gr_text E (at 195.9 153.5) (layer F.SilkS))
  (gr_line (start 244 25) (end 54 25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 244 160) (end 244 25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54 160) (end 244 160) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54 25) (end 54 160) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text ADC (at 87.1 22.4) (layer Eco2.User))
  (gr_text BED_T (at 70.1 22.4) (layer Eco2.User))
  (gr_text DOCK1_HEAT (at 36.1 72.4) (layer Eco2.User))
  (gr_text DOCK0_HEAT (at 36.1 85.4) (layer Eco2.User))
  (gr_text H_HEAT (at 36.1 98.4) (layer Eco2.User))
  (gr_text E_HEAT (at 36.1 111.4) (layer Eco2.User))
  (gr_text BED_HEAT (at 36.1 124.4) (layer Eco2.User))
  (gr_text PWR_IN (at 36.1 141.4) (layer Eco2.User))
  (gr_text μUSB-OTG (at 269.1 89.4) (layer Eco2.User))
  (gr_text USB-Host (at 268.1 75.4) (layer Eco2.User))
  (gr_text Ethernet (at 265.1 105.4) (layer Eco2.User))
  (gr_text μSD (at 256.1 47.4) (layer Eco2.User))
  (gr_text H (at 236 174) (layer Eco2.User))
  (gr_text E (at 219 174) (layer Eco2.User))
  (gr_text Z2 (at 200 174) (layer Eco2.User))
  (gr_text Z1 (at 183 174) (layer Eco2.User))
  (gr_text 24V_FANS (at 26.1 53.4) (layer Eco2.User))
  (gr_text END/ENC (at 233.1 21.4) (layer Eco2.User))
  (gr_text EPM (at 206.1 21.4) (layer Eco2.User))
  (gr_text SPI (at 150.1 19.4) (layer Eco2.User))
  (zone (net 19) (net_name "/Stepper Drivers/E_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 201.64 139.95) (xy 199.54 139.95) (xy 198.99 139.4) (xy 197.29 139.4) (xy 197.29 142.2)
        (xy 198.84 142.2) (xy 201.39 144.85) (xy 201.39 152.15) (xy 201.54 152.15) (xy 201.54 154.2)
        (xy 204.09 154.2) (xy 204.09 142.9) (xy 204.14 142.85) (xy 204.14 142.45)
      )
    )
  )
  (zone (net 18) (net_name "/Stepper Drivers/E_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 206.49 142.05) (xy 208.19 142.05) (xy 208.79 141.45) (xy 208.79 140.35) (xy 209.49 139.65)
        (xy 210.69 139.65) (xy 210.69 142.2) (xy 208.74 142.2) (xy 208.39 142.55) (xy 206.49 142.55)
      )
    )
  )
  (zone (net 18) (net_name "/Stepper Drivers/E_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 206.59 154.2) (xy 209.64 154.2) (xy 210.89 152.95) (xy 210.89 139.5) (xy 209.59 139.5)
        (xy 206.59 144.75)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 207.99 143.85) (xy 207.99 142.55) (xy 208.39 142.55) (xy 208.49 142.45) (xy 210.19 142.45)
        (xy 210.19 144.7) (xy 210.64 145.15) (xy 210.74 145.15) (xy 210.74 146.65) (xy 209.74 146.65)
        (xy 209.74 145.6) (xy 209.39 145.25) (xy 208.89 145.25) (xy 208.19 144.55) (xy 208.19 144.05)
      )
    )
  )
  (zone (net 21) (net_name "/Stepper Drivers/E_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.69 141.05) (xy 200.09 141.05) (xy 200.09 139.95) (xy 200.19 139.85) (xy 201.39 139.85)
        (xy 201.39 138.65) (xy 201.49 138.55) (xy 201.49 137.75) (xy 198.89 137.75) (xy 198.89 138.95)
        (xy 198.89 139.35) (xy 199.69 140.15) (xy 199.69 141.25) (xy 199.99 141.55) (xy 201.69 141.55)
      )
    )
  )
  (zone (net 20) (net_name "/Stepper Drivers/E_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 206.49 141.05) (xy 208.09 141.05) (xy 208.09 139.95) (xy 207.99 139.85) (xy 206.79 139.85)
        (xy 206.79 138.65) (xy 206.69 138.55) (xy 206.69 137.75) (xy 209.29 137.75) (xy 209.29 139.35)
        (xy 208.49 140.15) (xy 208.49 141.25) (xy 208.19 141.55) (xy 206.49 141.55)
      )
    )
  )
  (zone (net 19) (net_name "/Stepper Drivers/E_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.69 142.05) (xy 199.99 142.05) (xy 199.29 141.35) (xy 199.29 140.25) (xy 198.69 139.65)
        (xy 197.49 139.65) (xy 197.59 142.55) (xy 201.69 142.55)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.69 142.55) (xy 198.09 142.55) (xy 198.09 143.75) (xy 197.89 143.75) (xy 197.89 144.55)
        (xy 198.29 144.85) (xy 199.59 144.85) (xy 199.99 144.55) (xy 199.99 143.05) (xy 201.69 143.05)
      )
    )
  )
  (zone (net 21) (net_name "/Stepper Drivers/E_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 201.49 138.05) (xy 200.04 136.6) (xy 195.49 136.6) (xy 194.49 137.6) (xy 194.49 150.2)
        (xy 198.49 154.2) (xy 201.54 154.2) (xy 201.54 152.15) (xy 201.39 152.15) (xy 201.39 144.85)
        (xy 198.84 142.2) (xy 197.29 142.2) (xy 197.29 139.4) (xy 198.99 139.4) (xy 199.54 139.95)
        (xy 201.49 139.95)
      )
    )
  )
  (zone (net 20) (net_name "/Stepper Drivers/E_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 209.34 137.7) (xy 206.79 137.7) (xy 206.79 139.95) (xy 205.29 139.95) (xy 204.09 141.15)
        (xy 204.09 142.4) (xy 204.14 142.45) (xy 204.14 142.85) (xy 204.09 142.9) (xy 204.09 154.2)
        (xy 206.59 154.2) (xy 206.59 144.75) (xy 209.34 139.95)
      )
    )
  )
  (zone (net 469) (net_name "/Stepper Drivers/Z2_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 183.64 139.95) (xy 181.54 139.95) (xy 180.99 139.4) (xy 179.29 139.4) (xy 179.29 142.2)
        (xy 180.84 142.2) (xy 183.39 144.85) (xy 183.39 152.15) (xy 183.54 152.15) (xy 183.54 154.2)
        (xy 186.09 154.2) (xy 186.09 142.9) (xy 186.14 142.85) (xy 186.14 142.45)
      )
    )
  )
  (zone (net 471) (net_name "/Stepper Drivers/Z2_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.69 141.05) (xy 182.09 141.05) (xy 182.09 139.95) (xy 182.19 139.85) (xy 183.39 139.85)
        (xy 183.39 138.65) (xy 183.49 138.55) (xy 183.49 137.75) (xy 180.89 137.75) (xy 180.89 138.95)
        (xy 180.89 139.35) (xy 181.69 140.15) (xy 181.69 141.25) (xy 181.99 141.55) (xy 183.69 141.55)
      )
    )
  )
  (zone (net 470) (net_name "/Stepper Drivers/Z2_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 188.49 141.05) (xy 190.09 141.05) (xy 190.09 139.95) (xy 189.99 139.85) (xy 188.79 139.85)
        (xy 188.79 138.65) (xy 188.69 138.55) (xy 188.69 137.75) (xy 191.29 137.75) (xy 191.29 139.35)
        (xy 190.49 140.15) (xy 190.49 141.25) (xy 190.19 141.55) (xy 188.49 141.55)
      )
    )
  )
  (zone (net 469) (net_name "/Stepper Drivers/Z2_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.69 142.05) (xy 181.99 142.05) (xy 181.29 141.35) (xy 181.29 140.25) (xy 180.69 139.65)
        (xy 179.49 139.65) (xy 179.59 142.55) (xy 183.69 142.55)
      )
    )
  )
  (zone (net 471) (net_name "/Stepper Drivers/Z2_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 183.49 138.05) (xy 182.04 136.6) (xy 177.49 136.6) (xy 176.49 137.6) (xy 176.49 150.2)
        (xy 180.49 154.2) (xy 183.54 154.2) (xy 183.54 152.15) (xy 183.39 152.15) (xy 183.39 144.85)
        (xy 180.84 142.2) (xy 179.29 142.2) (xy 179.29 139.4) (xy 180.99 139.4) (xy 181.54 139.95)
        (xy 183.49 139.95)
      )
    )
  )
  (zone (net 470) (net_name "/Stepper Drivers/Z2_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 191.34 137.7) (xy 188.79 137.7) (xy 188.79 139.95) (xy 187.29 139.95) (xy 186.09 141.15)
        (xy 186.09 142.4) (xy 186.14 142.45) (xy 186.14 142.85) (xy 186.09 142.9) (xy 186.09 154.2)
        (xy 188.59 154.2) (xy 188.59 144.75) (xy 191.34 139.95)
      )
    )
  )
  (zone (net 468) (net_name "/Stepper Drivers/Z2_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 188.59 154.2) (xy 191.64 154.2) (xy 192.89 152.95) (xy 192.89 139.5) (xy 191.59 139.5)
        (xy 188.59 144.75)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 189.99 143.85) (xy 189.99 142.55) (xy 190.39 142.55) (xy 190.49 142.45) (xy 192.19 142.45)
        (xy 192.19 144.7) (xy 192.64 145.15) (xy 192.74 145.15) (xy 192.74 146.65) (xy 191.74 146.65)
        (xy 191.74 145.6) (xy 191.39 145.25) (xy 190.89 145.25) (xy 190.19 144.55) (xy 190.19 144.05)
      )
    )
  )
  (zone (net 468) (net_name "/Stepper Drivers/Z2_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 188.49 142.05) (xy 190.19 142.05) (xy 190.79 141.45) (xy 190.79 140.35) (xy 191.49 139.65)
        (xy 192.69 139.65) (xy 192.69 142.2) (xy 190.74 142.2) (xy 190.39 142.55) (xy 188.49 142.55)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.69 142.55) (xy 180.09 142.55) (xy 180.09 143.75) (xy 179.89 143.75) (xy 179.89 144.55)
        (xy 180.29 144.85) (xy 181.59 144.85) (xy 181.99 144.55) (xy 181.99 143.05) (xy 183.69 143.05)
      )
    )
  )
  (zone (net 464) (net_name "/Stepper Drivers/Z1_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.69 142.05) (xy 163.99 142.05) (xy 163.29 141.35) (xy 163.29 140.25) (xy 162.69 139.65)
        (xy 161.49 139.65) (xy 161.59 142.55) (xy 165.69 142.55)
      )
    )
  )
  (zone (net 466) (net_name "/Stepper Drivers/Z1_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.69 141.05) (xy 164.09 141.05) (xy 164.09 139.95) (xy 164.19 139.85) (xy 165.39 139.85)
        (xy 165.39 138.65) (xy 165.49 138.55) (xy 165.49 137.75) (xy 162.89 137.75) (xy 162.89 138.95)
        (xy 162.89 139.35) (xy 163.69 140.15) (xy 163.69 141.25) (xy 163.99 141.55) (xy 165.69 141.55)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 171.99 143.85) (xy 171.99 142.55) (xy 172.39 142.55) (xy 172.49 142.45) (xy 174.19 142.45)
        (xy 174.19 144.7) (xy 174.64 145.15) (xy 174.74 145.15) (xy 174.74 146.65) (xy 173.74 146.65)
        (xy 173.74 145.6) (xy 173.39 145.25) (xy 172.89 145.25) (xy 172.19 144.55) (xy 172.19 144.05)
      )
    )
  )
  (zone (net 463) (net_name "/Stepper Drivers/Z1_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 170.49 142.05) (xy 172.19 142.05) (xy 172.79 141.45) (xy 172.79 140.35) (xy 173.49 139.65)
        (xy 174.69 139.65) (xy 174.69 142.2) (xy 172.74 142.2) (xy 172.39 142.55) (xy 170.49 142.55)
      )
    )
  )
  (zone (net 465) (net_name "/Stepper Drivers/Z1_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 173.34 137.7) (xy 170.79 137.7) (xy 170.79 139.95) (xy 169.29 139.95) (xy 168.09 141.15)
        (xy 168.09 142.4) (xy 168.14 142.45) (xy 168.14 142.85) (xy 168.09 142.9) (xy 168.09 154.2)
        (xy 170.59 154.2) (xy 170.59 144.75) (xy 173.34 139.95)
      )
    )
  )
  (zone (net 464) (net_name "/Stepper Drivers/Z1_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 165.64 139.95) (xy 163.54 139.95) (xy 162.99 139.4) (xy 161.29 139.4) (xy 161.29 142.2)
        (xy 162.84 142.2) (xy 165.39 144.85) (xy 165.39 152.15) (xy 165.54 152.15) (xy 165.54 154.2)
        (xy 168.09 154.2) (xy 168.09 142.9) (xy 168.14 142.85) (xy 168.14 142.45)
      )
    )
  )
  (zone (net 466) (net_name "/Stepper Drivers/Z1_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 165.49 138.05) (xy 164.04 136.6) (xy 159.49 136.6) (xy 158.49 137.6) (xy 158.49 150.2)
        (xy 162.49 154.2) (xy 165.54 154.2) (xy 165.54 152.15) (xy 165.39 152.15) (xy 165.39 144.85)
        (xy 162.84 142.2) (xy 161.29 142.2) (xy 161.29 139.4) (xy 162.99 139.4) (xy 163.54 139.95)
        (xy 165.49 139.95)
      )
    )
  )
  (zone (net 465) (net_name "/Stepper Drivers/Z1_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 170.49 141.05) (xy 172.09 141.05) (xy 172.09 139.95) (xy 171.99 139.85) (xy 170.79 139.85)
        (xy 170.79 138.65) (xy 170.69 138.55) (xy 170.69 137.75) (xy 173.29 137.75) (xy 173.29 139.35)
        (xy 172.49 140.15) (xy 172.49 141.25) (xy 172.19 141.55) (xy 170.49 141.55)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.69 142.55) (xy 162.09 142.55) (xy 162.09 143.75) (xy 161.89 143.75) (xy 161.89 144.55)
        (xy 162.29 144.85) (xy 163.59 144.85) (xy 163.99 144.55) (xy 163.99 143.05) (xy 165.69 143.05)
      )
    )
  )
  (zone (net 197) (net_name "/Stepper Drivers/Z0_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 152.49 141.05) (xy 154.09 141.05) (xy 154.09 139.95) (xy 153.99 139.85) (xy 152.79 139.85)
        (xy 152.79 138.65) (xy 152.69 138.55) (xy 152.69 137.75) (xy 155.29 137.75) (xy 155.29 139.35)
        (xy 154.49 140.15) (xy 154.49 141.25) (xy 154.19 141.55) (xy 152.49 141.55)
      )
    )
  )
  (zone (net 196) (net_name "/Stepper Drivers/Z0_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 147.64 139.95) (xy 145.54 139.95) (xy 144.99 139.4) (xy 143.29 139.4) (xy 143.29 142.2)
        (xy 144.84 142.2) (xy 147.39 144.85) (xy 147.39 152.15) (xy 147.54 152.15) (xy 147.54 154.2)
        (xy 150.09 154.2) (xy 150.09 142.9) (xy 150.14 142.85) (xy 150.14 142.45)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.69 142.55) (xy 144.09 142.55) (xy 144.09 143.75) (xy 143.89 143.75) (xy 143.89 144.55)
        (xy 144.29 144.85) (xy 145.59 144.85) (xy 145.99 144.55) (xy 145.99 143.05) (xy 147.69 143.05)
      )
    )
  )
  (zone (net 195) (net_name "/Stepper Drivers/Z0_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 152.49 142.05) (xy 154.19 142.05) (xy 154.79 141.45) (xy 154.79 140.35) (xy 155.49 139.65)
        (xy 156.69 139.65) (xy 156.69 142.2) (xy 154.74 142.2) (xy 154.39 142.55) (xy 152.49 142.55)
      )
    )
  )
  (zone (net 198) (net_name "/Stepper Drivers/Z0_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.69 141.05) (xy 146.09 141.05) (xy 146.09 139.95) (xy 146.19 139.85) (xy 147.39 139.85)
        (xy 147.39 138.65) (xy 147.49 138.55) (xy 147.49 137.75) (xy 144.89 137.75) (xy 144.89 138.95)
        (xy 144.89 139.35) (xy 145.69 140.15) (xy 145.69 141.25) (xy 145.99 141.55) (xy 147.69 141.55)
      )
    )
  )
  (zone (net 196) (net_name "/Stepper Drivers/Z0_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.69 142.05) (xy 145.99 142.05) (xy 145.29 141.35) (xy 145.29 140.25) (xy 144.69 139.65)
        (xy 143.49 139.65) (xy 143.59 142.55) (xy 147.69 142.55)
      )
    )
  )
  (zone (net 198) (net_name "/Stepper Drivers/Z0_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 147.49 138.05) (xy 146.04 136.6) (xy 141.49 136.6) (xy 140.49 137.6) (xy 140.49 150.2)
        (xy 144.49 154.2) (xy 147.54 154.2) (xy 147.54 152.15) (xy 147.39 152.15) (xy 147.39 144.85)
        (xy 144.84 142.2) (xy 143.29 142.2) (xy 143.29 139.4) (xy 144.99 139.4) (xy 145.54 139.95)
        (xy 147.49 139.95)
      )
    )
  )
  (zone (net 195) (net_name "/Stepper Drivers/Z0_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 152.59 154.2) (xy 155.64 154.2) (xy 156.89 152.95) (xy 156.89 139.5) (xy 155.59 139.5)
        (xy 152.59 144.75)
      )
    )
  )
  (zone (net 197) (net_name "/Stepper Drivers/Z0_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 155.34 137.7) (xy 152.79 137.7) (xy 152.79 139.95) (xy 151.29 139.95) (xy 150.09 141.15)
        (xy 150.09 142.4) (xy 150.14 142.45) (xy 150.14 142.85) (xy 150.09 142.9) (xy 150.09 154.2)
        (xy 152.59 154.2) (xy 152.59 144.75) (xy 155.34 139.95)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 153.99 143.85) (xy 153.99 142.55) (xy 154.39 142.55) (xy 154.49 142.45) (xy 156.19 142.45)
        (xy 156.19 144.7) (xy 156.64 145.15) (xy 156.74 145.15) (xy 156.74 146.65) (xy 155.74 146.65)
        (xy 155.74 145.6) (xy 155.39 145.25) (xy 154.89 145.25) (xy 154.19 144.55) (xy 154.19 144.05)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.69 142.55) (xy 90.09 142.55) (xy 90.09 143.75) (xy 89.89 143.75) (xy 89.89 144.55)
        (xy 90.29 144.85) (xy 91.59 144.85) (xy 91.99 144.55) (xy 91.99 143.05) (xy 93.69 143.05)
      )
    )
  )
  (zone (net 200) (net_name "/Stepper Drivers/Y_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 98.59 154.2) (xy 101.64 154.2) (xy 102.89 152.95) (xy 102.89 139.5) (xy 101.59 139.5)
        (xy 98.59 144.75)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 99.99 143.85) (xy 99.99 142.55) (xy 100.39 142.55) (xy 100.49 142.45) (xy 102.19 142.45)
        (xy 102.19 144.7) (xy 102.64 145.15) (xy 102.74 145.15) (xy 102.74 146.65) (xy 101.74 146.65)
        (xy 101.74 145.6) (xy 101.39 145.25) (xy 100.89 145.25) (xy 100.19 144.55) (xy 100.19 144.05)
      )
    )
  )
  (zone (net 202) (net_name "/Stepper Drivers/Y_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 101.34 137.7) (xy 98.79 137.7) (xy 98.79 139.95) (xy 97.29 139.95) (xy 96.09 141.15)
        (xy 96.09 142.4) (xy 96.14 142.45) (xy 96.14 142.85) (xy 96.09 142.9) (xy 96.09 154.2)
        (xy 98.59 154.2) (xy 98.59 144.75) (xy 101.34 139.95)
      )
    )
  )
  (zone (net 203) (net_name "/Stepper Drivers/Y_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.69 141.05) (xy 92.09 141.05) (xy 92.09 139.95) (xy 92.19 139.85) (xy 93.39 139.85)
        (xy 93.39 138.65) (xy 93.49 138.55) (xy 93.49 137.75) (xy 90.89 137.75) (xy 90.89 138.95)
        (xy 90.89 139.35) (xy 91.69 140.15) (xy 91.69 141.25) (xy 91.99 141.55) (xy 93.69 141.55)
      )
    )
  )
  (zone (net 202) (net_name "/Stepper Drivers/Y_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 98.49 141.05) (xy 100.09 141.05) (xy 100.09 139.95) (xy 99.99 139.85) (xy 98.79 139.85)
        (xy 98.79 138.65) (xy 98.69 138.55) (xy 98.69 137.75) (xy 101.29 137.75) (xy 101.29 139.35)
        (xy 100.49 140.15) (xy 100.49 141.25) (xy 100.19 141.55) (xy 98.49 141.55)
      )
    )
  )
  (zone (net 201) (net_name "/Stepper Drivers/Y_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 93.64 139.95) (xy 91.54 139.95) (xy 90.99 139.4) (xy 89.29 139.4) (xy 89.29 142.2)
        (xy 90.84 142.2) (xy 93.39 144.85) (xy 93.39 152.15) (xy 93.54 152.15) (xy 93.54 154.2)
        (xy 96.09 154.2) (xy 96.09 142.9) (xy 96.14 142.85) (xy 96.14 142.45)
      )
    )
  )
  (zone (net 200) (net_name "/Stepper Drivers/Y_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 98.49 142.05) (xy 100.19 142.05) (xy 100.79 141.45) (xy 100.79 140.35) (xy 101.49 139.65)
        (xy 102.69 139.65) (xy 102.69 142.2) (xy 100.74 142.2) (xy 100.39 142.55) (xy 98.49 142.55)
      )
    )
  )
  (zone (net 201) (net_name "/Stepper Drivers/Y_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.69 142.05) (xy 91.99 142.05) (xy 91.29 141.35) (xy 91.29 140.25) (xy 90.69 139.65)
        (xy 89.49 139.65) (xy 89.59 142.55) (xy 93.69 142.55)
      )
    )
  )
  (zone (net 203) (net_name "/Stepper Drivers/Y_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 93.49 138.05) (xy 92.04 136.6) (xy 87.49 136.6) (xy 86.49 137.6) (xy 86.49 150.2)
        (xy 90.49 154.2) (xy 93.54 154.2) (xy 93.54 152.15) (xy 93.39 152.15) (xy 93.39 144.85)
        (xy 90.84 142.2) (xy 89.29 142.2) (xy 89.29 139.4) (xy 90.99 139.4) (xy 91.54 139.95)
        (xy 93.49 139.95)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 135.99 143.85) (xy 135.99 142.55) (xy 136.39 142.55) (xy 136.49 142.45) (xy 138.19 142.45)
        (xy 138.19 144.7) (xy 138.64 145.15) (xy 138.74 145.15) (xy 138.74 146.65) (xy 137.74 146.65)
        (xy 137.74 145.6) (xy 137.39 145.25) (xy 136.89 145.25) (xy 136.19 144.55) (xy 136.19 144.05)
      )
    )
  )
  (zone (net 191) (net_name "/Stepper Drivers/X1_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 137.34 137.7) (xy 134.79 137.7) (xy 134.79 139.95) (xy 133.29 139.95) (xy 132.09 141.15)
        (xy 132.09 142.4) (xy 132.14 142.45) (xy 132.14 142.85) (xy 132.09 142.9) (xy 132.09 154.2)
        (xy 134.59 154.2) (xy 134.59 144.75) (xy 137.34 139.95)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.69 142.55) (xy 126.09 142.55) (xy 126.09 143.75) (xy 125.89 143.75) (xy 125.89 144.55)
        (xy 126.29 144.85) (xy 127.59 144.85) (xy 127.99 144.55) (xy 127.99 143.05) (xy 129.69 143.05)
      )
    )
  )
  (zone (net 190) (net_name "/Stepper Drivers/X1_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.69 142.05) (xy 127.99 142.05) (xy 127.29 141.35) (xy 127.29 140.25) (xy 126.69 139.65)
        (xy 125.49 139.65) (xy 125.59 142.55) (xy 129.69 142.55)
      )
    )
  )
  (zone (net 189) (net_name "/Stepper Drivers/X1_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 134.59 154.2) (xy 137.64 154.2) (xy 138.89 152.95) (xy 138.89 139.5) (xy 137.59 139.5)
        (xy 134.59 144.75)
      )
    )
  )
  (zone (net 192) (net_name "/Stepper Drivers/X1_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.69 141.05) (xy 128.09 141.05) (xy 128.09 139.95) (xy 128.19 139.85) (xy 129.39 139.85)
        (xy 129.39 138.65) (xy 129.49 138.55) (xy 129.49 137.75) (xy 126.89 137.75) (xy 126.89 138.95)
        (xy 126.89 139.35) (xy 127.69 140.15) (xy 127.69 141.25) (xy 127.99 141.55) (xy 129.69 141.55)
      )
    )
  )
  (zone (net 191) (net_name "/Stepper Drivers/X1_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 134.49 141.05) (xy 136.09 141.05) (xy 136.09 139.95) (xy 135.99 139.85) (xy 134.79 139.85)
        (xy 134.79 138.65) (xy 134.69 138.55) (xy 134.69 137.75) (xy 137.29 137.75) (xy 137.29 139.35)
        (xy 136.49 140.15) (xy 136.49 141.25) (xy 136.19 141.55) (xy 134.49 141.55)
      )
    )
  )
  (zone (net 189) (net_name "/Stepper Drivers/X1_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 134.49 142.05) (xy 136.19 142.05) (xy 136.79 141.45) (xy 136.79 140.35) (xy 137.49 139.65)
        (xy 138.69 139.65) (xy 138.69 142.2) (xy 136.74 142.2) (xy 136.39 142.55) (xy 134.49 142.55)
      )
    )
  )
  (zone (net 190) (net_name "/Stepper Drivers/X1_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 129.64 139.95) (xy 127.54 139.95) (xy 126.99 139.4) (xy 125.29 139.4) (xy 125.29 142.2)
        (xy 126.84 142.2) (xy 129.39 144.85) (xy 129.39 152.15) (xy 129.54 152.15) (xy 129.54 154.2)
        (xy 132.09 154.2) (xy 132.09 142.9) (xy 132.14 142.85) (xy 132.14 142.45)
      )
    )
  )
  (zone (net 192) (net_name "/Stepper Drivers/X1_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 129.49 138.05) (xy 128.04 136.6) (xy 123.49 136.6) (xy 122.49 137.6) (xy 122.49 150.2)
        (xy 126.49 154.2) (xy 129.54 154.2) (xy 129.54 152.15) (xy 129.39 152.15) (xy 129.39 144.85)
        (xy 126.84 142.2) (xy 125.29 142.2) (xy 125.29 139.4) (xy 126.99 139.4) (xy 127.54 139.95)
        (xy 129.49 139.95)
      )
    )
  )
  (zone (net 183) (net_name "/Stepper Drivers/X0_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 116.59 154.2) (xy 119.64 154.2) (xy 120.89 152.95) (xy 120.89 139.5) (xy 119.59 139.5)
        (xy 116.59 144.75)
      )
    )
  )
  (zone (net 185) (net_name "/Stepper Drivers/X0_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 116.49 141.05) (xy 118.09 141.05) (xy 118.09 139.95) (xy 117.99 139.85) (xy 116.79 139.85)
        (xy 116.79 138.65) (xy 116.69 138.55) (xy 116.69 137.75) (xy 119.29 137.75) (xy 119.29 139.35)
        (xy 118.49 140.15) (xy 118.49 141.25) (xy 118.19 141.55) (xy 116.49 141.55)
      )
    )
  )
  (zone (net 184) (net_name "/Stepper Drivers/X0_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 111.64 139.95) (xy 109.54 139.95) (xy 108.99 139.4) (xy 107.29 139.4) (xy 107.29 142.2)
        (xy 108.84 142.2) (xy 111.39 144.85) (xy 111.39 152.15) (xy 111.54 152.15) (xy 111.54 154.2)
        (xy 114.09 154.2) (xy 114.09 142.9) (xy 114.14 142.85) (xy 114.14 142.45)
      )
    )
  )
  (zone (net 183) (net_name "/Stepper Drivers/X0_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 116.49 142.05) (xy 118.19 142.05) (xy 118.79 141.45) (xy 118.79 140.35) (xy 119.49 139.65)
        (xy 120.69 139.65) (xy 120.69 142.2) (xy 118.74 142.2) (xy 118.39 142.55) (xy 116.49 142.55)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.69 142.55) (xy 108.09 142.55) (xy 108.09 143.75) (xy 107.89 143.75) (xy 107.89 144.55)
        (xy 108.29 144.85) (xy 109.59 144.85) (xy 109.99 144.55) (xy 109.99 143.05) (xy 111.69 143.05)
      )
    )
  )
  (zone (net 184) (net_name "/Stepper Drivers/X0_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.69 142.05) (xy 109.99 142.05) (xy 109.29 141.35) (xy 109.29 140.25) (xy 108.69 139.65)
        (xy 107.49 139.65) (xy 107.59 142.55) (xy 111.69 142.55)
      )
    )
  )
  (zone (net 186) (net_name "/Stepper Drivers/X0_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 111.49 138.05) (xy 110.04 136.6) (xy 105.49 136.6) (xy 104.49 137.6) (xy 104.49 150.2)
        (xy 108.49 154.2) (xy 111.54 154.2) (xy 111.54 152.15) (xy 111.39 152.15) (xy 111.39 144.85)
        (xy 108.84 142.2) (xy 107.29 142.2) (xy 107.29 139.4) (xy 108.99 139.4) (xy 109.54 139.95)
        (xy 111.49 139.95)
      )
    )
  )
  (zone (net 185) (net_name "/Stepper Drivers/X0_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 119.34 137.7) (xy 116.79 137.7) (xy 116.79 139.95) (xy 115.29 139.95) (xy 114.09 141.15)
        (xy 114.09 142.4) (xy 114.14 142.45) (xy 114.14 142.85) (xy 114.09 142.9) (xy 114.09 154.2)
        (xy 116.59 154.2) (xy 116.59 144.75) (xy 119.34 139.95)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 117.99 143.85) (xy 117.99 142.55) (xy 118.39 142.55) (xy 118.49 142.45) (xy 120.19 142.45)
        (xy 120.19 144.7) (xy 120.64 145.15) (xy 120.74 145.15) (xy 120.74 146.65) (xy 119.74 146.65)
        (xy 119.74 145.6) (xy 119.39 145.25) (xy 118.89 145.25) (xy 118.19 144.55) (xy 118.19 144.05)
      )
    )
  )
  (zone (net 186) (net_name "/Stepper Drivers/X0_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.69 141.05) (xy 110.09 141.05) (xy 110.09 139.95) (xy 110.19 139.85) (xy 111.39 139.85)
        (xy 111.39 138.65) (xy 111.49 138.55) (xy 111.49 137.75) (xy 108.89 137.75) (xy 108.89 138.95)
        (xy 108.89 139.35) (xy 109.69 140.15) (xy 109.69 141.25) (xy 109.99 141.55) (xy 111.69 141.55)
      )
    )
  )
  (zone (net 473) (net_name "/Stepper Drivers/H_A2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 224.49 142.05) (xy 226.19 142.05) (xy 226.79 141.45) (xy 226.79 140.35) (xy 227.49 139.65)
        (xy 228.69 139.65) (xy 228.69 142.2) (xy 226.74 142.2) (xy 226.39 142.55) (xy 224.49 142.55)
      )
    )
  )
  (zone (net 474) (net_name "/Stepper Drivers/H_B2") (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 219.64 139.95) (xy 217.54 139.95) (xy 216.99 139.4) (xy 215.29 139.4) (xy 215.29 142.2)
        (xy 216.84 142.2) (xy 219.39 144.85) (xy 219.39 152.15) (xy 219.54 152.15) (xy 219.54 154.2)
        (xy 222.09 154.2) (xy 222.09 142.9) (xy 222.14 142.85) (xy 222.14 142.45)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 225.99 143.85) (xy 225.99 142.55) (xy 226.39 142.55) (xy 226.49 142.45) (xy 228.19 142.45)
        (xy 228.19 144.7) (xy 228.64 145.15) (xy 228.74 145.15) (xy 228.74 146.65) (xy 227.74 146.65)
        (xy 227.74 145.6) (xy 227.39 145.25) (xy 226.89 145.25) (xy 226.19 144.55) (xy 226.19 144.05)
      )
    )
  )
  (zone (net 476) (net_name "/Stepper Drivers/H_B1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.69 141.05) (xy 218.09 141.05) (xy 218.09 139.95) (xy 218.19 139.85) (xy 219.39 139.85)
        (xy 219.39 138.65) (xy 219.49 138.55) (xy 219.49 137.75) (xy 216.89 137.75) (xy 216.89 138.95)
        (xy 216.89 139.35) (xy 217.69 140.15) (xy 217.69 141.25) (xy 217.99 141.55) (xy 219.69 141.55)
      )
    )
  )
  (zone (net 475) (net_name "/Stepper Drivers/H_A1") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 224.49 141.05) (xy 226.09 141.05) (xy 226.09 139.95) (xy 225.99 139.85) (xy 224.79 139.85)
        (xy 224.79 138.65) (xy 224.69 138.55) (xy 224.69 137.75) (xy 227.29 137.75) (xy 227.29 139.35)
        (xy 226.49 140.15) (xy 226.49 141.25) (xy 226.19 141.55) (xy 224.49 141.55)
      )
    )
  )
  (zone (net 474) (net_name "/Stepper Drivers/H_B2") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.69 142.05) (xy 217.99 142.05) (xy 217.29 141.35) (xy 217.29 140.25) (xy 216.69 139.65)
        (xy 215.49 139.65) (xy 215.59 142.55) (xy 219.69 142.55)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.69 142.55) (xy 216.09 142.55) (xy 216.09 143.75) (xy 215.89 143.75) (xy 215.89 144.55)
        (xy 216.29 144.85) (xy 217.59 144.85) (xy 217.99 144.55) (xy 217.99 143.05) (xy 219.69 143.05)
      )
    )
  )
  (zone (net 475) (net_name "/Stepper Drivers/H_A1") (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 227.34 137.7) (xy 224.79 137.7) (xy 224.79 139.95) (xy 223.29 139.95) (xy 222.09 141.15)
        (xy 222.09 142.4) (xy 222.14 142.45) (xy 222.14 142.85) (xy 222.09 142.9) (xy 222.09 154.2)
        (xy 224.59 154.2) (xy 224.59 144.75) (xy 227.34 139.95)
      )
    )
  )
  (zone (net 463) (net_name "/Stepper Drivers/Z1_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 170.59 154.2) (xy 173.64 154.2) (xy 174.89 152.95) (xy 174.89 139.5) (xy 173.59 139.5)
        (xy 170.59 144.75)
      )
    )
  )
  (zone (net 476) (net_name "/Stepper Drivers/H_B1") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 219.49 138.05) (xy 218.04 136.6) (xy 213.49 136.6) (xy 212.49 137.6) (xy 212.49 150.2)
        (xy 216.49 154.2) (xy 219.54 154.2) (xy 219.54 152.15) (xy 219.39 152.15) (xy 219.39 144.85)
        (xy 216.84 142.2) (xy 215.29 142.2) (xy 215.29 139.4) (xy 216.99 139.4) (xy 217.54 139.95)
        (xy 219.49 139.95)
      )
    )
  )
  (zone (net 473) (net_name "/Stepper Drivers/H_A2") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 224.59 154.2) (xy 227.64 154.2) (xy 228.89 152.95) (xy 228.89 139.5) (xy 227.59 139.5)
        (xy 224.59 144.75)
      )
    )
  )
  (zone (net 478) (net_name "Net-(D15-Pad1)") (layer In3.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.401) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 75.9 143.2) (xy 75.9 142.2) (xy 76.9 141.2) (xy 77.15 140.2) (xy 77.15 138.95)
        (xy 83.4 138.95) (xy 85.4 141.45) (xy 85.4 148.2) (xy 76.65 148.2) (xy 76.65 143.95)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.372) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 84.4 140.2) (xy 85.4 140.2) (xy 85.4 134.7) (xy 68.4 134.7) (xy 68.4 140.45)
        (xy 72.65 140.45) (xy 73.4 139.2) (xy 77.15 139.2) (xy 77.15 138.95) (xy 83.4 138.95)
      )
    )
  )
  (zone (net 478) (net_name "Net-(D15-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.401) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 75.9 143.2) (xy 75.9 142.2) (xy 76.9 141.2) (xy 77.15 140.2) (xy 77.15 138.95)
        (xy 83.4 138.95) (xy 85.4 141.45) (xy 85.4 148.2) (xy 76.65 148.2) (xy 76.65 143.95)
      )
    )
  )
  (zone (net 478) (net_name "Net-(D15-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.401) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 75.9 143.2) (xy 75.9 142.2) (xy 76.9 141.2) (xy 77.15 140.2) (xy 77.15 138.95)
        (xy 83.4 138.95) (xy 85.4 141.45) (xy 85.4 148.2) (xy 76.65 148.2) (xy 76.65 143.95)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 84.15 134.7) (xy 85.4 134.7) (xy 85.4 140.2) (xy 84.4 140.2) (xy 83.4 138.95)
        (xy 77.15 138.95) (xy 77.15 139.2) (xy 73.4 139.2) (xy 72.65 140.45) (xy 68.4 140.45)
        (xy 68.4 134.7) (xy 77.65 134.7) (xy 77.65 115.5) (xy 84.15 115.5)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer In3.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 84.15 134.7) (xy 85.4 134.7) (xy 85.4 140.2) (xy 84.4 140.2) (xy 83.4 138.95)
        (xy 77.15 138.95) (xy 77.15 139.2) (xy 73.4 139.2) (xy 72.65 140.45) (xy 68.4 140.45)
        (xy 68.4 134.7) (xy 77.65 134.7) (xy 77.65 115.5) (xy 84.15 115.5)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 84.15 134.7) (xy 85.4 134.7) (xy 85.4 140.2) (xy 84.4 140.2) (xy 83.4 138.95)
        (xy 77.15 138.95) (xy 77.15 139.2) (xy 73.4 139.2) (xy 72.65 140.45) (xy 68.4 140.45)
        (xy 68.4 134.7) (xy 77.65 134.7) (xy 77.65 115.5) (xy 84.15 115.5)
      )
    )
  )
  (zone (net 505) (net_name "Net-(F2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 76.65 143.95) (xy 76.65 148.2) (xy 77.15 148.2) (xy 77.15 152.7) (xy 60.9 152.7)
        (xy 60.9 150.15) (xy 61.2 149.85) (xy 61.2 147.05) (xy 60.9 146.75) (xy 60.9 145.1)
        (xy 62.8 143.2) (xy 75.9 143.2)
      )
    )
  )
  (zone (net 505) (net_name "Net-(F2-Pad2)") (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 62.8 143.2) (xy 60.9 145.1) (xy 60.9 146.75) (xy 61.2 147.05) (xy 61.2 149.85)
        (xy 60.9 150.15) (xy 60.9 152.7) (xy 77.15 152.7) (xy 77.15 148.2) (xy 76.65 148.2)
        (xy 76.65 143.95) (xy 75.9 143.2)
      )
    )
  )
  (zone (net 505) (net_name "Net-(F2-Pad2)") (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 62.8 143.2) (xy 60.9 145.1) (xy 60.9 146.75) (xy 61.2 147.05) (xy 61.2 149.85)
        (xy 60.9 150.15) (xy 60.9 152.7) (xy 77.15 152.7) (xy 77.15 148.2) (xy 76.65 148.2)
        (xy 76.65 143.95) (xy 75.9 143.2)
      )
    )
  )
  (zone (net 478) (net_name "Net-(D15-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.401) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 75.9 143.2) (xy 75.9 142.2) (xy 76.9 141.2) (xy 77.15 140.2) (xy 77.15 138.95)
        (xy 83.4 138.95) (xy 85.4 141.45) (xy 85.4 148.2) (xy 76.65 148.2) (xy 76.65 143.95)
      )
    )
  )
  (zone (net 505) (net_name "Net-(F2-Pad2)") (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 62.8 143.2) (xy 60.9 145.1) (xy 60.9 146.75) (xy 61.2 147.05) (xy 61.2 149.85)
        (xy 60.9 150.15) (xy 60.9 152.7) (xy 77.15 152.7) (xy 77.15 148.2) (xy 76.65 148.2)
        (xy 76.65 143.95) (xy 75.9 143.2)
      )
    )
  )
  (zone (net 505) (net_name "Net-(F2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 62.8 143.2) (xy 60.9 145.1) (xy 60.9 146.75) (xy 61.2 147.05) (xy 61.2 149.85)
        (xy 60.9 150.15) (xy 60.9 152.7) (xy 77.15 152.7) (xy 77.15 148.2) (xy 76.65 148.2)
        (xy 76.65 143.95) (xy 75.9 143.2)
      )
    )
  )
  (zone (net 479) (net_name "Net-(D18-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 67.4 116.75) (xy 77.65 116.75) (xy 77.65 131.75) (xy 73.9 131.75) (xy 73.9 125.5)
        (xy 66.15 125.5) (xy 66.15 118) (xy 67.4 118)
      )
    )
  )
  (zone (net 479) (net_name "Net-(D18-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 118) (xy 67.4 118) (xy 67.4 116.75) (xy 77.65 116.75) (xy 77.65 125.5)
        (xy 66.15 125.5)
      )
    )
  )
  (zone (net 479) (net_name "Net-(D18-Pad1)") (layer In3.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 118) (xy 67.4 118) (xy 67.4 116.75) (xy 77.65 116.75) (xy 77.65 125.5)
        (xy 66.15 125.5)
      )
    )
  )
  (zone (net 479) (net_name "Net-(D18-Pad1)") (layer In4.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 118) (xy 67.4 118) (xy 67.4 116.75) (xy 77.65 116.75) (xy 77.65 125.5)
        (xy 66.15 125.5)
      )
    )
  )
  (zone (net 479) (net_name "Net-(D18-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 118) (xy 67.4 118) (xy 67.4 116.75) (xy 77.65 116.75) (xy 77.65 125.5)
        (xy 66.15 125.5)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 2))
    (polygon
      (pts
        (xy 67.4 116.75) (xy 67.4 118) (xy 66.15 118) (xy 66.15 115.5) (xy 83.65 115.5)
        (xy 84.15 115.5) (xy 84.15 122) (xy 77.65 122) (xy 77.65 116.75)
      )
    )
  )
  (zone (net 504) (net_name "Net-(F2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 68.4 140.7) (xy 55.3 140.7) (xy 55.3 130.7) (xy 68.4 130.7)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 245 161) (xy 53 161) (xy 53 24) (xy 245 24)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 245 161) (xy 53 161) (xy 53 24) (xy 245 24)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 245 161) (xy 53 161) (xy 53 24) (xy 245 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 118) (xy 55.15 118) (xy 55.15 123.75) (xy 54.15 123.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 118) (xy 55.15 118) (xy 55.15 123.75) (xy 54.15 123.75)
      )
    )
  )
  (zone (net 504) (net_name "Net-(F2-Pad1)") (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 68.4 140.7) (xy 53 140.7) (xy 53 130.7) (xy 68.4 130.7)
      )
    )
  )
  (zone (net 504) (net_name "Net-(F2-Pad1)") (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 68.4 140.7) (xy 55.3 140.7) (xy 55.3 130.7) (xy 68.4 130.7)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.7621))
    (polygon
      (pts
        (xy 245 161) (xy 53 161) (xy 53 24) (xy 245 24)
      )
    )
  )
  (zone (net 478) (net_name "Net-(D15-Pad1)") (layer In4.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.401) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 75.9 143.2) (xy 75.9 142.2) (xy 76.9 141.2) (xy 77.15 140.2) (xy 77.15 138.95)
        (xy 83.4 138.95) (xy 85.4 141.45) (xy 85.4 148.2) (xy 76.65 148.2) (xy 76.65 143.95)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.59 139.8) (xy 98.59 139.8) (xy 98.59 144.3) (xy 93.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.59 139.8) (xy 98.59 139.8) (xy 98.59 144.3) (xy 93.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.59 139.8) (xy 98.59 139.8) (xy 98.59 144.3) (xy 93.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.59 139.8) (xy 116.59 139.8) (xy 116.59 144.3) (xy 111.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.59 139.8) (xy 116.59 139.8) (xy 116.59 144.3) (xy 111.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.59 139.8) (xy 116.59 139.8) (xy 116.59 144.3) (xy 111.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.59 139.8) (xy 134.59 139.8) (xy 134.59 144.3) (xy 129.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.59 139.8) (xy 134.59 139.8) (xy 134.59 144.3) (xy 129.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.59 139.8) (xy 134.59 139.8) (xy 134.59 144.3) (xy 129.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.59 139.8) (xy 152.59 139.8) (xy 152.59 144.3) (xy 147.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.59 139.8) (xy 152.59 139.8) (xy 152.59 144.3) (xy 147.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.59 139.8) (xy 152.59 139.8) (xy 152.59 144.3) (xy 147.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.59 139.8) (xy 170.59 139.8) (xy 170.59 144.3) (xy 165.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.59 139.8) (xy 170.59 139.8) (xy 170.59 144.3) (xy 165.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.59 139.8) (xy 170.59 139.8) (xy 170.59 144.3) (xy 165.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.59 139.8) (xy 188.59 139.8) (xy 188.59 144.3) (xy 183.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.59 139.8) (xy 188.59 139.8) (xy 188.59 144.3) (xy 183.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.59 139.8) (xy 188.59 139.8) (xy 188.59 144.3) (xy 183.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.59 139.8) (xy 206.59 139.8) (xy 206.59 144.3) (xy 201.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.59 139.8) (xy 206.59 139.8) (xy 206.59 144.3) (xy 201.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.59 139.8) (xy 206.59 139.8) (xy 206.59 144.3) (xy 201.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.59 139.8) (xy 224.59 139.8) (xy 224.59 144.3) (xy 219.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.59 139.8) (xy 224.59 139.8) (xy 224.59 144.3) (xy 219.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.59 139.8) (xy 224.59 139.8) (xy 224.59 144.3) (xy 219.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.59 139.8) (xy 116.59 139.8) (xy 116.59 144.3) (xy 111.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.59 139.8) (xy 134.59 139.8) (xy 134.59 144.3) (xy 129.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.59 139.8) (xy 152.59 139.8) (xy 152.59 144.3) (xy 147.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.59 139.8) (xy 170.59 139.8) (xy 170.59 144.3) (xy 165.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.59 139.8) (xy 188.59 139.8) (xy 188.59 144.3) (xy 183.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.59 139.8) (xy 206.59 139.8) (xy 206.59 144.3) (xy 201.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.59 139.8) (xy 224.59 139.8) (xy 224.59 144.3) (xy 219.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.59 139.8) (xy 98.59 139.8) (xy 98.59 144.3) (xy 93.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 111.59 139.8) (xy 116.59 139.8) (xy 116.59 144.3) (xy 111.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 129.59 139.8) (xy 134.59 139.8) (xy 134.59 144.3) (xy 129.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 147.59 139.8) (xy 152.59 139.8) (xy 152.59 144.3) (xy 147.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 165.59 139.8) (xy 170.59 139.8) (xy 170.59 144.3) (xy 165.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 183.59 139.8) (xy 188.59 139.8) (xy 188.59 144.3) (xy 183.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 201.59 139.8) (xy 206.59 139.8) (xy 206.59 144.3) (xy 201.59 144.3)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 219.59 139.8) (xy 224.59 139.8) (xy 224.59 144.3) (xy 219.59 144.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 118) (xy 55.15 118) (xy 55.15 123.75) (xy 54.15 123.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 118) (xy 55.15 118) (xy 55.15 123.75) (xy 54.15 123.75)
      )
    )
  )
  (zone (net 22) (net_name /Heaters/BED_HEAT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 55.15 118.25) (xy 61.4 118.25) (xy 61.4 116) (xy 66.15 116) (xy 66.15 125)
        (xy 61.4 125) (xy 61.4 123.5) (xy 55.15 123.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 118) (xy 55.15 118) (xy 55.15 123.75) (xy 54.15 123.75)
      )
    )
  )
  (zone (net 22) (net_name /Heaters/BED_HEAT) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 123.5) (xy 55.15 123.5) (xy 55.15 118.25) (xy 66.15 118.25)
      )
    )
  )
  (zone (net 22) (net_name /Heaters/BED_HEAT) (layer In3.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 123.5) (xy 55.15 123.5) (xy 55.15 118.25) (xy 66.15 118.25)
      )
    )
  )
  (zone (net 22) (net_name /Heaters/BED_HEAT) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 123.5) (xy 55.15 123.5) (xy 55.15 118.25) (xy 66.15 118.25)
      )
    )
  )
  (zone (net 22) (net_name /Heaters/BED_HEAT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.15 123.5) (xy 55.15 123.5) (xy 55.15 118.25) (xy 66.15 118.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 61.15 115.75) (xy 66.05 115.75) (xy 66.05 118.25) (xy 61.15 118.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 61.15 115.75) (xy 66.05 115.75) (xy 66.05 118.25) (xy 61.15 118.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 61.15 115.75) (xy 66.05 115.75) (xy 66.05 118.25) (xy 61.15 118.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 118) (xy 61.15 118) (xy 61.15 115.75) (xy 66.05 115.75) (xy 66.05 125.3)
        (xy 61.15 125.3) (xy 61.15 123.75) (xy 53 123.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 61.15 123.75) (xy 66.05 123.75) (xy 66.05 125.3) (xy 61.15 125.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 61.15 123.75) (xy 66.05 123.75) (xy 66.05 125.3) (xy 61.15 125.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 61.15 123.75) (xy 66.05 123.75) (xy 66.05 125.3) (xy 61.15 125.3)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch full 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 72.5 108) (xy 71.9 108.6) (xy 71.9 110.2) (xy 72.2 110.5) (xy 73.6 110.5)
        (xy 74.8 109.3) (xy 75.3 109.3) (xy 75.3 108.3) (xy 75.7 108.3) (xy 75.7 107.6)
        (xy 75.3 107.6) (xy 75.3 107.4) (xy 74.4 107.4) (xy 74.4 108) (xy 73.3 108)
        (xy 73.3 106.9) (xy 77.5 106.9) (xy 77.5 104.1) (xy 66.95 104.1) (xy 66.95 105.8)
        (xy 72.5 105.8)
      )
    )
  )
  (zone (net 480) (net_name "Net-(D20-Pad1)") (layer F.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.5 105.8) (xy 72.5 105.8) (xy 72.5 108) (xy 71.9 108.6) (xy 71.9 110.2)
        (xy 71.6 110.2) (xy 71.6 112) (xy 71.7 112) (xy 71.7 113.4) (xy 66.5 113.4)
      )
    )
  )
  (zone (net 649) (net_name "Net-(C7-Pad1)") (layer F.Cu) (hatch full 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 116.4 107.85) (xy 115.3 107.85) (xy 115.3 121.6) (xy 121.05 121.6) (xy 121.15 121.6)
        (xy 121.15 119.225) (xy 126.15 119.225) (xy 126.15 110.2) (xy 121.475 110.2) (xy 121.475 115.25)
        (xy 119.525 117.2) (xy 117.6 117.2) (xy 116.4 116)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.9 115.55) (xy 67.4 115.55) (xy 67.4 118) (xy 66.15 118) (xy 66.15 118.25)
        (xy 60.9 118.25)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch full 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 72.5 95.67) (xy 71.9 96.27) (xy 71.9 97.87) (xy 72.2 98.17) (xy 73.6 98.17)
        (xy 74.8 96.97) (xy 75.3 96.97) (xy 75.3 95.97) (xy 75.7 95.97) (xy 75.7 95.27)
        (xy 75.3 95.27) (xy 75.3 95.07) (xy 74.4 95.07) (xy 74.4 95.67) (xy 73.3 95.67)
        (xy 73.3 94.57) (xy 77.5 94.57) (xy 77.5 91.77) (xy 66.95 91.77) (xy 66.95 93.47)
        (xy 72.5 93.47)
      )
    )
  )
  (zone (net 537) (net_name "Net-(D24-Pad1)") (layer F.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.5 93.47) (xy 72.5 93.47) (xy 72.5 95.67) (xy 71.9 96.27) (xy 71.9 97.87)
        (xy 71.6 97.87) (xy 71.6 99.67) (xy 71.7 99.67) (xy 71.7 101.07) (xy 66.5 101.07)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch full 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 72.5 83.34) (xy 71.9 83.94) (xy 71.9 85.54) (xy 72.2 85.84) (xy 73.6 85.84)
        (xy 74.8 84.64) (xy 75.3 84.64) (xy 75.3 83.64) (xy 75.7 83.64) (xy 75.7 82.94)
        (xy 75.3 82.94) (xy 75.3 82.74) (xy 74.4 82.74) (xy 74.4 83.34) (xy 73.3 83.34)
        (xy 73.3 82.24) (xy 77.5 82.24) (xy 77.5 79.44) (xy 66.95 79.44) (xy 66.95 81.14)
        (xy 72.5 81.14)
      )
    )
  )
  (zone (net 536) (net_name "Net-(D21-Pad1)") (layer F.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.5 81.14) (xy 72.5 81.14) (xy 72.5 83.34) (xy 71.9 83.94) (xy 71.9 85.54)
        (xy 71.6 85.54) (xy 71.6 87.34) (xy 71.7 87.34) (xy 71.7 88.74) (xy 66.5 88.74)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer F.Cu) (hatch full 0.508)
    (priority 3)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 72.5 71.01) (xy 71.9 71.61) (xy 71.9 73.21) (xy 72.2 73.51) (xy 73.6 73.51)
        (xy 74.8 72.31) (xy 75.3 72.31) (xy 75.3 71.31) (xy 75.7 71.31) (xy 75.7 70.61)
        (xy 75.3 70.61) (xy 75.3 70.41) (xy 74.4 70.41) (xy 74.4 71.01) (xy 73.3 71.01)
        (xy 73.3 69.91) (xy 77.5 69.91) (xy 77.5 67.11) (xy 66.95 67.11) (xy 66.95 68.81)
        (xy 72.5 68.81)
      )
    )
  )
  (zone (net 538) (net_name "Net-(D25-Pad1)") (layer F.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.5 68.81) (xy 72.5 68.81) (xy 72.5 71.01) (xy 71.9 71.61) (xy 71.9 73.21)
        (xy 71.6 73.21) (xy 71.6 75.01) (xy 71.7 75.01) (xy 71.7 76.41) (xy 66.5 76.41)
      )
    )
  )
  (zone (net 4) (net_name +24V) (layer In4.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 77.65 105.85) (xy 84.15 112.35) (xy 84.15 122.1) (xy 91.3 122.1) (xy 100.4 113)
        (xy 100.4 107.5) (xy 108.4 107.5) (xy 108.4 113) (xy 92 131.5) (xy 92 142.5)
        (xy 104 142.5) (xy 104 131.5) (xy 110 131.5) (xy 110 142.5) (xy 122 142.5)
        (xy 122 131.5) (xy 128 131.5) (xy 128 142.5) (xy 140 142.5) (xy 140 131.5)
        (xy 146 131.5) (xy 146 142.5) (xy 158 142.5) (xy 158 131.5) (xy 164 131.5)
        (xy 164 142.5) (xy 176 142.5) (xy 176 131.5) (xy 182 131.5) (xy 182 142.5)
        (xy 194 142.5) (xy 194 131.5) (xy 200 131.5) (xy 200 142.5) (xy 212 142.5)
        (xy 212 131.5) (xy 218 131.5) (xy 218 142.5) (xy 227.25 142.5) (xy 227.25 148)
        (xy 85.4 148) (xy 85.4 141.45) (xy 83.4 138.95) (xy 77.15 138.95) (xy 77.15 139.2)
        (xy 73.4 139.2) (xy 72.65 140.45) (xy 68.4 140.45) (xy 68.4 134.7) (xy 77.65 134.7)
        (xy 77.65 116.75) (xy 70.65 116.75) (xy 70.65 69) (xy 77.65 69)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 40.5) (xy 53 40.5) (xy 53 43.05) (xy 62.5 43.05) (xy 62.5 42.23)
        (xy 63.75 42.23) (xy 63.75 44.25) (xy 65.5 44.25) (xy 65.5 39) (xy 63.75 39)
        (xy 63.75 41.37) (xy 62.5 41.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 40.5) (xy 53 40.5) (xy 53 43.05) (xy 62.5 43.05) (xy 62.5 42.23)
        (xy 63.75 42.23) (xy 63.75 44.25) (xy 65.5 44.25) (xy 65.5 39) (xy 63.75 39)
        (xy 63.75 41.37) (xy 62.5 41.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 40.5) (xy 53 40.5) (xy 53 43.05) (xy 62.5 43.05) (xy 62.5 42.23)
        (xy 63.75 42.23) (xy 63.75 44.25) (xy 65.5 44.25) (xy 65.5 39) (xy 63.75 39)
        (xy 63.75 41.37) (xy 62.5 41.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 40.5) (xy 53 40.5) (xy 53 43.05) (xy 62.5 43.05) (xy 62.5 42.23)
        (xy 63.75 42.23) (xy 63.75 44.25) (xy 65.5 44.25) (xy 65.5 39) (xy 63.75 39)
        (xy 63.75 41.37) (xy 62.5 41.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 40.5) (xy 53 40.5) (xy 53 43.05) (xy 62.5 43.05) (xy 62.5 42.23)
        (xy 63.75 42.23) (xy 63.75 44.25) (xy 65.5 44.25) (xy 65.5 39) (xy 63.75 39)
        (xy 63.75 41.37) (xy 62.5 41.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 63.75 41.37) (xy 62.5 41.37) (xy 62.5 40.5) (xy 53 40.5) (xy 53 43)
        (xy 53 43.05) (xy 62.5 43.05) (xy 62.5 42.23) (xy 63.75 42.23) (xy 63.75 44.25)
        (xy 65.5 44.25) (xy 65.5 39) (xy 63.75 39)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 49.5) (xy 53 49.5) (xy 53 52.05) (xy 62.5 52.05) (xy 62.5 51.23)
        (xy 63.75 51.23) (xy 63.75 53.25) (xy 65.5 53.25) (xy 65.5 48) (xy 63.75 48)
        (xy 63.75 50.37) (xy 62.5 50.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 49.5) (xy 53 49.5) (xy 53 52.05) (xy 62.5 52.05) (xy 62.5 51.23)
        (xy 63.75 51.23) (xy 63.75 53.25) (xy 65.5 53.25) (xy 65.5 48) (xy 63.75 48)
        (xy 63.75 50.37) (xy 62.5 50.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 49.5) (xy 53 49.5) (xy 53 52.05) (xy 62.5 52.05) (xy 62.5 51.23)
        (xy 63.75 51.23) (xy 63.75 53.25) (xy 65.5 53.25) (xy 65.5 48) (xy 63.75 48)
        (xy 63.75 50.37) (xy 62.5 50.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 63.75 50.37) (xy 62.5 50.37) (xy 62.5 49.5) (xy 53 49.5) (xy 53 52)
        (xy 53 52.05) (xy 62.5 52.05) (xy 62.5 51.23) (xy 63.75 51.23) (xy 63.75 53.25)
        (xy 65.5 53.25) (xy 65.5 48) (xy 63.75 48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 49.5) (xy 53 49.5) (xy 53 52.05) (xy 62.5 52.05) (xy 62.5 51.23)
        (xy 63.75 51.23) (xy 63.75 53.25) (xy 65.5 53.25) (xy 65.5 48) (xy 63.75 48)
        (xy 63.75 50.37) (xy 62.5 50.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 49.5) (xy 53 49.5) (xy 53 52.05) (xy 62.5 52.05) (xy 62.5 51.23)
        (xy 63.75 51.23) (xy 63.75 53.25) (xy 65.5 53.25) (xy 65.5 48) (xy 63.75 48)
        (xy 63.75 50.37) (xy 62.5 50.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 58.5) (xy 53 58.5) (xy 53 61.05) (xy 62.5 61.05) (xy 62.5 60.23)
        (xy 63.75 60.23) (xy 63.75 62.25) (xy 65.5 62.25) (xy 65.5 57) (xy 63.75 57)
        (xy 63.75 59.37) (xy 62.5 59.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 58.5) (xy 53 58.5) (xy 53 61.05) (xy 62.5 61.05) (xy 62.5 60.23)
        (xy 63.75 60.23) (xy 63.75 62.25) (xy 65.5 62.25) (xy 65.5 57) (xy 63.75 57)
        (xy 63.75 59.37) (xy 62.5 59.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 58.5) (xy 53 58.5) (xy 53 61.05) (xy 62.5 61.05) (xy 62.5 60.23)
        (xy 63.75 60.23) (xy 63.75 62.25) (xy 65.5 62.25) (xy 65.5 57) (xy 63.75 57)
        (xy 63.75 59.37) (xy 62.5 59.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 58.5) (xy 53 58.5) (xy 53 61.05) (xy 62.5 61.05) (xy 62.5 60.23)
        (xy 63.75 60.23) (xy 63.75 62.25) (xy 65.5 62.25) (xy 65.5 57) (xy 63.75 57)
        (xy 63.75 59.37) (xy 62.5 59.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 62.5 58.5) (xy 53 58.5) (xy 53 61.05) (xy 62.5 61.05) (xy 62.5 60.23)
        (xy 63.75 60.23) (xy 63.75 62.25) (xy 65.5 62.25) (xy 65.5 57) (xy 63.75 57)
        (xy 63.75 59.37) (xy 62.5 59.37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 63.75 59.37) (xy 62.5 59.37) (xy 62.5 58.5) (xy 53 58.5) (xy 53 61)
        (xy 53 61.05) (xy 62.5 61.05) (xy 62.5 60.23) (xy 63.75 60.23) (xy 63.75 62.25)
        (xy 65.5 62.25) (xy 65.5 57) (xy 63.75 57)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 105.67) (xy 61.15 105.67) (xy 61.15 104.32) (xy 66.4 104.32) (xy 66.4 112.82)
        (xy 61.15 112.82) (xy 61.15 111.42) (xy 53 111.42)
      )
    )
  )
  (zone (net 23) (net_name /Heaters/E_HEAT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 55.15 105.92) (xy 61.4 105.92) (xy 61.4 104.57) (xy 66.5 104.57) (xy 66.5 112.52)
        (xy 61.4 112.52) (xy 61.4 111.17) (xy 55.15 111.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.1 104.32) (xy 66.1 105.8) (xy 66.4 105.8) (xy 66.4 104.32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 105.67) (xy 55.15 105.67) (xy 55.15 111.42) (xy 54.15 111.42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 105.67) (xy 61.15 105.67) (xy 61.15 104.32) (xy 66.4 104.32) (xy 66.4 112.82)
        (xy 61.15 112.82) (xy 61.15 111.42) (xy 53 111.42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 105.67) (xy 61.15 105.67) (xy 61.15 104.32) (xy 66.4 104.32) (xy 66.4 112.82)
        (xy 61.15 112.82) (xy 61.15 111.42) (xy 53 111.42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 105.67) (xy 61.15 105.67) (xy 61.15 104.32) (xy 66.4 104.32) (xy 66.4 112.82)
        (xy 61.15 112.82) (xy 61.15 111.42) (xy 53 111.42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 105.67) (xy 61.15 105.67) (xy 61.15 104.32) (xy 66.4 104.32) (xy 66.4 112.82)
        (xy 61.15 112.82) (xy 61.15 111.42) (xy 53 111.42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 105.67) (xy 61.15 105.67) (xy 61.15 104.32) (xy 66.4 104.32) (xy 66.4 112.82)
        (xy 61.15 112.82) (xy 61.15 111.42) (xy 53 111.42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 93.34) (xy 61.15 93.34) (xy 61.15 91.99) (xy 66.4 91.99) (xy 66.4 100.49)
        (xy 61.15 100.49) (xy 61.15 99.09) (xy 53 99.09)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 93.34) (xy 61.15 93.34) (xy 61.15 91.99) (xy 66.4 91.99) (xy 66.4 100.49)
        (xy 61.15 100.49) (xy 61.15 99.09) (xy 53 99.09)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.1 91.99) (xy 66.1 93.47) (xy 66.4 93.47) (xy 66.4 91.99)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 93.34) (xy 61.15 93.34) (xy 61.15 91.99) (xy 66.4 91.99) (xy 66.4 100.49)
        (xy 61.15 100.49) (xy 61.15 99.09) (xy 53 99.09)
      )
    )
  )
  (zone (net 25) (net_name /Heaters/H_HEAT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 55.15 93.59) (xy 61.4 93.59) (xy 61.4 92.24) (xy 66.5 92.24) (xy 66.5 100.19)
        (xy 61.4 100.19) (xy 61.4 98.84) (xy 55.15 98.84)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 93.34) (xy 61.15 93.34) (xy 61.15 91.99) (xy 66.4 91.99) (xy 66.4 100.49)
        (xy 61.15 100.49) (xy 61.15 99.09) (xy 53 99.09)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 93.34) (xy 61.15 93.34) (xy 61.15 91.99) (xy 66.4 91.99) (xy 66.4 100.49)
        (xy 61.15 100.49) (xy 61.15 99.09) (xy 53 99.09)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 93.34) (xy 61.15 93.34) (xy 61.15 91.99) (xy 66.4 91.99) (xy 66.4 100.49)
        (xy 61.15 100.49) (xy 61.15 99.09) (xy 53 99.09)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 81.01) (xy 61.15 81.01) (xy 61.15 79.66) (xy 66.4 79.66) (xy 66.4 88.16)
        (xy 61.15 88.16) (xy 61.15 86.76) (xy 53 86.76)
      )
    )
  )
  (zone (net 24) (net_name /Heaters/DOCK0_HEAT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 55.15 81.26) (xy 61.4 81.26) (xy 61.4 79.91) (xy 66.5 79.91) (xy 66.5 87.86)
        (xy 61.4 87.86) (xy 61.4 86.51) (xy 55.15 86.51)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 81.01) (xy 61.15 81.01) (xy 61.15 79.66) (xy 66.4 79.66) (xy 66.4 88.16)
        (xy 61.15 88.16) (xy 61.15 86.76) (xy 53 86.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.1 79.66) (xy 66.1 81.14) (xy 66.4 81.14) (xy 66.4 79.66)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 81.01) (xy 61.15 81.01) (xy 61.15 79.66) (xy 66.4 79.66) (xy 66.4 88.16)
        (xy 61.15 88.16) (xy 61.15 86.76) (xy 53 86.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 81.01) (xy 61.15 81.01) (xy 61.15 79.66) (xy 66.4 79.66) (xy 66.4 88.16)
        (xy 61.15 88.16) (xy 61.15 86.76) (xy 53 86.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 81.01) (xy 61.15 81.01) (xy 61.15 79.66) (xy 66.4 79.66) (xy 66.4 88.16)
        (xy 61.15 88.16) (xy 61.15 86.76) (xy 53 86.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 81.01) (xy 61.15 81.01) (xy 61.15 79.66) (xy 66.4 79.66) (xy 66.4 88.16)
        (xy 61.15 88.16) (xy 61.15 86.76) (xy 53 86.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 66.1 67.33) (xy 66.1 68.81) (xy 66.4 68.81) (xy 66.4 67.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 68.68) (xy 61.15 68.68) (xy 61.15 67.33) (xy 66.4 67.33) (xy 66.4 75.83)
        (xy 61.15 75.83) (xy 61.15 74.43) (xy 53 74.43)
      )
    )
  )
  (zone (net 26) (net_name /Heaters/DOCK1_HEAT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 55.15 68.93) (xy 61.4 68.93) (xy 61.4 67.58) (xy 66.5 67.58) (xy 66.5 75.53)
        (xy 61.4 75.53) (xy 61.4 74.18) (xy 55.15 74.18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 68.68) (xy 61.15 68.68) (xy 61.15 67.33) (xy 66.4 67.33) (xy 66.4 75.83)
        (xy 61.15 75.83) (xy 61.15 74.43) (xy 53 74.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 68.68) (xy 61.15 68.68) (xy 61.15 67.33) (xy 66.4 67.33) (xy 66.4 75.83)
        (xy 61.15 75.83) (xy 61.15 74.43) (xy 53 74.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 68.68) (xy 61.15 68.68) (xy 61.15 67.33) (xy 66.4 67.33) (xy 66.4 75.83)
        (xy 61.15 75.83) (xy 61.15 74.43) (xy 53 74.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 68.68) (xy 61.15 68.68) (xy 61.15 67.33) (xy 66.4 67.33) (xy 66.4 75.83)
        (xy 61.15 75.83) (xy 61.15 74.43) (xy 53 74.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 53 68.68) (xy 61.15 68.68) (xy 61.15 67.33) (xy 66.4 67.33) (xy 66.4 75.83)
        (xy 61.15 75.83) (xy 61.15 74.43) (xy 53 74.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 93.34) (xy 55.15 93.34) (xy 55.15 99.09) (xy 54.15 99.09)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 81.01) (xy 55.15 81.01) (xy 55.15 86.76) (xy 54.15 86.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.203))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 3.5))
    (polygon
      (pts
        (xy 54.15 68.68) (xy 55.15 68.68) (xy 55.15 74.43) (xy 54.15 74.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.1 24) (xy 66.1 35.9) (xy 81.2 35.9) (xy 81.2 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.1 24) (xy 66.1 35.9) (xy 81.2 35.9) (xy 81.2 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.1 24) (xy 66.1 35.9) (xy 81.2 35.9) (xy 81.2 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.1 24) (xy 66.1 35.9) (xy 81.2 35.9) (xy 81.2 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.1 24) (xy 66.1 35.9) (xy 81.2 35.9) (xy 81.2 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.1 24) (xy 66.1 35.9) (xy 81.2 35.9) (xy 81.2 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 24) (xy 87 35.9) (xy 104.6 35.9) (xy 104.6 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 24) (xy 87 35.9) (xy 104.6 35.9) (xy 104.6 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 24) (xy 87 35.9) (xy 104.6 35.9) (xy 104.6 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 24) (xy 87 35.9) (xy 104.6 35.9) (xy 104.6 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 24) (xy 87 35.9) (xy 104.6 35.9) (xy 104.6 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 24) (xy 87 35.9) (xy 104.6 35.9) (xy 104.6 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.4 24) (xy 110.4 35.9) (xy 128 35.9) (xy 128 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.4 24) (xy 110.4 35.9) (xy 128 35.9) (xy 128 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.4 24) (xy 110.4 35.9) (xy 128 35.9) (xy 128 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.4 24) (xy 110.4 35.9) (xy 128 35.9) (xy 128 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.4 24) (xy 110.4 35.9) (xy 128 35.9) (xy 128 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.4 24) (xy 110.4 35.9) (xy 128 35.9) (xy 128 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8 24) (xy 133.8 35.9) (xy 151.4 35.9) (xy 151.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8 24) (xy 133.8 35.9) (xy 151.4 35.9) (xy 151.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8 24) (xy 133.8 35.9) (xy 151.4 35.9) (xy 151.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8 24) (xy 133.8 35.9) (xy 151.4 35.9) (xy 151.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8 24) (xy 133.8 35.9) (xy 151.4 35.9) (xy 151.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8 24) (xy 133.8 35.9) (xy 151.4 35.9) (xy 151.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.2 24) (xy 157.2 35.9) (xy 174.8 35.9) (xy 174.8 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.2 24) (xy 157.2 35.9) (xy 174.8 35.9) (xy 174.8 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.2 24) (xy 157.2 35.9) (xy 174.8 35.9) (xy 174.8 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.2 24) (xy 157.2 35.9) (xy 174.8 35.9) (xy 174.8 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.2 24) (xy 157.2 35.9) (xy 174.8 35.9) (xy 174.8 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.2 24) (xy 157.2 35.9) (xy 174.8 35.9) (xy 174.8 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.4 24) (xy 199.4 35.9) (xy 201.9 35.9) (xy 201.9 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.4 24) (xy 199.4 35.9) (xy 201.9 35.9) (xy 201.9 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.4 24) (xy 199.4 35.9) (xy 201.9 35.9) (xy 201.9 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.4 24) (xy 199.4 35.9) (xy 201.9 35.9) (xy 201.9 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.4 24) (xy 199.4 35.9) (xy 201.9 35.9) (xy 201.9 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.4 24) (xy 199.4 35.9) (xy 201.9 35.9) (xy 201.9 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.72 24) (xy 215.72 35.9) (xy 218.22 35.9) (xy 218.22 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.72 24) (xy 215.72 35.9) (xy 218.22 35.9) (xy 218.22 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.72 24) (xy 215.72 35.9) (xy 218.22 35.9) (xy 218.22 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.72 24) (xy 215.72 35.9) (xy 218.22 35.9) (xy 218.22 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.72 24) (xy 215.72 35.9) (xy 218.22 35.9) (xy 218.22 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.72 24) (xy 215.72 35.9) (xy 218.22 35.9) (xy 218.22 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.88 24) (xy 223.88 35.9) (xy 226.38 35.9) (xy 226.38 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.88 24) (xy 223.88 35.9) (xy 226.38 35.9) (xy 226.38 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.88 24) (xy 223.88 35.9) (xy 226.38 35.9) (xy 226.38 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.88 24) (xy 223.88 35.9) (xy 226.38 35.9) (xy 226.38 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.88 24) (xy 223.88 35.9) (xy 226.38 35.9) (xy 226.38 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.88 24) (xy 223.88 35.9) (xy 226.38 35.9) (xy 226.38 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.04 24) (xy 232.04 35.9) (xy 234.54 35.9) (xy 234.54 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.04 24) (xy 232.04 35.9) (xy 234.54 35.9) (xy 234.54 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.04 24) (xy 232.04 35.9) (xy 234.54 35.9) (xy 234.54 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.04 24) (xy 232.04 35.9) (xy 234.54 35.9) (xy 234.54 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.04 24) (xy 232.04 35.9) (xy 234.54 35.9) (xy 234.54 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.04 24) (xy 232.04 35.9) (xy 234.54 35.9) (xy 234.54 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.6 24) (xy 180.6 36.1) (xy 185.4 36.1) (xy 185.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.6 24) (xy 180.6 36.1) (xy 185.4 36.1) (xy 185.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.6 24) (xy 180.6 36.1) (xy 185.4 36.1) (xy 185.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.6 24) (xy 180.6 36.1) (xy 185.4 36.1) (xy 185.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.6 24) (xy 180.6 36.1) (xy 185.4 36.1) (xy 185.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.6 24) (xy 180.6 36.1) (xy 185.4 36.1) (xy 185.4 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.24 24) (xy 191.24 35.9) (xy 193.74 35.9) (xy 193.74 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.24 24) (xy 191.24 35.9) (xy 193.74 35.9) (xy 193.74 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.24 24) (xy 191.24 35.9) (xy 193.74 35.9) (xy 193.74 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.24 24) (xy 191.24 35.9) (xy 193.74 35.9) (xy 193.74 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.24 24) (xy 191.24 35.9) (xy 193.74 35.9) (xy 193.74 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.24 24) (xy 191.24 35.9) (xy 193.74 35.9) (xy 193.74 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.5 24) (xy 207.5 35.9) (xy 211.6 35.9) (xy 211.6 34.5) (xy 210.1 33)
        (xy 210.1 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.5 24) (xy 207.5 35.9) (xy 211.6 35.9) (xy 211.6 34.5) (xy 210.1 33)
        (xy 210.1 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.5 24) (xy 207.5 35.9) (xy 211.6 35.9) (xy 211.6 34.5) (xy 210.1 33)
        (xy 210.1 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.5 24) (xy 207.5 35.9) (xy 211.6 35.9) (xy 211.6 34.5) (xy 210.1 33)
        (xy 210.1 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.5 24) (xy 207.5 35.9) (xy 211.6 35.9) (xy 211.6 34.5) (xy 210.1 33)
        (xy 210.1 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.5 24) (xy 207.5 35.9) (xy 211.6 35.9) (xy 211.6 34.5) (xy 210.1 33)
        (xy 210.1 24)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 162.5 106) (xy 162.5 79) (xy 135.5 79) (xy 135.5 106)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 93.59 139.8) (xy 98.59 139.8) (xy 98.59 144.3) (xy 93.59 144.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.8 109.1) (xy 155.8 109) (xy 155.9 109) (xy 155.9 109.1)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 162.5 106) (xy 162.5 79) (xy 135.5 79) (xy 135.5 106)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.8 112.5) (xy 154.2 112.5) (xy 154.2 113.2) (xy 154.8 113.2)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 152 110) (xy 152 116) (xy 156 116) (xy 156 110)
      )
    )
  )
  (zone (net 648) (net_name "Net-(C5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.335) (thermal_bridge_width 0.7621))
    (polygon
      (pts
        (xy 141.8 103.825) (xy 141.8 105.8) (xy 141.55 105.8) (xy 141.55 107.63) (xy 143.8 107.63)
        (xy 143.8 105.8) (xy 143.5 105.8) (xy 143.5 103.825)
      )
    )
  )
  (zone (net 521) (net_name VDD_5V) (layer In4.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.7621))
    (polygon
      (pts
        (xy 126.2 104.6) (xy 126.2 108.2) (xy 128.9 108.2) (xy 128.9 104.6)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 160.9 100) (xy 160.9 102.8) (xy 162.5 102.8) (xy 162.5 100)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer In4.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.7621))
    (polygon
      (pts
        (xy 245 161) (xy 53 161) (xy 53 24) (xy 245 24)
      )
    )
  )
  (zone (net 1) (net_name CGND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.7621))
    (polygon
      (pts
        (xy 245 161) (xy 53 161) (xy 53 24) (xy 245 24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In4.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.75 103.775) (xy 141.75 105.75) (xy 141.5 105.75) (xy 141.5 107.75) (xy 143.9 107.75)
        (xy 143.875 105.75) (xy 143.55 105.75) (xy 143.55 103.775)
      )
    )
  )
)
