(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 64)
    (no_connects 0)
    (area 89.942857 50.325 197.057143 140.500001)
    (thickness 1.6)
    (drawings 7)
    (tracks 168)
    (zones 0)
    (modules 28)
    (nets 43)
  )
  (page A4)
  (title_block
    (title GLCD)
    (date 2016-09-30)
    (rev 0.7)
    (company "Aleph Objects Inc.")
    (comment 1 "GNU GPLv2, Copyright 2016")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.6576 2.032)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 VCC)
  (net 4 /SD_DET)
  (net 5 "Net-(DS1-Pad7)")
  (net 6 "Net-(DS1-Pad8)")
  (net 7 "Net-(DS1-Pad9)")
  (net 8 "Net-(DS1-Pad10)")
  (net 9 "Net-(DS1-Pad11)")
  (net 10 "Net-(DS1-Pad12)")
  (net 11 "Net-(DS1-Pad13)")
  (net 12 "Net-(DS1-Pad14)")
  (net 13 "Net-(DS1-Pad19)")
  (net 14 /BTN_EN1)
  (net 15 /BTN_EN2)
  (net 16 /BTN_ENC)
  (net 17 "Net-(IC1-Pad16)")
  (net 18 "Net-(IC1-Pad13)")
  (net 19 "Net-(IC1-Pad6)")
  (net 20 "Net-(IC1-Pad4)")
  (net 21 "Net-(IC1-Pad2)")
  (net 22 /Beeper)
  (net 23 "Net-(Q1-Pad1)")
  (net 24 "Net-(Q1-Pad3)")
  (net 25 "Net-(IC1-Pad12)")
  (net 26 "Net-(IC1-Pad10)")
  (net 27 "Net-(IC1-Pad15)")
  (net 28 "Net-(SD1-Pad8)")
  (net 29 "Net-(SD1-Pad9)")
  (net 30 "Net-(SD1-Pad11)")
  (net 31 /MISO)
  (net 32 /SCK)
  (net 33 /SS)
  (net 34 /MOSI)
  (net 35 "/LCDRS(CS)")
  (net 36 "/LCDRW(SID)")
  (net 37 "/LCDE(SCLK)")
  (net 38 "Net-(EXP1-Pad3)")
  (net 39 "Net-(EXP1-Pad4)")
  (net 40 "Net-(EXP1-Pad5)")
  (net 41 "Net-(EXP2-Pad1)")
  (net 42 "Net-(EXP2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /BTN_EN1)
    (add_net /BTN_EN2)
    (add_net /BTN_ENC)
    (add_net /Beeper)
    (add_net "/LCDE(SCLK)")
    (add_net "/LCDRS(CS)")
    (add_net "/LCDRW(SID)")
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /SD_DET)
    (add_net /SS)
    (add_net "Net-(DS1-Pad10)")
    (add_net "Net-(DS1-Pad11)")
    (add_net "Net-(DS1-Pad12)")
    (add_net "Net-(DS1-Pad13)")
    (add_net "Net-(DS1-Pad14)")
    (add_net "Net-(DS1-Pad19)")
    (add_net "Net-(DS1-Pad7)")
    (add_net "Net-(DS1-Pad8)")
    (add_net "Net-(DS1-Pad9)")
    (add_net "Net-(EXP1-Pad3)")
    (add_net "Net-(EXP1-Pad4)")
    (add_net "Net-(EXP1-Pad5)")
    (add_net "Net-(EXP2-Pad1)")
    (add_net "Net-(EXP2-Pad3)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(SD1-Pad11)")
    (add_net "Net-(SD1-Pad8)")
    (add_net "Net-(SD1-Pad9)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net VCC)
  )
  (module GLCD:Rotary_Encoder locked (layer F.Cu) (tedit 580550B3)
    (at 180 132.5)
    (fp_text reference EN1 (at 0.135 -1) (layer F.SilkS))
    (fp_text value EC11E15244B2 (at -0.5 -8.62) (layer F.Fab))
    (pad 1 thru_hole circle (at -7.5 -3.5) (size 1.25 1.25) (drill 1) (layers *.Cu *.Mask)
      (net 14 /BTN_EN1) (solder_mask_margin 0.1))
    (pad 2 thru_hole circle (at -7.5 -1) (size 1.25 1.25) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1))
    (pad 3 thru_hole circle (at -7.5 1.5) (size 1.25 1.25) (drill 1) (layers *.Cu *.Mask)
      (net 15 /BTN_EN2) (solder_mask_margin 0.1))
    (pad 6 thru_hole circle (at 0 -6.5) (size 3.375 3.375) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1))
    (pad 7 thru_hole circle (at 0 4.5) (size 3.375 3.375) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1))
    (pad 4 thru_hole circle (at 7 1.5) (size 1.25 1.25) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1))
    (pad 5 thru_hole circle (at 7 -3.5) (size 1.25 1.25) (drill 1) (layers *.Cu *.Mask)
      (net 16 /BTN_ENC) (solder_mask_margin 0.1))
  )
  (module GLCD:Bumper locked (layer F.Cu) (tedit 57EED6F5)
    (at 109.5 101.5)
    (fp_text reference REF** (at 0 13) (layer F.SilkS) hide)
    (fp_text value Bumper (at 0 -5.5) (layer F.Fab))
  )
  (module GLCD:Bumper locked (layer F.Cu) (tedit 57EED6EA)
    (at 177.5 101.5)
    (fp_text reference REF** (at 0 13) (layer F.SilkS) hide)
    (fp_text value Bumper (at 0 -5.5) (layer F.Fab))
  )
  (module GLCD:Bumper locked (layer F.Cu) (tedit 57EED6DA)
    (at 143.5 71.5)
    (fp_text reference REF** (at 0 13) (layer F.SilkS) hide)
    (fp_text value Bumper (at 0 -5.5) (layer F.Fab))
  )
  (module GLCD:SOT-666 locked (layer B.Cu) (tedit 580550B3)
    (at 151.638 116.586 180)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference Z1 (at 0 2 180) (layer B.SilkS))
    (fp_text value ZENER_4_CHANNEL (at 0 -2 180) (layer F.Fab))
    (pad 6 smd rect (at 0.725 0.5 90) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 37 "/LCDE(SCLK)"))
    (pad 5 smd rect (at 0.725 0 90) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.725 -0.5 90) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 36 "/LCDRW(SID)"))
    (pad 3 smd rect (at -0.725 -0.5 90) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at -0.725 0 90) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.725 0.5 90) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 35 "/LCDRS(CS)"))
    (model smd_qfn/dfn6-3x3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module GLCD:SD_Card_Receptacle locked (layer B.Cu) (tedit 580550B3)
    (at 124 88 90)
    (fp_text reference SD1 (at 14 -14 180) (layer B.SilkS))
    (fp_text value SD_CARD (at 11 -14 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9.4996 -3.55092 90) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -11.50112 -3.55092 90) (size 1.0922 1.0922) (drill 1.0922) (layers *.Cu *.Mask B.SilkS))
    (pad 11 smd rect (at -12.25042 -0.7493 90) (size 0.70104 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(SD1-Pad11)"))
    (pad 10 smd rect (at -11.049 -0.7493 90) (size 0.70104 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 4 /SD_DET))
    (pad 1 smd rect (at 6.87578 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(IC1-Pad15)"))
    (pad 13 smd rect (at 11.45032 -2.55016 90) (size 1.50114 2.79908) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -13.64996 -2.55016 90) (size 1.50114 2.79908) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 13.64996 -24.05126 90) (size 1.50114 2.79908) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -13.64996 -24.05126 90) (size 1.50114 2.79908) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 9.37514 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(SD1-Pad9)"))
    (pad 8 smd rect (at -9.75106 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(SD1-Pad8)"))
    (pad 7 smd rect (at -8.04926 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 31 /MISO))
    (pad 6 smd rect (at -5.6261 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -3.1242 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC1-Pad10)"))
    (pad 4 smd rect (at -0.62484 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 1.87452 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.37388 -0.7493 90) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(IC1-Pad12)"))
  )
  (module TO_SOT_Packages_SMD:SOT-223 locked (layer B.Cu) (tedit 58C6A382)
    (at 137 80.25 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 5.5 180) (layer B.SilkS))
    (fp_text value MIC5209-3.3YS (at 0 7 180) (layer F.Fab))
    (pad 1 smd rect (at -2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 3 smd rect (at 2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-N locked (layer B.Cu) (tedit 580550B3)
    (at 137 95.75 270)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference IC1 (at -6.5 0 360) (layer B.SilkS))
    (fp_text value 74HC4050 (at 6.75 0 360) (layer F.Fab))
    (pad 15 smd rect (at -3.175 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(IC1-Pad15)"))
    (pad 1 smd rect (at -4.445 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -3.175 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at 3.175 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 4.445 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.445 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 32 /SCK))
    (pad 10 smd rect (at 3.175 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 34 /MOSI))
    (pad 12 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /SS))
    (pad 16 smd rect (at -4.445 3.175 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(IC1-Pad16)"))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering locked (layer B.Cu) (tedit 580550B3)
    (at 143.5 80.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3 0 540) (layer B.SilkS))
    (fp_text value 100nF (at 3.25 0 360) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering locked (layer B.Cu) (tedit 580550B3)
    (at 130.5 80.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3 0 360) (layer B.SilkS))
    (fp_text value 100nF (at 3.25 0 360) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering locked (layer B.Cu) (tedit 580550B3)
    (at 141.5 87.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75) (layer B.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering locked (layer B.Cu) (tedit 580550B3)
    (at 163.75 113.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.25 0 360) (layer B.SilkS))
    (fp_text value 1kΩ (at 0 -2.75 360) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 /Beeper))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering locked (layer B.Cu) (tedit 580550B3)
    (at 127 91.15 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -4 0 360) (layer B.SilkS))
    (fp_text value 1uF (at 4.25 0 360) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering locked (layer B.Cu) (tedit 580550B3)
    (at 164.75 120.5)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -3.5) (layer B.SilkS))
    (fp_text value BC817-40 (at 5.75 -0.5) (layer F.Fab))
    (pad 3 smd rect (at 0 1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(Q1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x20 locked (layer F.Cu) (tedit 580550B3)
    (at 159.25 120.5 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference DS1 (at -2.5 22 360) (layer B.SilkS))
    (fp_text value LCD_Panel (at -4 22.5 360) (layer F.Fab))
    (pad 20 thru_hole oval (at 0 48.26 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 19 thru_hole oval (at 0 45.72 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(DS1-Pad19)"))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(DS1-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(DS1-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(DS1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(DS1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(DS1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(DS1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(DS1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(DS1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "/LCDE(SCLK)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "/LCDRW(SID)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "/LCDRS(CS)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x20.wrl
      (at (xyz 0 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:IDC_Header_Straight_10pins locked (layer B.Cu) (tedit 580550B3)
    (at 123.14 62.46)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference EXP2 (at 5.08 -5) (layer B.SilkS))
    (fp_text value CONN_02X05 (at 5.08 7) (layer F.Fab))
    (pad 10 thru_hole oval (at 10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 /MISO))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 /SCK))
    (pad 8 thru_hole oval (at 7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 /BTN_EN2))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 /SS))
    (pad 6 thru_hole oval (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 /BTN_EN1))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 /MOSI))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /SD_DET))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 42 "Net-(EXP2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 41 "Net-(EXP2-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 580550B3)
    (at 99.5 55.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4.15 4.15) (drill 3.4) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 580550B3)
    (at 187.5 120.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4.15 4.15) (drill 3.4) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 580550B3)
    (at 99.5 120.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4.15 4.15) (drill 3.4) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module Resistors_SMD:R_0805_HandSoldering locked (layer B.Cu) (tedit 580550B3)
    (at 116.06784 124.49556 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference RBL1 (at -0.25 1.75 180) (layer B.SilkS))
    (fp_text value 68Ω (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(DS1-Pad19)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buzzers_Beepers:Buzzer_12x9.5RM7.6 locked (layer F.Cu) (tedit 580550B3)
    (at 161 131.5)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference SP1 (at 0 -2) (layer F.SilkS))
    (fp_text value SPEAKER (at -0.24 3.342) (layer F.Fab))
    (fp_text user + (at -3.81 -2.54) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.79984 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole circle (at -3.79984 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model Buzzers_Beepers.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module GLCD:LulzBot locked (layer F.Cu) (tedit 0)
    (at 108 131)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module GLCD:copyleft locked (layer F.Cu) (tedit 0)
    (at 130 134.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module GLCD:OSHW locked (layer F.Cu) (tedit 0)
    (at 126 126)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 580550B3)
    (at 187.5 55.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4.15 4.15) (drill 3.4) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module GLCD:AO locked (layer F.Cu) (tedit 0)
    (at 122 134.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connect:IDC_Header_Straight_10pins locked (layer B.Cu) (tedit 580550B3)
    (at 153.64 62.46)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference EXP1 (at 5.08 -5) (layer B.SilkS))
    (fp_text value CONN_02X05 (at 5.08 7) (layer F.Fab))
    (pad 10 thru_hole oval (at 10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 /Beeper))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 /BTN_ENC))
    (pad 8 thru_hole oval (at 7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 36 "/LCDRW(SID)"))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 35 "/LCDRS(CS)"))
    (pad 6 thru_hole oval (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 37 "/LCDE(SCLK)"))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 40 "Net-(EXP1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 39 "Net-(EXP1-Pad4)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 38 "Net-(EXP1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 VCC))
  )
  (module "AO Parts:MM5_DRILL" (layer F.Cu) (tedit 5CAE4D7A)
    (at 127 102)
    (fp_text reference REF** (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value MM5_DRILL (at 0 4) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (gr_text "Copyright\nAleph Objects Inc.\n2016" (at 144 133) (layer F.SilkS))
  (gr_text v0.7 (at 108 64) (layer B.SilkS))
  (gr_text "GNU GPLv2" (at 144 127) (layer F.SilkS))
  (gr_line (start 190 140) (end 190 53) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97 140) (end 190 140) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97 53) (end 97 140) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190 53) (end 97 53) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 190.5 140.5) (xy 96.5 140.5) (xy 96.5 52.5) (xy 190.5 52.5)
      )
    )
  )
)
