(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 68)
    (no_connects 0)
    (area 126.924999 83.744999 193.115001 119.455001)
    (thickness 1.6)
    (drawings 11)
    (tracks 244)
    (zones 0)
    (modules 33)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 127 83.82)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../PCB_Gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 "Net-(F1-Pad1)")
  (net 5 "Net-(P1-Pad4)")
  (net 6 "Net-(P1-Pad6)")
  (net 7 "Net-(P1-Pad8)")
  (net 8 "Net-(P1-Pad10)")
  (net 9 "Net-(P2-Pad3)")
  (net 10 "Net-(P2-Pad2)")
  (net 11 "Net-(R2-Pad1)")
  (net 12 "Net-(R5-Pad2)")
  (net 13 "Net-(U2-Pad4)")
  (net 14 "Net-(U2-Pad6)")
  (net 15 "Net-(U2-Pad10)")
  (net 16 "Net-(C8-Pad1)")
  (net 17 "Net-(P1-Pad3)")
  (net 18 "Net-(P1-Pad5)")
  (net 19 "Net-(P1-Pad7)")
  (net 20 "Net-(P1-Pad9)")
  (net 21 "Net-(U2-Pad16)")
  (net 22 "Net-(U2-Pad13)")
  (net 23 "Net-(U2-Pad12)")
  (net 24 "Net-(U2-Pad15)")
  (net 25 "Net-(U3-Pad1)")
  (net 26 "Net-(U3-Pad4)")
  (net 27 "Net-(U3-Pad5)")
  (net 28 "Net-(U3-Pad6)")
  (net 29 "Net-(U3-Pad7)")
  (net 30 "Net-(U3-Pad8)")
  (net 31 "Net-(U3-Pad9)")
  (net 32 "Net-(U3-Pad10)")
  (net 33 "Net-(U3-Pad11)")
  (net 34 "Net-(U3-Pad26)")
  (net 35 "Net-(U3-Pad27)")
  (net 36 "Net-(U3-Pad28)")
  (net 37 "Net-(U3-Pad29)")
  (net 38 "Net-(U3-Pad30)")
  (net 39 "Net-(U3-Pad31)")
  (net 40 "Net-(U3-Pad32)")
  (net 41 "Net-(C6-Pad1)")
  (net 42 "Net-(U3-Pad17)")
  (net 43 "Net-(OSC1-Pad1)")
  (net 44 "Net-(OSC1-Pad3)")
  (net 45 "Net-(U3-Pad25)")
  (net 46 "Net-(C2-Pad1)")
  (net 47 "Net-(R3-Pad1)")
  (net 48 "Net-(R6-Pad2)")
  (net 49 "Net-(R7-Pad2)")
  (net 50 "Net-(U1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(OSC1-Pad1)")
    (add_net "Net-(OSC1-Pad3)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad25)")
    (add_net "Net-(U3-Pad26)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad29)")
    (add_net "Net-(U3-Pad30)")
    (add_net "Net-(U3-Pad31)")
    (add_net "Net-(U3-Pad32)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(F1-Pad1)")
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 5C2652A6)
    (at 152.908 116.078 180)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C1 (at 7.366 -1.016 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.09906 3.59918 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 5C265273)
    (at 152.908 110.998 180)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C3 (at 7.366 0.762 180) (layer F.SilkS))
    (fp_text value 33uF (at -0.09906 3.59918 180) (layer F.Fab) hide)
    (fp_text user + (at -7.62 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module AO_Parts:FA-328_Crystal (layer F.Cu) (tedit 5C264B10)
    (at 164.75 94.25)
    (attr smd)
    (fp_text reference OSC1 (at 4.668 -1.032) (layer F.SilkS))
    (fp_text value Oscillator (at 0 -4.8) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(OSC1-Pad1)"))
    (pad 2 smd rect (at 1.1 0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(OSC1-Pad3)"))
    (pad 4 smd rect (at -1.1 -0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B4F5261)
    (at 170.18 96.52)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 4.064 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B4F526A)
    (at 170.18 98.552)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 4.064 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A84A36C)
    (at 187.96 113.03)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference F1 (at 0 -1.905) (layer F.SilkS))
    (fp_text value Polyfuse (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:IDC_Header_Straight_10pins (layer F.Cu) (tedit 5B4F52C3)
    (at 134.62 106.68 90)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P1 (at -6.477 -1.27 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 5.08 5.223 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad10)"))
  )
  (module "AO Parts:USB_A_TH" (layer F.Cu) (tedit 5A84AFA6)
    (at 193.04 101.6)
    (fp_text reference P2 (at -5.08 7.62) (layer F.SilkS))
    (fp_text value USB_A (at -7.62 0) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at -13 -1) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at -13 1) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 4 thru_hole circle (at -13 -3.5) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -13 3.5) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 5 thru_hole circle (at -10.3 6.5) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.3 -6.5) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B4F478C)
    (at 162.56 116.078)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.778) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B4F479E)
    (at 140.97 106.68 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad10)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5C264B6C)
    (at 146.05 108.204 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5C264B0A)
    (at 159.512 94.488)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.524 1.524 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(OSC1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A84B488)
    (at 154.94 94.488 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GLCD:SOT-666 (layer F.Cu) (tedit 5A84BAAF)
    (at 176.53 101.6 90)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference Z1 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value ZENER_4_CHANNEL (at 0 2 90) (layer F.Fab) hide)
    (pad 6 smd rect (at 0.725 -0.5 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 5 smd rect (at 0.725 0 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.725 0.5 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P2-Pad3)"))
    (pad 3 smd rect (at -0.725 0.5 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 2 smd rect (at -0.725 0 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.725 -0.5 180) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model smd_qfn/dfn6-3x3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A84606B)
    (at 142.24 90.17)
    (fp_text reference MH1 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value "MOUNTING HOLE" (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A846072)
    (at 142.24 113.03)
    (fp_text reference MH2 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value "MOUNTING HOLE" (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "AO Parts:MH_M3x6mm" (layer F.Cu) (tedit 5A846079)
    (at 176.53 113.03)
    (fp_text reference MH3 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value "MOUNTING HOLE" (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "AO Parts:MH_M3x6mm" (layer F.Cu) (tedit 5A846081)
    (at 176.53 90.17)
    (fp_text reference MH4 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value "MOUNTING HOLE" (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A84A42F)
    (at 187.96 117.475 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -3.175 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A846A34)
    (at 187.96 115.57 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L1 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-N (layer F.Cu) (tedit 5B4F52B9)
    (at 151.13 100.33 180)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 6.985 3.302 180) (layer F.SilkS))
    (fp_text value 74HC4050 (at 0 1.27 180) (layer F.Fab) hide)
    (pad 16 smd rect (at -4.445 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad16)"))
    (pad 14 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad9)"))
    (pad 13 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad13)"))
    (pad 12 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad12)"))
    (pad 11 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad7)"))
    (pad 10 smd rect (at 3.175 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad10)"))
    (pad 9 smd rect (at 4.445 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P1-Pad5)"))
    (pad 8 smd rect (at 4.445 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 3.175 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at -3.175 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -4.445 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at -3.175 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad15)"))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-32_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 5C264AFC)
    (at 163.195 101.6)
    (descr "LQFP32: plastic low profile quad flat package; 32 leads; body 5 x 5 x 1.4 mm (see NXP sot401-1_fr.pdf and sot401-1_po.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U3 (at 0.381 -4.826) (layer F.SilkS))
    (fp_text value MAX3421E (at 0 4.85) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.25 -1.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -3.25 -1.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.25 -0.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -3.25 -0.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -3.25 0.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -3.25 0.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -3.25 1.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -3.25 1.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U3-Pad8)"))
    (pad 9 smd rect (at -1.75 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at -1.25 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at -0.75 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U3-Pad11)"))
    (pad 12 smd rect (at -0.25 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R5-Pad2)"))
    (pad 13 smd rect (at 0.25 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad15)"))
    (pad 14 smd rect (at 0.75 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad12)"))
    (pad 15 smd rect (at 1.25 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 16 smd rect (at 1.75 3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad10)"))
    (pad 17 smd rect (at 3.25 1.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U3-Pad17)"))
    (pad 18 smd rect (at 3.25 1.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R3-Pad1)"))
    (pad 19 smd rect (at 3.25 0.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 3.25 0.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R6-Pad2)"))
    (pad 21 smd rect (at 3.25 -0.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R7-Pad2)"))
    (pad 22 smd rect (at 3.25 -0.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C6-Pad1)"))
    (pad 23 smd rect (at 3.25 -1.25) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 24 smd rect (at 3.25 -1.75) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(OSC1-Pad3)"))
    (pad 25 smd rect (at 1.75 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U3-Pad25)"))
    (pad 26 smd rect (at 1.25 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U3-Pad26)"))
    (pad 27 smd rect (at 0.75 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U3-Pad27)"))
    (pad 28 smd rect (at 0.25 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U3-Pad28)"))
    (pad 29 smd rect (at -0.25 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U3-Pad29)"))
    (pad 30 smd rect (at -0.75 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U3-Pad30)"))
    (pad 31 smd rect (at -1.25 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U3-Pad31)"))
    (pad 32 smd rect (at -1.75 -3.25 90) (size 1.2 0.28) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U3-Pad32)"))
    (model Housings_QFP.3dshapes/LQFP-32_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "AO Parts:GND_PAD" (layer F.Cu) (tedit 5B4F4326)
    (at 132.08 86.36)
    (fp_text reference PAD1 (at 0 2.6) (layer F.SilkS) hide)
    (fp_text value "PAD FOR GROUND WIRE" (at 0 -2.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5C264AEA)
    (at 157.988 97.282 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -3.048 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5C264EA8)
    (at 171.958 102.87 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 3.208 -0.13 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5C264BA1)
    (at 169.926 116.078)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5C264B4F)
    (at 164.592 91.44)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 4.318 -0.762) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5C264EB1)
    (at 171.958 100.33 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 3.208 0.08 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P2-Pad3)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5C264C0A)
    (at 166.116 112.776 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value TLV75533 (at -0.05 2.35 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5C2656B6)
    (at 188 87.4)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (attr smd)
    (fp_text reference REF** (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab) hide)
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5C26627C)
    (at 137.16 88.9)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5C26628D)
    (at 182.88 88.9)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5C266291)
    (at 170.18 109.22)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (gr_text + (at 160.4 108.8) (layer F.SilkS))
  (gr_text + (at 160.4 113.9) (layer F.SilkS))
  (gr_text GPLv3 (at 157.988 91.44) (layer F.SilkS))
  (gr_text "REV. C" (at 149.86 91.44) (layer F.SilkS))
  (gr_text "USB DRIVE READER" (at 156.845 88.9) (layer F.SilkS))
  (gr_text "©2018 Aleph Objects, Inc" (at 159.385 86.36) (layer F.SilkS))
  (gr_line (start 193.04 83.82) (end 127 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 119.38) (end 193.04 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 119.38) (end 193.04 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 83.82) (end 127 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 192.532 118.872) (xy 127.508 118.872) (xy 127.508 84.328) (xy 192.532 84.328)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 192.532 118.872) (xy 127.508 118.872) (xy 127.508 84.328) (xy 192.532 84.328)
      )
    )
  )
)
