(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 34)
    (no_connects 0)
    (area 117.681904 75.906545 202.358096 119.455001)
    (thickness 1.6)
    (drawings 7)
    (tracks 109)
    (zones 0)
    (modules 15)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory SD_Reader_Gerbers_Rev_A1/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 /MOSI_3V3)
  (net 5 /SCLK_3V3)
  (net 6 "Net-(CON1-Pad7)")
  (net 7 "Net-(CON1-Pad8)")
  (net 8 "Net-(CON1-Pad9)")
  (net 9 /CS_3V3)
  (net 10 /SD_DET)
  (net 11 "Net-(CON1-Pad11)")
  (net 12 "Net-(P1-Pad3)")
  (net 13 "Net-(P1-Pad6)")
  (net 14 "Net-(P1-Pad8)")
  (net 15 "Net-(P1-Pad5)")
  (net 16 "Net-(P1-Pad7)")
  (net 17 "Net-(P1-Pad9)")
  (net 18 "Net-(U2-Pad16)")
  (net 19 "Net-(U2-Pad13)")
  (net 20 "Net-(U2-Pad6)")
  (net 21 "Net-(U2-Pad4)")
  (net 22 "Net-(U2-Pad2)")
  (net 23 "Net-(P1-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /CS_3V3)
    (add_net /MOSI_3V3)
    (add_net /SCLK_3V3)
    (add_net /SD_DET)
    (add_net GND)
    (add_net "Net-(CON1-Pad11)")
    (add_net "Net-(CON1-Pad7)")
    (add_net "Net-(CON1-Pad8)")
    (add_net "Net-(CON1-Pad9)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad6)")
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 5A85ACDE)
    (at 148.59 91.44 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C1 (at -3.81 -3.81 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.09906 3.59918 90) (layer F.Fab) hide)
    (fp_text user + (at -6.85546 -2.70002 90) (layer F.SilkS))
    (pad 2 smd rect (at 3.88874 0 90) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.88874 0 90) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 5A85F0DD)
    (at 156.21 111.76 180)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C2 (at 0 -4.445 180) (layer F.SilkS))
    (fp_text value 33uF (at -0.09906 3.59918 180) (layer F.Fab) hide)
    (fp_text user + (at -6.85546 -2.70002 180) (layer F.SilkS))
    (pad 2 smd rect (at 3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A85F0F1)
    (at 153.035 97.79 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A85ACB5)
    (at 165.1 101.6 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 3.175 -1.905 180) (layer F.SilkS))
    (fp_text value 1.0uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GLCD:SD_Card_Receptacle (layer F.Cu) (tedit 5A85F0AA)
    (at 167.005 101.6 90)
    (fp_text reference CON1 (at -13.97 12.7 180) (layer F.SilkS))
    (fp_text value GLCD_SD_Card (at 0 26.5 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 4.37388 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI_3V3))
    (pad 3 smd rect (at 1.87452 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.62484 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at -3.1242 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCLK_3V3))
    (pad 6 smd rect (at -5.6261 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -8.04926 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CON1-Pad7)"))
    (pad 8 smd rect (at -9.75106 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CON1-Pad8)"))
    (pad 9 smd rect (at 9.37514 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CON1-Pad9)"))
    (pad 15 smd rect (at -13.64996 24.05126 90) (size 1.50114 2.79908) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 13.64996 24.05126 90) (size 1.50114 2.79908) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -13.64996 2.55016 90) (size 1.50114 2.79908) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 11.45032 2.55016 90) (size 1.50114 2.79908) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 6.87578 0.7493 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 9 /CS_3V3))
    (pad 10 smd rect (at -11.049 0.7493 90) (size 0.70104 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 10 /SD_DET))
    (pad 11 smd rect (at -12.25042 0.7493 90) (size 0.70104 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CON1-Pad11)"))
    (pad "" np_thru_hole circle (at -11.50112 3.55092 90) (size 1.0922 1.0922) (drill 1.0922) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 9.4996 3.55092 90) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A85AACE)
    (at 142.24 90.17)
    (fp_text reference MH1 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value "MOUNTING HOLE" (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A85AAD5)
    (at 142.24 113.03)
    (fp_text reference MH2 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value "MOUNTING HOLE" (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connectors:IDC_Header_Straight_10pins (layer F.Cu) (tedit 5A85AAC1)
    (at 132.08 96.52 270)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P1 (at 16.51 1.27 360) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 5.08 5.223 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SD_DET))
    (pad 5 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P1-Pad10)"))
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 5A85AC90)
    (at 155.575 91.44 270)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference U1 (at 0 -10.414 270) (layer F.SilkS))
    (fp_text value LM1117_3V3 (at 0 -2.413 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -6.35 270) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A85AAE3)
    (at 160.02 101.6)
    (fp_text reference MH3 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value "MOUNTING HOLE" (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMD_Packages:SO-16-N (layer F.Cu) (tedit 5A85F5DF)
    (at 148.59 102.87 180)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 6.985 1.905 180) (layer F.SilkS))
    (fp_text value 74HC4050 (at 0 1.27 180) (layer F.Fab) hide)
    (pad 16 smd rect (at -4.445 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad16)"))
    (pad 14 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P1-Pad7)"))
    (pad 13 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad13)"))
    (pad 12 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI_3V3))
    (pad 11 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P1-Pad5)"))
    (pad 10 smd rect (at 3.175 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCLK_3V3))
    (pad 9 smd rect (at 4.445 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P1-Pad9)"))
    (pad 8 smd rect (at 4.445 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 3.175 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.175 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -4.445 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at -3.175 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 /CS_3V3))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A85BEFF)
    (at 160.02 107.315 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.54 1.905 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CON1-Pad7)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P1-Pad10)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5A85C0E9)
    (at 185.42 86.36)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5A85C11D)
    (at 134.62 114.3)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5A85C180)
    (at 132.715 87.63 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (attr smd)
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (gr_text "SD Card Reader Rev. A" (at 175.768 117.348) (layer F.SilkS))
  (gr_text GPLv3 (at 137.414 87.63 270) (layer F.SilkS))
  (gr_text "©2018 Aleph Objects, Inc." (at 168.656 86.36) (layer F.SilkS))
  (gr_line (start 127 83.82) (end 193.04 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 119.38) (end 127 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 119.38) (end 127 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 83.82) (end 193.04 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 192.532 118.872) (xy 127.508 118.872) (xy 127.508 84.328) (xy 192.532 84.328)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 192.532 118.872) (xy 127.508 118.872) (xy 127.508 84.328) (xy 192.532 84.328)
      )
    )
  )
)
