%
% Specs.tex
% Specs Development
%
% LulzBot Mini Developer's Guide
%
% Copyright (C) 2014 Aleph Objects, Inc.
%
% This document is licensed under the Creative Commons Attribution 4.0
% International Public License (CC BY-SA 4.0) by Aleph Objects, Inc.
%

\section{Specifications}

\subsection{Printing}
\begin{itemize}
\item Print Surface: Heated Borosilicate glass bed covered with PEI film
\item Print Area:155mm x 155mm x 155mm (6.1in x 6.1in x 6.1in)
\item Print Volume: 3,726cm3 (227.4 in3) of usable space
\item Top Print Speed: 275mm/sec (10.8in/sec)
\item Print Tolerance: 0.1mm (0.0039in) in X and Y axes. Z axis is dependent on layer thickness
\item Layer Thickness: 0.075mm to 0.50mm (0.003in - 0.020in)
\item Supported Materials: ABS, PLA, HIPS, PVA, wood filled filaments, Polyester (Tritan), PETT, filled PLA, Bronze and copper filled filaments, Polycarbonate, Nylon, PETG, Conductive PLA and ABS, UV luminescent filaments, PCTPE, PC-ABS, and more every day.
\item Usable Filament Sizes: standard 3mm (0.1in)
\end{itemize}
\subsection{Phyiscal Dimensions}
\begin{itemize}
\item Overall Dimensions: 435mm x 340mm x 385mm (17.1in x 13.4in x 15.2in)
\item Weight: 8.55kg (18.85lbs)
\end{itemize}
\subsection{Electrical}
\begin{itemize}
\item Power Requirements: 100 - 240 VAC
\item Power Supply: 24V 150W
\item US, UK, and EU electrical plugs available
\end{itemize}
\subsection{Temperature}
\begin{itemize}
\item Temperature: Maximum operating temperature (Extruder), 300C (572F)
\item Temperature: Maximum operating temperature (Heated Bed), 120C (248F)
\end{itemize}

