(module TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 58175C2F)
  (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
  (fp_text reference P6 (at 1.27 -4.50088) (layer F.SilkS) hide)
  (fp_text value HEAT (at 1.25 -4.25) (layer F.SilkS))
  (pad 1 thru_hole rect (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS))
  (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
    (at (xyz 0.05 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
